(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 52)
    (zones 0)
    (modules 10)
    (nets 32)
  )
  (page A3)
  (title_block
    (date "15 nov 2012")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.9)
    (via_drill 0.6)
    (via_min_size 0.8)
    (via_min_drill 0.5)
    (uvia_size 0.5)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.5)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.02 2.02)
    (pad_drill 1.02)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 200 150)
    (grid_origin 200 150)
    (visible_elements 7FFFE7FF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 +5V)
  (net 3 GND)
  (net 4 /ID_SD)
  (net 5 /ID_SC)
  (net 6 /GPIO5)
  (net 7 /GPIO6)
  (net 8 /GPIO26)
  (net 9 "/GPIO2(SDA1)")
  (net 10 "/GPIO3(SCL1)")
  (net 11 "/GPIO4(GCLK)")
  (net 12 "/GPIO14(TXD0)")
  (net 13 "/GPIO15(RXD0)")
  (net 14 "/GPIO17(GEN0)")
  (net 15 "/GPIO27(GEN2)")
  (net 16 "/GPIO22(GEN3)")
  (net 17 "/GPIO23(GEN4)")
  (net 18 "/GPIO24(GEN5)")
  (net 19 "/GPIO25(GEN6)")
  (net 20 "/GPIO18(GEN1)(PWM0)")
  (net 21 "/GPIO10(SPI0_MOSI)")
  (net 22 "/GPIO9(SPI0_MISO)")
  (net 23 "/GPIO11(SPI0_SCK)")
  (net 24 "/GPIO8(SPI0_CE_N)")
  (net 25 "/GPIO7(SPI1_CE_N)")
  (net 26 "/GPIO12(PWM0)")
  (net 27 "/GPIO13(PWM1)")
  (net 28 "/GPIO19(SPI1_MISO)")
  (net 29 /GPIO16)
  (net 30 "/GPIO20(SPI1_MOSI)")
  (net 31 "/GPIO21(SPI1_SCK)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.9)
    (via_drill 0.6)
    (uvia_dia 0.5)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net "/GPIO10(SPI0_MOSI)")
    (add_net "/GPIO11(SPI0_SCK)")
    (add_net "/GPIO12(PWM0)")
    (add_net "/GPIO13(PWM1)")
    (add_net "/GPIO14(TXD0)")
    (add_net "/GPIO15(RXD0)")
    (add_net /GPIO16)
    (add_net "/GPIO17(GEN0)")
    (add_net "/GPIO18(GEN1)(PWM0)")
    (add_net "/GPIO19(SPI1_MISO)")
    (add_net "/GPIO2(SDA1)")
    (add_net "/GPIO20(SPI1_MOSI)")
    (add_net "/GPIO21(SPI1_SCK)")
    (add_net "/GPIO22(GEN3)")
    (add_net "/GPIO23(GEN4)")
    (add_net "/GPIO24(GEN5)")
    (add_net "/GPIO25(GEN6)")
    (add_net /GPIO26)
    (add_net "/GPIO27(GEN2)")
    (add_net "/GPIO3(SCL1)")
    (add_net "/GPIO4(GCLK)")
    (add_net /GPIO5)
    (add_net /GPIO6)
    (add_net "/GPIO7(SPI1_CE_N)")
    (add_net "/GPIO8(SPI0_CE_N)")
    (add_net "/GPIO9(SPI0_MISO)")
    (add_net /ID_SC)
    (add_net /ID_SD)
    (add_net GND)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.7)
    (uvia_dia 0.5)
    (uvia_drill 0.1)
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 249.53 163.97)
    (fp_text reference "" (at 246.99 162.7) (layer F.SilkS))
    (fp_text value "" (at 246.99 162.7) (layer F.SilkS))
    (fp_text user MK2 (at 247.53 162.16) (layer F.SilkS))
  )
  (module digikey-footprints:PinHeader_1x3_P2.54mm_Drill1.02mm (layer F.Cu) (tedit 5A43C851)
    (at 246.99 162.7 180)
    (descr http://www.molex.com/pdm_docs/sd/022232031_sd.pdf)
    (fp_text reference FS3 (at 2.71 -4.59) (layer F.SilkS))
    (fp_text value 0022232031 (at 2.82 4.63) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 "/GPIO25(GEN6)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module digikey-footprints:PinHeader_1x3_P2.54mm_Drill1.02mm (layer F.Cu) (tedit 5A43C851)
    (at 234.29 162.7 180)
    (descr http://www.molex.com/pdm_docs/sd/022232031_sd.pdf)
    (fp_text reference FS2 (at 2.71 -4.59) (layer F.SilkS))
    (fp_text value 0022232031 (at 2.82 4.63) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 "/GPIO24(GEN5)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module digikey-footprints:PinHeader_1x3_P2.54mm_Drill1.02mm (layer F.Cu) (tedit 5DA232C0)
    (at 221.59 162.7 180)
    (descr http://www.molex.com/pdm_docs/sd/022232031_sd.pdf)
    (fp_text reference FS1 (at 2.71 -4.59) (layer F.SilkS))
    (fp_text value 0022232031 (at 2.82 4.63) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 "/GPIO23(GEN4)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 238.1 156.35 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "/GPIO25(GEN6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 231.75 156.35 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "/GPIO24(GEN5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 225.4 156.35 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "/GPIO23(GEN4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A433)
    (at 207.1 153.38 270)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference P1 (at 2.208 1.512) (layer B.SilkS))
    (fp_text value Conn_02x20_Odd_Even (at -1.27 -51.03 270) (layer B.Fab))
    (fp_text user %R (at -1.27 -24.13 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/GPIO2(SDA1)"))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/GPIO3(SCL1)"))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/GPIO4(GCLK)"))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/GPIO14(TXD0)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/GPIO15(RXD0)"))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/GPIO17(GEN0)"))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/GPIO18(GEN1)(PWM0)"))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/GPIO27(GEN2)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/GPIO22(GEN3)"))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/GPIO23(GEN4)"))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/GPIO24(GEN5)"))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/GPIO10(SPI0_MOSI)"))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/GPIO9(SPI0_MISO)"))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/GPIO25(GEN6)"))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/GPIO11(SPI0_SCK)"))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/GPIO8(SPI0_CE_N)"))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/GPIO7(SPI1_CE_N)"))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /ID_SD))
    (pad 28 thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /ID_SC))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GPIO5))
    (pad 30 thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 31 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GPIO6))
    (pad 32 thru_hole oval (at -2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/GPIO12(PWM0)"))
    (pad 33 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/GPIO13(PWM1)"))
    (pad 34 thru_hole oval (at -2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 35 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/GPIO19(SPI1_MISO)"))
    (pad 36 thru_hole oval (at -2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /GPIO16))
    (pad 37 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIO26))
    (pad 38 thru_hole oval (at -2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/GPIO20(SPI1_MOSI)"))
    (pad 39 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 40 thru_hole oval (at -2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/GPIO21(SPI1_SCK)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 260.23 152.11 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference " " (at 0 -3.7 180) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7 180) (layer F.Fab))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 202.23 152.11 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference " " (at 0 -3.7 180) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7 180) (layer F.Fab))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_text S (at 219.05 165.24) (layer F.SilkS))
  (gr_text S (at 231.75 165.24) (layer F.SilkS))
  (gr_text S (at 244.45 165.24) (layer F.SilkS))
  (gr_text 5v (at 215.24 165.24) (layer F.SilkS))
  (gr_text 5v (at 227.94 165.24) (layer F.SilkS))
  (gr_text 5v (at 240.64 165.24) (layer F.SilkS))
  (gr_text G (at 221.59 165.24) (layer F.SilkS))
  (gr_text G (at 234.29 165.24) (layer F.SilkS))
  (gr_text G (at 246.99 165.24) (layer F.SilkS))
  (gr_text v01 (at 201.64 165.84) (layer F.SilkS))
  (gr_text "FLOW METER" (at 206.35 163.97) (layer F.SilkS))
  (gr_text BRUI (at 206.35 161.43) (layer F.SilkS))
  (gr_text "RASPBERRY-PI 40-PIN ADDON BOARD\nVIEW FROM TOP\nNOTE: P1 SHOULD BE FITTED ON THE REVERSE OF THE BOARD\n\nADD EDGE CUTS FROM CAMERA AND DISPLAY PORTS AS REQUIRED" (at 200 180.48) (layer Dwgs.User))
  (gr_arc (start 201.73 166.61) (end 201.73 169.61) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 260.73 166.61) (end 263.73 166.61) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 201.73 169.61) (end 260.73 169.61) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 263.73 166.61) (end 263.73 151.61) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 198.73 151.61) (end 198.73 166.61) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 260.73 151.61) (end 260.73 148.61) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 201.73 151.61) (end 198.73 151.61) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 260.73 148.61) (end 201.73 148.61) (layer Edge.Cuts) (width 0.1))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 264.77 147.46) (xy 264.77 170.32) (xy 197.46 170.32) (xy 197.46 147.46)
      )
    )
  )
)
