(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 49)
    (no_connects 0)
    (area 108.449999 76.080999 170.277 123.829001)
    (thickness 1.6002)
    (drawings 6)
    (tracks 149)
    (zones 0)
    (modules 24)
    (nets 18)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEEF7F)
    (pcbplotparams
      (layerselection 0x000a0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 /3.3V)
  (net 6 GND)
  (net 7 /5V)
  (net 8 +12V)
  (net 9 "Net-(D1-Pad1)")
  (net 10 /SPI_MISO)
  (net 11 /SPI_CLK)
  (net 12 "Net-(MCU1-Pad10)")
  (net 13 "Net-(MCU1-Pad11)")
  (net 14 "Net-(MCU1-Pad12)")
  (net 15 "Net-(Q1-Pad2)")
  (net 16 "Net-(Q1-Pad3)")
  (net 17 /MOTOR_PWM)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /MOTOR_PWM)
    (add_net /SPI_CLK)
    (add_net /SPI_MISO)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(MCU1-Pad10)")
    (add_net "Net-(MCU1-Pad11)")
    (add_net "Net-(MCU1-Pad12)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.79)
    (via_dia 0.79)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /3.3V)
    (add_net /5V)
    (add_net "Net-(D1-Pad1)")
  )
  (module Power_Integrations:SO-8 (layer F.Cu) (tedit 585A4EE0)
    (at 140.7 100.33 180)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U2 (at 0 0 180) (layer F.SilkS))
    (fp_text value MAX31855KASA (at -2.55 -4.67 180) (layer F.Fab))
    (pad 1 smd oval (at -1.905 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 6 GND))
    (pad 2 smd oval (at -0.635 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 3 smd oval (at 0.635 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd oval (at 1.905 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 5 /3.3V))
    (pad 5 smd oval (at 1.905 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 11 /SPI_CLK))
    (pad 6 smd oval (at 0.635 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 13 "Net-(MCU1-Pad11)"))
    (pad 7 smd oval (at -0.635 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 10 /SPI_MISO))
    (pad 8 smd oval (at -1.905 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask))
  )
  (module Connect:1pin (layer F.Cu) (tedit 5858DD0C)
    (at 112 118)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 585A4F4E)
    (at 148.32 93.98 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0.07 1.48 180) (layer F.SilkS))
    (fp_text value 10nf (at -1.43 -1.52 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 585A4F63)
    (at 140.7 93.98)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0.05 -1.48) (layer F.SilkS))
    (fp_text value 10nf (at 0.8 1.52) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 585A588F)
    (at 144.5 96.5 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 5 /3.3V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ad-hoc:Barrel_Jack_PJ-002AH-SMT (layer F.Cu) (tedit 585A4932)
    (at 146 118.5 90)
    (fp_text reference CON1 (at 2.6 -9.1 270) (layer F.SilkS))
    (fp_text value "12V + BARREL" (at 3.75 -2.5 90) (layer F.Fab))
    (pad 3 smd rect (at 6.1 0 90) (size 2.8 2.4) (layers F.Cu F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 0 0 90) (size 2.8 2.4) (layers F.Cu F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at 6.1 -11.4 90) (size 2.8 2.4) (layers F.Cu F.Mask)
      (net 8 +12V))
    (pad 1 smd rect (at 0 -11.4 90) (size 2.8 2.4) (layers F.Cu F.Mask)
      (net 8 +12V))
    (pad "" np_thru_hole circle (at 0 -5.7 90) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 4.5 -5.7 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
  )
  (module particle:photon (layer F.Cu) (tedit 585A5C25)
    (at 120 98 180)
    (fp_text reference PHOTON (at 0 -16.51 180) (layer F.SilkS))
    (fp_text value PHOTON (at 0 -13.97 180) (layer F.SilkS))
    (fp_text user "all layers" (at 0 19.05 180) (layer Cmts.User))
    (fp_text user "recommended on" (at 0 16.51 180) (layer Cmts.User))
    (fp_text user "signal keep out" (at 0 13.97 180) (layer Cmts.User))
    (fp_text user "ground plane and" (at 0 11.43 180) (layer Cmts.User))
    (pad 1 thru_hole circle (at -8.89 -15.24 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 7 /5V))
    (pad 2 thru_hole circle (at -8.89 -12.7 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 3 thru_hole circle (at -8.89 -10.16 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at -8.89 -7.62 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at -8.89 -5.08 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -8.89 -2.54 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -8.89 0 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 17 /MOTOR_PWM))
    (pad 8 thru_hole circle (at -8.89 2.54 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SPI_MISO))
    (pad 9 thru_hole circle (at -8.89 5.08 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SPI_CLK))
    (pad 10 thru_hole circle (at -8.89 7.62 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(MCU1-Pad10)"))
    (pad 11 thru_hole circle (at -8.89 10.16 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(MCU1-Pad11)"))
    (pad 12 thru_hole circle (at -8.89 12.7 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(MCU1-Pad12)"))
    (pad 24 thru_hole circle (at 8.89 -15.24 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 5 /3.3V))
    (pad 23 thru_hole circle (at 8.89 -12.7 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole circle (at 8.89 -10.16 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole circle (at 8.89 -7.62 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole circle (at 8.89 -5.08 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole circle (at 8.89 -2.54 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 8.89 0 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at 8.89 2.54 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at 8.89 5.08 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole circle (at 8.89 7.62 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 8.89 10.16 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 8.89 12.7 180) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 585A593A)
    (at 164.83 111.76 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference FAN (at 5.99 1.33 270) (layer F.SilkS))
    (fp_text value "1x2 Header for Motor" (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 585A4F39)
    (at 156.21 101.6 270)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at -2.1 -0.04 360) (layer F.SilkS))
    (fp_text value PN2222A (at -3.6 -0.29 360) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 585A58B4)
    (at 164.83 97.79 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q2 (at -0.04 2.83 270) (layer F.SilkS))
    (fp_text value IRF9540N (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 8 +12V))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(Q1-Pad3)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 585A583C)
    (at 152.4 104.14 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.89 -0.1 270) (layer F.SilkS))
    (fp_text value 1k (at 2.86 -0.1 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 15 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 17 /MOTOR_PWM))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 585A58A5)
    (at 159.75 103 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -3 0 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 16 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 8 +12V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 585A4DDA)
    (at 153.5 86 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.75 0 180) (layer F.SilkS))
    (fp_text value 10/100k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 14 "Net-(MCU1-Pad12)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 585A590B)
    (at 157 90 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference THM1 (at 6.5 1.25 90) (layer F.SilkS))
    (fp_text value 100k (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(MCU1-Pad12)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /3.3V))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:SO-8 (layer F.Cu) (tedit 0)
    (at 148.32 100.33 180)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U1 (at 0 0 180) (layer F.SilkS))
    (fp_text value MAX31855KASA (at 0 0 180) (layer F.Fab))
    (pad 1 smd oval (at -1.905 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 6 GND))
    (pad 2 smd oval (at -0.635 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 smd oval (at 0.635 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 smd oval (at 1.905 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 5 /3.3V))
    (pad 5 smd oval (at 1.905 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 11 /SPI_CLK))
    (pad 6 smd oval (at 0.635 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 12 "Net-(MCU1-Pad10)"))
    (pad 7 smd oval (at -0.635 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask)
      (net 10 /SPI_MISO))
    (pad 8 smd oval (at -1.905 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Mask))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 585A588C)
    (at 137 96.5 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 0.1uf (at -2 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 5 /3.3V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 585A4915)
    (at 132 112 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -3 0 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 4 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 7 /5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 585A4C5C)
    (at 158.48 113.03 180)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C6 (at 3.48 2.53 270) (layer F.SilkS))
    (fp_text value 10uf (at 0.98 3.53 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /5V))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 585A56B9)
    (at 149.59 113.03)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C7 (at -1.34 -2.53 90) (layer F.SilkS))
    (fp_text value 100uf (at 0.91 -3.53) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 585A58E9)
    (at 147.05 90.17 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference THK1 (at 6.42 1.45 90) (layer F.SilkS))
    (fp_text value "1x2 TC HEADER" (at 3.67 -2.3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 585A58ED)
    (at 139.43 90.17 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference THK2 (at 6.42 1.32 90) (layer F.SilkS))
    (fp_text value "1x2 TC HEADER" (at 3.67 -2.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 585A4C95)
    (at 154.67 118.11 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U3 (at 0.42 2.61 180) (layer F.SilkS))
    (fp_text value LM7805CT (at 0 -4.318 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 8 +12V))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 7 /5V))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 585A4CC8)
    (at 165 108.5 180)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D1 (at 0 2.5 180) (layer F.SilkS))
    (fp_text value 1N4004 (at 0.05 -2 180) (layer F.Fab))
    (fp_text user A (at -2.25 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D1-Pad1)"))
  )
  (module Connect:1pin (layer F.Cu) (tedit 5858DD0C)
    (at 165 84)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text "Silver Smoker v1" (at 141 105.25) (layer F.SilkS))
  (gr_line (start 108.5 121.5) (end 108.5 80.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110 121.5) (end 108.5 121.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.5 121.5) (end 110 121.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.5 80.5) (end 168.5 121.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.5 80.5) (end 168.5 80.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.5 89) (xy 112.5 89) (xy 112.5 80.5) (xy 127.5 80.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.5 89) (xy 112.5 89) (xy 112.5 80.5) (xy 127.5 80.5)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.5 121.5) (xy 108.5 121.5) (xy 108.5 80.5) (xy 168.5 80.5)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.5 121.5) (xy 108.5 121.5) (xy 108.5 80.5) (xy 168.5 80.5)
      )
    )
  )
)
