<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="-8.89" y1="3.81" x2="-8.89" y2="29.21" width="0.127" layer="20"/>
<wire x1="-2.54" y1="35.56" x2="40.64" y2="35.56" width="0.127" layer="20"/>
<wire x1="46.99" y1="29.21" x2="46.99" y2="3.81" width="0.127" layer="20"/>
<wire x1="40.64" y1="-2.54" x2="-2.54" y2="-2.54" width="0.127" layer="20"/>
<text>Point me
towards
Bean+ !!!</text>
<text>A4</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>AREF</text>
<text>VREF</text>
<text>5V</text>
<text>3.3V</text>
<text>D0</text>
<text>D1</text>
<text>D2</text>
<text>D3</text>
<text>D4</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>D8</text>
<text>D9</text>
<text>SCK</text>
<text>MISO</text>
<text>MOSI</text>
<text>SS</text>
<text>SDA</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>RST</text>
<text>A5</text>
<wire x1="-8.89" y1="29.21" x2="-2.54" y2="35.56" width="0.127" layer="20" curve="-90"/>
<wire x1="-8.89" y1="3.81" x2="-2.54" y2="-2.54" width="0.127" layer="20" curve="90"/>
<wire x1="46.99" y1="3.81" x2="40.64" y2="-2.54" width="0.127" layer="20" curve="-90"/>
<wire x1="46.99" y1="29.21" x2="40.64" y2="35.56" width="0.127" layer="20" curve="90"/>
<text>SCK</text>
<text>MISO</text>
<text>MOSI</text>
<text>SS</text>
<text>SDA</text>
<text>SCL</text>
<text>nm3210</text>
<text>2016</text>
<text>Bean+ Breakout+ 5V</text>
<text>Rev1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BEAN+JUMPERS">
</package>
<package name="1X11-BEAN+RHS">
</package>
<package name="1X12_BEAN+LHS">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0207/9">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Connectors" package="BEAN+JUMPERS" value="BEAN+JUMPERSBASE"/>
<element name="JP2" library="SparkFun-Connectors" package="1X11-BEAN+RHS" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X12_BEAN+LHS" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="R1" library="adafruit" package="0207/9" value="10K">
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="S2" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="R2" library="adafruit" package="0207/9" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0207/9" value="10K">
<attribute name="VALUE"/>
</element>
<element name="JP_S2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="JP_S1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="100nf">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="100nf">
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="100nf">
<attribute name="VALUE"/>
</element>
<element name="JP_5V" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="D0">
<contactref element="U$1" pad="D0"/>
<contactref element="JP1" pad="D0"/>
</signal>
<signal name="D1">
<contactref element="U$1" pad="D1"/>
<contactref element="JP1" pad="D1"/>
</signal>
<signal name="D2">
<contactref element="U$1" pad="D2"/>
<contactref element="JP1" pad="D2"/>
</signal>
<signal name="D3">
<contactref element="U$1" pad="D3"/>
<contactref element="JP1" pad="D3"/>
</signal>
<signal name="D4">
<contactref element="U$1" pad="D4"/>
<contactref element="JP1" pad="D4"/>
</signal>
<signal name="D5">
<contactref element="U$1" pad="D5"/>
<contactref element="JP1" pad="D5"/>
</signal>
<signal name="D6/SS">
<contactref element="U$1" pad="D6/SS"/>
<contactref element="JP1" pad="D6/SS"/>
</signal>
<signal name="D7/MOSI">
<contactref element="U$1" pad="D7/MOSI"/>
<contactref element="JP1" pad="D7/MOSI"/>
</signal>
<signal name="D8/MISO">
<contactref element="U$1" pad="D8/MISO"/>
<contactref element="JP1" pad="D8/MISO"/>
</signal>
<signal name="D9/SCK">
<contactref element="U$1" pad="D9/SCK"/>
<contactref element="JP1" pad="D9/SCK"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="RST"/>
<contactref element="JP1" pad="RST"/>
<contactref element="R1" pad="1"/>
<contactref element="RESET" pad="1"/>
<contactref element="RESET" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="5V">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="5V"/>
<contactref element="JP2" pad="5V"/>
<contactref element="JP_5V" pad="1"/>
</signal>
<signal name="VREF">
<contactref element="U$1" pad="VREF"/>
<contactref element="JP2" pad="VREF"/>
</signal>
<signal name="AREF">
<contactref element="U$1" pad="AREF"/>
<contactref element="JP2" pad="AREF"/>
</signal>
<signal name="A0">
<contactref element="U$1" pad="A0"/>
<contactref element="JP2" pad="A0"/>
</signal>
<signal name="A1">
<contactref element="U$1" pad="A1"/>
<contactref element="JP2" pad="A1"/>
</signal>
<signal name="A2">
<contactref element="U$1" pad="A2"/>
<contactref element="JP2" pad="A2"/>
</signal>
<signal name="A3">
<contactref element="U$1" pad="A3"/>
<contactref element="JP2" pad="A3"/>
</signal>
<signal name="A4/SDA">
<contactref element="U$1" pad="A4/SDA"/>
<contactref element="JP2" pad="A4/SDA"/>
</signal>
<signal name="A5/SCL">
<contactref element="U$1" pad="A5/SCL"/>
<contactref element="JP2" pad="A5/SCL"/>
</signal>
<signal name="S2-NODE">
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="JP_S1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="S3-NODE">
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="JP_S2" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND1"/>
<contactref element="JP1" pad="GND"/>
<contactref element="U$1" pad="GND"/>
<contactref element="JP2" pad="GND"/>
<contactref element="RESET" pad="3"/>
<contactref element="RESET" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="3.3V"/>
<contactref element="JP2" pad="3.3V"/>
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
