(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 1450)
    (zones 0)
    (modules 177)
    (nets 201)
  )
  (page USLetter)
  (title_block
    (title "39 Probe Switcher")
    (date 2020-01-13)
    (rev 0)
    (company "Umit H. Coskun / University of Kentucky")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 AR1)
  (net 2 GND)
  (net 3 AR2)
  (net 4 AR3)
  (net 5 AR4)
  (net 6 AR5)
  (net 7 AR6)
  (net 8 AR7)
  (net 9 AR8)
  (net 10 AR9)
  (net 11 AR10)
  (net 12 AR11)
  (net 13 AR12)
  (net 14 AR13)
  (net 15 AR14)
  (net 16 AR15)
  (net 17 AR16)
  (net 18 AR17)
  (net 19 AR18)
  (net 20 AR19)
  (net 21 AR20)
  (net 22 AR21)
  (net 23 AR22)
  (net 24 AR23)
  (net 25 AR24)
  (net 26 AR25)
  (net 27 AR26)
  (net 28 AR27)
  (net 29 AR28)
  (net 30 AR29)
  (net 31 AR30)
  (net 32 AR31)
  (net 33 AR32)
  (net 34 AR33)
  (net 35 AR34)
  (net 36 AR35)
  (net 37 AR36)
  (net 38 AR37)
  (net 39 AR38)
  (net 40 AR39)
  (net 41 1FBB)
  (net 42 1FBA)
  (net 43 1EXB)
  (net 44 1EXA)
  (net 45 2EXA)
  (net 46 2EXB)
  (net 47 2FBA)
  (net 48 2FBB)
  (net 49 3FBB)
  (net 50 3FBA)
  (net 51 3EXB)
  (net 52 3EXA)
  (net 53 4EXA)
  (net 54 4EXB)
  (net 55 4FBA)
  (net 56 4FBB)
  (net 57 5EXA)
  (net 58 5EXB)
  (net 59 5FBA)
  (net 60 5FBB)
  (net 61 6FBB)
  (net 62 6FBA)
  (net 63 6EXB)
  (net 64 6EXA)
  (net 65 7EXA)
  (net 66 7EXB)
  (net 67 7FBA)
  (net 68 7FBB)
  (net 69 8EXA)
  (net 70 8EXB)
  (net 71 8FBA)
  (net 72 8FBB)
  (net 73 9FBB)
  (net 74 9FBA)
  (net 75 9EXB)
  (net 76 9EXA)
  (net 77 10EXA)
  (net 78 10EXB)
  (net 79 10FBA)
  (net 80 10FBB)
  (net 81 11EXA)
  (net 82 11EXB)
  (net 83 11FBA)
  (net 84 11FBB)
  (net 85 12FBB)
  (net 86 12FBA)
  (net 87 12EXB)
  (net 88 12EXA)
  (net 89 13EXA)
  (net 90 13EXB)
  (net 91 13FBA)
  (net 92 13FBB)
  (net 93 14EXA)
  (net 94 14EXB)
  (net 95 14FBA)
  (net 96 14FBB)
  (net 97 15FBB)
  (net 98 15FBA)
  (net 99 15EXB)
  (net 100 15EXA)
  (net 101 16EXA)
  (net 102 16EXB)
  (net 103 16FBA)
  (net 104 16FBB)
  (net 105 17EXA)
  (net 106 17EXB)
  (net 107 17FBA)
  (net 108 17FBB)
  (net 109 18FBB)
  (net 110 18FBA)
  (net 111 18EXB)
  (net 112 18EXA)
  (net 113 19EXA)
  (net 114 19EXB)
  (net 115 19FBA)
  (net 116 19FBB)
  (net 117 20EXA)
  (net 118 20EXB)
  (net 119 20FBA)
  (net 120 20FBB)
  (net 121 21FBB)
  (net 122 21FBA)
  (net 123 21EXB)
  (net 124 21EXA)
  (net 125 22EXA)
  (net 126 22EXB)
  (net 127 22FBA)
  (net 128 22FBB)
  (net 129 23EXA)
  (net 130 23EXB)
  (net 131 23FBA)
  (net 132 23FBB)
  (net 133 24FBB)
  (net 134 24FBA)
  (net 135 24EXB)
  (net 136 24EXA)
  (net 137 25EXA)
  (net 138 25EXB)
  (net 139 25FBA)
  (net 140 25FBB)
  (net 141 26EXA)
  (net 142 26EXB)
  (net 143 26FBA)
  (net 144 26FBB)
  (net 145 27FBB)
  (net 146 27FBA)
  (net 147 27EXB)
  (net 148 27EXA)
  (net 149 28EXA)
  (net 150 28EXB)
  (net 151 28FBA)
  (net 152 28FBB)
  (net 153 29EXA)
  (net 154 29EXB)
  (net 155 29FBA)
  (net 156 29FBB)
  (net 157 30FBB)
  (net 158 30FBA)
  (net 159 30EXB)
  (net 160 30EXA)
  (net 161 31FBB)
  (net 162 31FBA)
  (net 163 31EXB)
  (net 164 31EXA)
  (net 165 32FBB)
  (net 166 32FBA)
  (net 167 32EXB)
  (net 168 32EXA)
  (net 169 33FBB)
  (net 170 33FBA)
  (net 171 33EXB)
  (net 172 33EXA)
  (net 173 34FBB)
  (net 174 34FBA)
  (net 175 34EXB)
  (net 176 34EXA)
  (net 177 35FBB)
  (net 178 35FBA)
  (net 179 35EXB)
  (net 180 35EXA)
  (net 181 36FBB)
  (net 182 36FBA)
  (net 183 36EXB)
  (net 184 36EXA)
  (net 185 37FBB)
  (net 186 37FBA)
  (net 187 37EXB)
  (net 188 37EXA)
  (net 189 38FBB)
  (net 190 38FBA)
  (net 191 38EXB)
  (net 192 38EXA)
  (net 193 39FBB)
  (net 194 39FBA)
  (net 195 39EXB)
  (net 196 39EXA)
  (net 197 EXAO)
  (net 198 EXBO)
  (net 199 FBAO)
  (net 200 FBBO)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 10EXA)
    (add_net 10EXB)
    (add_net 10FBA)
    (add_net 10FBB)
    (add_net 11EXA)
    (add_net 11EXB)
    (add_net 11FBA)
    (add_net 11FBB)
    (add_net 12EXA)
    (add_net 12EXB)
    (add_net 12FBA)
    (add_net 12FBB)
    (add_net 13EXA)
    (add_net 13EXB)
    (add_net 13FBA)
    (add_net 13FBB)
    (add_net 14EXA)
    (add_net 14EXB)
    (add_net 14FBA)
    (add_net 14FBB)
    (add_net 15EXA)
    (add_net 15EXB)
    (add_net 15FBA)
    (add_net 15FBB)
    (add_net 16EXA)
    (add_net 16EXB)
    (add_net 16FBA)
    (add_net 16FBB)
    (add_net 17EXA)
    (add_net 17EXB)
    (add_net 17FBA)
    (add_net 17FBB)
    (add_net 18EXA)
    (add_net 18EXB)
    (add_net 18FBA)
    (add_net 18FBB)
    (add_net 19EXA)
    (add_net 19EXB)
    (add_net 19FBA)
    (add_net 19FBB)
    (add_net 1EXA)
    (add_net 1EXB)
    (add_net 1FBA)
    (add_net 1FBB)
    (add_net 20EXA)
    (add_net 20EXB)
    (add_net 20FBA)
    (add_net 20FBB)
    (add_net 21EXA)
    (add_net 21EXB)
    (add_net 21FBA)
    (add_net 21FBB)
    (add_net 22EXA)
    (add_net 22EXB)
    (add_net 22FBA)
    (add_net 22FBB)
    (add_net 23EXA)
    (add_net 23EXB)
    (add_net 23FBA)
    (add_net 23FBB)
    (add_net 24EXA)
    (add_net 24EXB)
    (add_net 24FBA)
    (add_net 24FBB)
    (add_net 25EXA)
    (add_net 25EXB)
    (add_net 25FBA)
    (add_net 25FBB)
    (add_net 26EXA)
    (add_net 26EXB)
    (add_net 26FBA)
    (add_net 26FBB)
    (add_net 27EXA)
    (add_net 27EXB)
    (add_net 27FBA)
    (add_net 27FBB)
    (add_net 28EXA)
    (add_net 28EXB)
    (add_net 28FBA)
    (add_net 28FBB)
    (add_net 29EXA)
    (add_net 29EXB)
    (add_net 29FBA)
    (add_net 29FBB)
    (add_net 2EXA)
    (add_net 2EXB)
    (add_net 2FBA)
    (add_net 2FBB)
    (add_net 30EXA)
    (add_net 30EXB)
    (add_net 30FBA)
    (add_net 30FBB)
    (add_net 31EXA)
    (add_net 31EXB)
    (add_net 31FBA)
    (add_net 31FBB)
    (add_net 32EXA)
    (add_net 32EXB)
    (add_net 32FBA)
    (add_net 32FBB)
    (add_net 33EXA)
    (add_net 33EXB)
    (add_net 33FBA)
    (add_net 33FBB)
    (add_net 34EXA)
    (add_net 34EXB)
    (add_net 34FBA)
    (add_net 34FBB)
    (add_net 35EXA)
    (add_net 35EXB)
    (add_net 35FBA)
    (add_net 35FBB)
    (add_net 36EXA)
    (add_net 36EXB)
    (add_net 36FBA)
    (add_net 36FBB)
    (add_net 37EXA)
    (add_net 37EXB)
    (add_net 37FBA)
    (add_net 37FBB)
    (add_net 38EXA)
    (add_net 38EXB)
    (add_net 38FBA)
    (add_net 38FBB)
    (add_net 39EXA)
    (add_net 39EXB)
    (add_net 39FBA)
    (add_net 39FBB)
    (add_net 3EXA)
    (add_net 3EXB)
    (add_net 3FBA)
    (add_net 3FBB)
    (add_net 4EXA)
    (add_net 4EXB)
    (add_net 4FBA)
    (add_net 4FBB)
    (add_net 5EXA)
    (add_net 5EXB)
    (add_net 5FBA)
    (add_net 5FBB)
    (add_net 6EXA)
    (add_net 6EXB)
    (add_net 6FBA)
    (add_net 6FBB)
    (add_net 7EXA)
    (add_net 7EXB)
    (add_net 7FBA)
    (add_net 7FBB)
    (add_net 8EXA)
    (add_net 8EXB)
    (add_net 8FBA)
    (add_net 8FBB)
    (add_net 9EXA)
    (add_net 9EXB)
    (add_net 9FBA)
    (add_net 9FBB)
    (add_net AR1)
    (add_net AR10)
    (add_net AR11)
    (add_net AR12)
    (add_net AR13)
    (add_net AR14)
    (add_net AR15)
    (add_net AR16)
    (add_net AR17)
    (add_net AR18)
    (add_net AR19)
    (add_net AR2)
    (add_net AR20)
    (add_net AR21)
    (add_net AR22)
    (add_net AR23)
    (add_net AR24)
    (add_net AR25)
    (add_net AR26)
    (add_net AR27)
    (add_net AR28)
    (add_net AR29)
    (add_net AR3)
    (add_net AR30)
    (add_net AR31)
    (add_net AR32)
    (add_net AR33)
    (add_net AR34)
    (add_net AR35)
    (add_net AR36)
    (add_net AR37)
    (add_net AR38)
    (add_net AR39)
    (add_net AR4)
    (add_net AR5)
    (add_net AR6)
    (add_net AR7)
    (add_net AR8)
    (add_net AR9)
    (add_net EXAO)
    (add_net EXBO)
    (add_net FBAO)
    (add_net FBBO)
    (add_net GND)
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF57C)
    (at 243.767438 93.98)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D39 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 AR39))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 67.31 111.76 90)
    (fp_text reference K7 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 53 4EXA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 54 4EXB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 AR4))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 142.24 83.82 270)
    (fp_text reference K59 (at 5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 160 30EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 159 30EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 AR30))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 147.32 83.82 270)
    (fp_text reference K60 (at -5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 AR30))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 157 30FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 158 30FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BDCB0)
    (at 34.29 101.6 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (fp_text user K (at -2.54 0 180) (layer F.Fab))
    (fp_text user K (at -2.54 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 AR1))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BDCB8)
    (at 38.1 101.6)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user K (at -2.54 0) (layer F.SilkS) hide)
    (fp_text user K (at -2.54 0) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 AR2))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BDDB0)
    (at 57.15 101.6 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (fp_text user K (at -2.54 0 180) (layer F.Fab))
    (fp_text user K (at -1.27 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 AR3))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BDDD3)
    (at 60.96 101.6)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D4 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at -2.54 0) (layer F.Fab))
    (fp_text user K (at -2.54 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 AR4))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BDDFF)
    (at 80.01 101.6 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D5 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (fp_text user K (at -2.54 0 180) (layer F.Fab))
    (fp_text user K (at -2.54 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 AR5))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BDE24)
    (at 83.82 101.6)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D6 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at -2.54 0) (layer F.Fab))
    (fp_text user K (at -2.54 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 AR6))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BDE4F)
    (at 102.87 101.6 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D7 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text user K (at -2.54 0 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 AR7))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BDE6E)
    (at 106.68 101.6)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D8 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user K (at -2.54 0) (layer F.SilkS) hide)
    (fp_text user K (at -2.54 0) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 AR8))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BDEC3)
    (at 125.73 101.6 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D9 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 AR9))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BDFD4)
    (at 129.54 101.6)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D10 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 AR10))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE074)
    (at 148.59 101.6 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D11 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 AR11))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE0C7)
    (at 152.4 101.6)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D12 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 AR12))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE139)
    (at 171.45 101.6 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D13 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 AR13))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE1DA)
    (at 175.26 101.6)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D14 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 AR14))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE21A)
    (at 194.31 101.6 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D15 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 AR15))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE254)
    (at 198.12 101.6)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D16 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 AR16))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE293)
    (at 217.17 101.6 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D17 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 AR17))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE2D2)
    (at 220.98 101.6)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D18 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 AR18))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE318)
    (at 240.03 101.6 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D19 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 AR19))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE373)
    (at 34.29 93.98 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D20 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 AR20))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE3D0)
    (at 38.1 93.98)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D21 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 AR21))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE57A)
    (at 57.15 93.98 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D22 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 AR22))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE5BF)
    (at 60.887438 93.98)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D23 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 AR23))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE5FE)
    (at 80.01 93.98 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D24 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 AR24))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BE633)
    (at 83.747438 93.98)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D25 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 AR25))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF2CD)
    (at 102.87 93.98 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D26 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 AR26))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF34D)
    (at 106.607438 93.98)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D27 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 AR27))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF3BD)
    (at 125.73 93.98 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D28 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 AR28))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF3CE)
    (at 129.467438 93.98)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D29 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 AR29))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF3DB)
    (at 148.59 93.98 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D30 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 AR30))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF41D)
    (at 152.4 93.98)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D31 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 AR31))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF47E)
    (at 171.45 93.98 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D32 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 AR32))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF512)
    (at 175.187438 93.98)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D33 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 AR33))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF523)
    (at 194.31 93.98 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D34 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 AR34))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF530)
    (at 198.12 93.98)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D35 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 AR35))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF541)
    (at 217.17 93.98 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D36 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 AR36))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF54E)
    (at 220.907438 93.98)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D37 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 AR37))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5E1BF55C)
    (at 240.03 93.98 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D38 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 AR38))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 26.67 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J1 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 1FBB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 42 1FBA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 43 1EXB))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 1EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 45.72 124.46 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J2 (at 3.81 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 2EXA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 46 2EXB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 47 2FBA))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 48 2FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 49.53 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J3 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 3FBB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 50 3FBA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 3EXB))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 52 3EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 68.58 124.46 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J4 (at 3.81 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 53 4EXA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 54 4EXB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 55 4FBA))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 56 4FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 72.39 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J5 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 57 5EXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 58 5EXB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 59 5FBA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 60 5FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 91.44 124.46 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J6 (at 3.81 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 61 6FBB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 62 6FBA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 63 6EXB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 64 6EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 95.25 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J7 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 65 7EXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 66 7EXB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 67 7FBA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 68 7FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 114.3 124.46 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J8 (at 3.81 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 69 8EXA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 70 8EXB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 71 8FBA))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 72 8FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 118.11 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J9 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 73 9FBB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 74 9FBA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 75 9EXB))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 76 9EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 137.16 124.46 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J10 (at 3.81 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 77 10EXA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 78 10EXB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 79 10FBA))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 80 10FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 140.97 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J11 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 81 11EXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 82 11EXB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 83 11FBA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 84 11FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 160.02 124.46 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J12 (at 3.81 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 85 12FBB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 86 12FBA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 87 12EXB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 88 12EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 163.83 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J13 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 89 13EXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 90 13EXB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 91 13FBA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 92 13FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 182.88 124.46 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J14 (at 3.81 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 93 14EXA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 94 14EXB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 95 14FBA))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 96 14FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 186.69 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J15 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 97 15FBB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 15FBA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 99 15EXB))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 100 15EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 205.74 124.46 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J16 (at 3.81 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 101 16EXA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 102 16EXB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 103 16FBA))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 104 16FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 209.55 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J17 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 105 17EXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 106 17EXB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 107 17FBA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 108 17FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 228.6 124.46 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J18 (at 3.81 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 109 18FBB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 110 18FBA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 111 18EXB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 112 18EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 232.41 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J19 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 113 19EXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 114 19EXB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 115 19FBA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 116 19FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 26.67 71.12)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J20 (at 3.81 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 117 20EXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 118 20EXB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 119 20FBA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 120 20FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 45.72 71.12 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J21 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 121 21FBB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 122 21FBA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 123 21EXB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 124 21EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 49.53 71.12)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J22 (at 3.81 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 125 22EXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 126 22EXB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 127 22FBA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 128 22FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 68.58 71.12 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J23 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 129 23EXA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 130 23EXB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 131 23FBA))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 132 23FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 72.39 71.12)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J24 (at 3.81 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 133 24FBB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 134 24FBA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 135 24EXB))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 136 24EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 91.44 71.12 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J25 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 137 25EXA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 138 25EXB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 139 25FBA))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 140 25FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 95.25 71.12)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J26 (at 3.81 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 141 26EXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 142 26EXB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 143 26FBA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 144 26FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 114.3 71.12 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J27 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 145 27FBB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 146 27FBA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 147 27EXB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 148 27EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 118.11 71.12)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J28 (at 3.81 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 149 28EXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 150 28EXB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 151 28FBA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 152 28FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 137.16 71.12 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J29 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 153 29EXA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 154 29EXB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 155 29FBA))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 156 29FBB))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 140.97 71.12)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J30 (at 3.81 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 157 30FBB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 158 30FBA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 159 30EXB))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 160 30EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 160.02 71.12 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J31 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 161 31FBB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 162 31FBA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 163 31EXB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 164 31EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 163.83 71.12)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J32 (at 3.81 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 165 32FBB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 166 32FBA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 167 32EXB))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 168 32EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 182.88 71.12 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J33 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 169 33FBB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 170 33FBA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 171 33EXB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 172 33EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 186.617438 71.12)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J34 (at 3.81 -3.81 -180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 173 34FBB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 174 34FBA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 175 34EXB))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 176 34EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 205.74 71.12 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J35 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 177 35FBB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 178 35FBA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 179 35EXB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 180 35EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 209.477438 71.12)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J36 (at 3.882562 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 181 36FBB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 182 36FBA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 183 36EXB))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 184 36EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 228.6 71.12 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J37 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 185 37FBB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 186 37FBA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 187 37EXB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 188 37EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 232.41 71.12)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J38 (at 3.81 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 189 38FBB))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 190 38FBA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 191 38EXB))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 192 38EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 251.46 71.12 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J39 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 193 39FBB))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 194 39FBA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 195 39EXB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 196 39EXA))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 27.94 111.76 90)
    (fp_text reference K1 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 1EXA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 1EXB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 AR1))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 33.02 111.76 90)
    (fp_text reference K2 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 AR1))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 1FBB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 1FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 44.45 111.76 90)
    (fp_text reference K3 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 AR2))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 46 2EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 45 2EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 39.37 111.76 90)
    (fp_text reference K4 (at -6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 47 2FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 48 2FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 AR2))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 50.8 111.76 90)
    (fp_text reference K5 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 AR3))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 51 3EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 52 3EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 55.88 111.76 90)
    (fp_text reference K6 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 50 3FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 49 3FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 AR3))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 62.23 111.76 90)
    (fp_text reference K8 (at -6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 AR4))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 56 4FBB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 55 4FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 73.66 111.76 90)
    (fp_text reference K9 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 AR5))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 58 5EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 57 5EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 78.74 111.76 90)
    (fp_text reference K10 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 59 5FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 60 5FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 AR5))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 90.17 111.76 90)
    (fp_text reference K11 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 AR6))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 63 6EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 64 6EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 85.09 111.76 90)
    (fp_text reference K12 (at -6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 62 6FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 61 6FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 AR6))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 96.52 111.76 90)
    (fp_text reference K13 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 65 7EXA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 7EXB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 AR7))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 101.6 111.76 90)
    (fp_text reference K14 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 AR7))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 68 7FBB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 7FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 113.03 111.76 90)
    (fp_text reference K15 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 AR8))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 70 8EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 69 8EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 107.95 111.76 90)
    (fp_text reference K16 (at -6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 71 8FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 72 8FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 AR8))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 119.38 111.76 90)
    (fp_text reference K17 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 AR9))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 75 9EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 76 9EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 124.46 111.76 90)
    (fp_text reference K18 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 74 9FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 73 9FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 AR9))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 135.89 111.76 90)
    (fp_text reference K19 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 77 10EXA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 78 10EXB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 AR10))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 130.81 111.76 90)
    (fp_text reference K20 (at -6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 AR10))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 80 10FBB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 79 10FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 142.24 111.76 90)
    (fp_text reference K21 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 AR11))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 82 11EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 81 11EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 147.32 111.76 90)
    (fp_text reference K22 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 83 11FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 84 11FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 AR11))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 158.75 111.76 90)
    (fp_text reference K23 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 AR12))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 87 12EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 88 12EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 153.67 111.76 90)
    (fp_text reference K24 (at -6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 86 12FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 85 12FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 AR12))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 165.1 111.76 90)
    (fp_text reference K25 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 89 13EXA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 90 13EXB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 AR13))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 170.18 111.76 90)
    (fp_text reference K26 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 AR13))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 92 13FBB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 91 13FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 181.61 111.76 90)
    (fp_text reference K27 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 93 14EXA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 94 14EXB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 AR14))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 176.53 111.76 90)
    (fp_text reference K28 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 95 14FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 96 14FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 AR14))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 187.96 111.76 90)
    (fp_text reference K29 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 AR15))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 99 15EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 100 15EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 193.04 111.76 90)
    (fp_text reference K30 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 98 15FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 97 15FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 AR15))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 204.47 111.76 90)
    (fp_text reference K31 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 AR16))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 102 16EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 101 16EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 199.39 111.76 90)
    (fp_text reference K32 (at -6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 103 16FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 104 16FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 AR16))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 210.82 111.76 90)
    (fp_text reference K33 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 105 17EXA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 106 17EXB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 AR17))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 215.9 111.76 90)
    (fp_text reference K34 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 AR17))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 108 17FBB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 107 17FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 227.33 111.76 90)
    (fp_text reference K35 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 112 18EXA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 111 18EXB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 AR18))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 222.25 111.76 90)
    (fp_text reference K36 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 AR18))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 109 18FBB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 110 18FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 233.68 111.76 90)
    (fp_text reference K37 (at 6.35 2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 AR19))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 114 19EXB))
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 113 19EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 238.76 111.76 90)
    (fp_text reference K38 (at -6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 115 19FBA))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 116 19FBB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 AR19))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 27.867438 83.82 270)
    (fp_text reference K39 (at 5.08 -2.612562 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 AR20))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 118 20EXB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 117 20EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 32.947438 83.82 270)
    (fp_text reference K40 (at -5.08 2.467438 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 AR20))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 120 20FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 119 20FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 44.45 83.82 270)
    (fp_text reference K41 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 AR21))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 123 21EXB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 124 21EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 39.37 83.82 270)
    (fp_text reference K42 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 122 21FBA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 121 21FBB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 AR21))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 50.8 83.82 270)
    (fp_text reference K43 (at 5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 22EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 126 22EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 AR22))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 55.88 83.82 270)
    (fp_text reference K44 (at -5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 AR22))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 128 22FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 127 22FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 67.31 83.82 270)
    (fp_text reference K45 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 129 23EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 130 23EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 AR23))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 62.23 83.82 270)
    (fp_text reference K46 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 AR23))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 132 23FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 131 23FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 73.66 83.82 270)
    (fp_text reference K47 (at 5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 136 24EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 135 24EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 AR24))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 78.74 83.82 270)
    (fp_text reference K48 (at -5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 AR24))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 133 24FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 134 24FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 90.17 83.82 270)
    (fp_text reference K49 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 AR25))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 138 25EXB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 137 25EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 85.09 83.82 270)
    (fp_text reference K50 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 139 25FBA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 140 25FBB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 AR25))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 96.52 83.82 270)
    (fp_text reference K51 (at 5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 141 26EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 142 26EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 AR26))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 101.6 83.82 270)
    (fp_text reference K52 (at -5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 143 26FBA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 144 26FBB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 AR26))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 113.03 83.82 270)
    (fp_text reference K53 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 148 27EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 147 27EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 AR27))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 107.95 83.82 270)
    (fp_text reference K54 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 AR27))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 145 27FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 146 27FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 119.38 83.82 270)
    (fp_text reference K55 (at 5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 AR28))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 150 28EXB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 149 28EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 124.46 83.82 270)
    (fp_text reference K56 (at -5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 151 28FBA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 152 28FBB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 AR28))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 135.89 83.82 270)
    (fp_text reference K57 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 153 29EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 154 29EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 AR29))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 130.81 83.82 270)
    (fp_text reference K58 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 AR29))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 156 29FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 155 29FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 158.75 83.82 270)
    (fp_text reference K61 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 AR31))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 163 31EXB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 164 31EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 153.67 83.82 270)
    (fp_text reference K62 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 162 31FBA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 161 31FBB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 AR31))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 165.1 83.82 270)
    (fp_text reference K63 (at 5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 AR32))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 167 32EXB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 168 32EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 170.18 83.82 270)
    (fp_text reference K64 (at -5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 166 32FBA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 165 32FBB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 AR32))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 181.61 83.82 270)
    (fp_text reference K65 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 AR33))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 171 33EXB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 172 33EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 176.475506 83.82 270)
    (fp_text reference K66 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 AR33))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 169 33FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 170 33FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 187.96 83.82 270)
    (fp_text reference K67 (at 5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 176 34EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 175 34EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 AR34))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 193.04 83.82 270)
    (fp_text reference K68 (at -5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 AR34))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 173 34FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 174 34FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 204.47 83.82 270)
    (fp_text reference K69 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 AR35))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 179 35EXB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 180 35EXA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 199.335506 83.82 270)
    (fp_text reference K70 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 178 35FBA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 177 35FBB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 AR35))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 210.82 83.82 270)
    (fp_text reference K71 (at 5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 184 36EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 183 36EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 AR36))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 215.9 83.82 270)
    (fp_text reference K72 (at -5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 AR36))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 181 36FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 182 36FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 227.33 83.82 270)
    (fp_text reference K73 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 188 37EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 187 37EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 AR37))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 222.195506 83.82 270)
    (fp_text reference K74 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 AR37))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 185 37FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 186 37FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 233.68 83.82 270)
    (fp_text reference K75 (at 5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 192 38EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 191 38EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 AR38))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 238.76 83.82 270)
    (fp_text reference K76 (at -5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 AR38))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 189 38FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 190 38FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 250.19 83.82 270)
    (fp_text reference K77 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 196 39EXA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 195 39EXB))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 AR39))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Coto9092:Coto9092 (layer F.Cu) (tedit 5E1BD05B)
    (at 245.11 83.82 270)
    (fp_text reference K78 (at -5.08 -2.54 270) (layer F.SilkS))
    (fp_text value Coto9092 (at -5.08 -3.81 270) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 AR39))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 193 39FBB))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 194 39FBA))
    (model ${KIPRJMOD}/Coto9092.pretty/9092.stp
      (offset (xyz -7.619999885559082 1.650999975204468 1.269999980926514))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 31.75 97.79 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J41 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 AR2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 AR1))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 54.61 97.79 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J42 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 AR3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 AR4))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 77.47 97.79 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J43 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 AR6))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 AR5))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 100.33 97.79 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J44 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 AR7))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 AR8))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 123.19 97.79 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J45 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 AR10))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 AR9))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 146.05 97.79 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J46 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 AR12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 AR11))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 168.91 97.79 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J47 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 AR13))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 AR14))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 191.77 97.79 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J48 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 AR16))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 AR15))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 214.63 97.79 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J49 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 AR18))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 AR17))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 234.95 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J50 (at 0 5.08 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 AR19))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 40.64 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J51 (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 AR20))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 AR21))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 63.5 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J52 (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 AR23))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 AR22))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 86.36 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J53 (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 AR25))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 AR24))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 109.22 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J54 (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 AR26))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 AR27))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 132.08 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J55 (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 AR29))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 AR28))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 154.94 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J56 (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 AR30))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 AR31))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 177.8 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J57 (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 AR33))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 AR32))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 200.66 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J58 (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 AR35))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 AR34))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 223.52 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J59 (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 AR36))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 AR37))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 241.3 97.79 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J60 (at 0 -2.77 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 5.31 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 AR39))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 AR38))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 243.84 124.46)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J40 (at 3.81 3.81) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 200 FBBO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 198 EXBO))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 199 FBAO))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 197 EXAO))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "39 Probe Switcher\nRev 0\n1/13/2020" (at 250.825 117.475 270) (layer B.SilkS))
  (gr_line (start 257.81 64.77) (end 20.32 64.77) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 257.81 130.81) (end 257.81 64.77) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.32 130.81) (end 257.81 130.81) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.32 64.77) (end 20.32 130.81) (layer Edge.Cuts) (width 0.15))
  (gr_text FBBO (at 243.84 117.475 90) (layer F.SilkS))
  (gr_text FBAO (at 248.92 117.475 90) (layer F.SilkS))
  (gr_text EXBO (at 246.38 117.475 90) (layer F.SilkS))
  (gr_text EXAO (at 251.46 117.475 90) (layer F.SilkS))
  (gr_text "MAG-01H\nOUTPUT" (at 247.015 107.95) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45.72 113.03) (xy 49.53 113.03) (xy 48.26 111.76) (xy 48.26 102.87) (xy 49.53 101.6)
        (xy 45.72 101.6) (xy 46.99 102.87) (xy 46.99 111.76)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45.72 101.6) (xy 49.53 101.6) (xy 49.53 93.98) (xy 45.72 93.98)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45.72 93.98) (xy 46.99 92.71) (xy 46.99 83.82) (xy 45.72 82.55) (xy 49.53 82.55)
        (xy 48.26 83.82) (xy 48.26 92.71) (xy 49.53 93.98)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.58 113.03) (xy 72.39 113.03) (xy 71.12 111.76) (xy 71.12 102.87) (xy 72.39 101.6)
        (xy 68.58 101.6) (xy 69.85 102.87) (xy 69.85 111.76)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.39 101.6) (xy 72.39 93.98) (xy 68.58 93.98) (xy 68.58 101.6)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.58 93.98) (xy 72.39 93.98) (xy 71.12 92.71) (xy 71.12 83.82) (xy 72.39 82.55)
        (xy 68.58 82.55) (xy 69.85 83.82) (xy 69.85 92.71)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.44 113.03) (xy 95.25 113.03) (xy 93.98 111.76) (xy 93.98 102.87) (xy 95.25 101.6)
        (xy 91.44 101.6) (xy 92.71 102.87) (xy 92.71 111.76)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.44 93.98) (xy 91.44 101.6) (xy 95.25 101.6) (xy 95.25 93.98)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.44 93.98) (xy 95.25 93.98) (xy 93.98 92.71) (xy 93.98 83.82) (xy 95.25 82.55)
        (xy 91.44 82.55) (xy 92.71 83.82) (xy 92.71 92.71)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 113.03) (xy 118.11 113.03) (xy 116.84 111.76) (xy 116.84 102.87) (xy 118.11 101.6)
        (xy 118.11 93.98) (xy 116.84 92.71) (xy 116.84 83.82) (xy 118.11 82.55) (xy 114.3 82.55)
        (xy 115.57 83.82) (xy 115.57 92.71) (xy 114.3 93.98) (xy 114.3 101.6) (xy 115.57 102.87)
        (xy 115.57 111.76)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 205.74 113.03) (xy 209.55 113.03) (xy 208.28 111.76) (xy 208.28 102.87) (xy 209.55 101.6)
        (xy 209.55 93.98) (xy 208.28 92.71) (xy 208.28 83.82) (xy 209.55 82.55) (xy 205.74 82.55)
        (xy 207.01 83.82) (xy 207.01 92.71) (xy 205.74 93.98) (xy 205.74 101.6) (xy 207.01 102.87)
        (xy 207.01 111.76)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 182.88 113.03) (xy 186.69 113.03) (xy 185.42 111.76) (xy 185.42 102.87) (xy 186.69 101.6)
        (xy 186.69 93.98) (xy 185.42 92.71) (xy 185.42 83.82) (xy 186.69 82.55) (xy 182.88 82.55)
        (xy 184.15 83.82) (xy 184.15 92.71) (xy 182.88 93.98) (xy 182.88 101.6) (xy 184.15 102.87)
        (xy 184.15 111.76)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 113.03) (xy 163.83 113.03) (xy 162.56 111.76) (xy 162.56 102.87) (xy 163.83 101.6)
        (xy 163.83 93.98) (xy 162.56 92.71) (xy 162.56 83.82) (xy 163.83 82.55) (xy 160.02 82.55)
        (xy 161.29 83.82) (xy 161.29 92.71) (xy 160.02 93.98) (xy 160.02 101.6) (xy 161.29 102.87)
        (xy 161.29 111.76)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.97 113.03) (xy 139.7 111.76) (xy 139.7 102.87) (xy 140.97 101.6) (xy 140.97 93.98)
        (xy 139.7 92.71) (xy 139.7 83.82) (xy 140.97 82.55) (xy 137.16 82.55) (xy 138.43 83.82)
        (xy 138.43 92.71) (xy 137.16 93.98) (xy 137.16 101.6) (xy 138.43 102.87) (xy 138.43 111.76)
        (xy 137.16 113.03)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232.41 113.03) (xy 231.14 111.76) (xy 231.14 102.87) (xy 232.41 101.6) (xy 232.41 97.79)
        (xy 232.41 93.98) (xy 231.14 92.71) (xy 231.14 83.82) (xy 232.41 82.55) (xy 228.6 82.55)
        (xy 229.87 83.82) (xy 229.87 92.71) (xy 228.6 93.98) (xy 228.6 101.6) (xy 229.87 102.87)
        (xy 229.87 111.76) (xy 228.6 113.03)
      )
    )
  )
)
