(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 18)
    (no_connects 1)
    (area 106.553 83.439 229.235 148.463)
    (thickness 1.6)
    (drawings 25)
    (tracks 245)
    (zones 0)
    (modules 15)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad5)")
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad7)")
  (net 5 "Net-(J1-Pad8)")
  (net 6 "Net-(J1-Pad17A)")
  (net 7 "Net-(J1-Pad3V1)")
  (net 8 "Net-(J1-PadG2)")
  (net 9 "Net-(J1-PadPGM)")
  (net 10 "Net-(J1-PadDAC)")
  (net 11 "Net-(J1-PadG3)")
  (net 12 "Net-(J1-PadVIN)")
  (net 13 "Net-(J1-Pad21)")
  (net 14 "Net-(J1-Pad20)")
  (net 15 "Net-(J1-Pad14)")
  (net 16 /CS)
  (net 17 /RST)
  (net 18 /GND)
  (net 19 /VIN)
  (net 20 /Data)
  (net 21 /CLK)
  (net 22 /DC)
  (net 23 "Net-(J2-Pad3)")
  (net 24 "Net-(CAP0-Pad1)")
  (net 25 "Net-(CAP1-Pad1)")
  (net 26 "Net-(CAP3-Pad1)")
  (net 27 "Net-(CAP4-Pad1)")
  (net 28 /CAP16)
  (net 29 /CAP18)
  (net 30 /CAP17)
  (net 31 /CAP22)
  (net 32 /CAP19)
  (net 33 /CAP23)
  (net 34 /CAP15)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CAP15)
    (add_net /CAP16)
    (add_net /CAP17)
    (add_net /CAP18)
    (add_net /CAP19)
    (add_net /CAP22)
    (add_net /CAP23)
    (add_net /CLK)
    (add_net /CS)
    (add_net /DC)
    (add_net /Data)
    (add_net /GND)
    (add_net /RST)
    (add_net /VIN)
    (add_net "Net-(CAP0-Pad1)")
    (add_net "Net-(CAP1-Pad1)")
    (add_net "Net-(CAP3-Pad1)")
    (add_net "Net-(CAP4-Pad1)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad17A)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad3V1)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadG2)")
    (add_net "Net-(J1-PadG3)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVIN)")
    (add_net "Net-(J2-Pad3)")
  )
  (module Wickerlib:TEENSY-LC (layer F.Cu) (tedit 578C46F8)
    (at 151.511 105.918)
    (fp_text reference J1 (at 2.8829 20.2184) (layer F.SilkS) hide)
    (fp_text value TEENSY-LC (at -2.54 20.32) (layer F.Fab))
    (fp_text user "TEENSY LC" (at -3.5941 10.5664) (layer F.SilkS) hide)
    (pad G1 thru_hole circle (at -10.16 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /GND))
    (pad 0 thru_hole circle (at -10.16 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(CAP0-Pad1)"))
    (pad 1 thru_hole circle (at -10.16 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(CAP1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(CAP3-Pad1)"))
    (pad 4 thru_hole circle (at -10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(CAP4-Pad1)"))
    (pad 5 thru_hole circle (at -10.16 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /Data))
    (pad 10 thru_hole circle (at -10.16 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /CLK))
    (pad 11 thru_hole circle (at -10.16 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /DC))
    (pad 12 thru_hole circle (at -10.16 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /CS))
    (pad 17A thru_hole circle (at -7.62 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad17A)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad3V1)"))
    (pad G2 thru_hole circle (at -2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-PadG2)"))
    (pad PGM thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /RST))
    (pad 16 thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /CAP16))
    (pad 3V2 thru_hole circle (at 5.08 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /VIN))
    (pad 18 thru_hole circle (at 5.08 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /CAP18))
    (pad 17 thru_hole circle (at 5.08 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CAP17))
    (pad G3 thru_hole circle (at 5.08 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-PadG3)"))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /CAP22))
    (pad VIN thru_hole circle (at 5.08 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /CAP19))
    (pad 23 thru_hole circle (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /CAP23))
    (pad 14 thru_hole circle (at 5.08 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /CAP15))
  )
  (module Wickerlib:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 5773C0FA)
    (at 167.767 133.985 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module Wickerlib:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 5773C005)
    (at 168.91 108.077)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value OLED_128x64 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /VIN))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /CS))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /RST))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /DC))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /CLK))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /Data))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C810C)
    (at 114.3 97.155)
    (fp_text reference CAP0 (at 0.127 0) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 24 "Net-(CAP0-Pad1)") (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C8085)
    (at 128.905 93.472 90)
    (fp_text reference CAP1 (at 0 0 360) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0 90) (size 10.16 10.16) (layers F.Cu)
      (net 25 "Net-(CAP1-Pad1)") (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C8037)
    (at 114.427 111.379)
    (fp_text reference CAP3 (at 0 0) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 26 "Net-(CAP3-Pad1)") (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C803D)
    (at 128.524 107.061)
    (fp_text reference CAP4 (at 0 0) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 27 "Net-(CAP4-Pad1)") (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C80DE)
    (at 115.062 125.476)
    (fp_text reference CAP15 (at 0 0.127) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 34 /CAP15) (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C80DA)
    (at 128.524 121.412)
    (fp_text reference CAP16 (at -0.0889 0.1651) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 28 /CAP16) (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C8103)
    (at 115.57 139.573)
    (fp_text reference CAP17 (at 0 -0.3175) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 30 /CAP17) (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C8106)
    (at 128.778 136.144)
    (fp_text reference CAP18 (at 0 -0.3175) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 29 /CAP18) (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C8067)
    (at 142.367 139.827)
    (fp_text reference CAP19 (at -0.254 0.3556) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 32 /CAP19) (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C80E4)
    (at 157.48 139.954)
    (fp_text reference CAP22 (at -0.4064 0.0889) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 31 /CAP22) (clearance 0.508))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578C80D3)
    (at 165.227 99.695)
    (fp_text reference CAP23 (at -0.127 0.1016) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 33 /CAP23) (clearance 0.508))
  )
  (module teensy-big-oled:oshpark-silk-dpi72 (layer B.Cu) (tedit 0)
    (at 140.843 116.967)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text "DREW FUSTINI" (at 151.511 88.646) (layer F.Mask))
  (gr_text "drew@oshpark.com\n" (at 150.876 91.186) (layer B.Mask))
  (gr_text "drew@oshpark.com\n" (at 151.765 91.186) (layer F.Mask))
  (gr_text "DREW FUSTINI" (at 108.458 106.299 270) (layer F.SilkS))
  (gr_text "DREW FUSTINI" (at 165.354 112.141 270) (layer F.SilkS))
  (gr_text "drew@oshpark.com\n" (at 162.306 119.253 270) (layer F.SilkS))
  (gr_circle (center 168.402 141.859) (end 167.386 139.7) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 168.275 90.297) (end 167.259 88.138) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 166.624 86.106) (end 169.672 86.106) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 166.243 146.05) (end 169.418 146.05) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106.934 143.637) (end 106.934 89.154) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 166.497 146.05) (end 109.855 146.05) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 172.974 90.043) (end 172.974 142.748) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 110.744 86.106) (end 167.005 86.106) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 109.601 143.383) (end 109.855 146.05) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 169.291 142.367) (end 172.974 142.621) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 169.418 89.662) (end 169.672 86.106) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 110.363 89.535) (end 106.934 89.154) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_text "drew@oshpark.com\n" (at 128.778 144.272) (layer F.SilkS))
  (gr_text "drew@oshpark.com\n" (at 109.22 131.064 270) (layer F.SilkS))
  (gr_text "DREW FUSTINI" (at 151.511 88.646) (layer B.Mask))
  (zone (net 18) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.973 86.868) (xy 111.125 86.868) (xy 109.093 87.503) (xy 107.823 89.027) (xy 107.823 143.891)
        (xy 108.204 144.526) (xy 108.966 145.161) (xy 109.347 145.415) (xy 166.878 145.415) (xy 167.132 145.415)
        (xy 167.386 145.415) (xy 169.672 145.034) (xy 171.196 144.526) (xy 171.831 143.129) (xy 171.831 87.757)
        (xy 170.688 86.995) (xy 169.672 86.868) (xy 167.894 86.868) (xy 166.878 86.868) (xy 164.973 86.868)
      )
    )
  )
)
