(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 7)
    (no_connects 5)
    (area 143.434999 98.984999 153.745001 109.364)
    (thickness 1.6)
    (drawings 16)
    (tracks 0)
    (zones 0)
    (modules 1)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad6)")
  (net 2 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad6)")
  )
  (module Connectors_USB:USB_Micro-B_Molex-105017-0001 (layer F.Cu) (tedit 598B308E)
    (at 148.5011 104.839)
    (descr http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
    (tags "Micro-USB SMD Typ-B")
    (attr smd)
    (fp_text reference J1 (at 0 -4) (layer F.SilkS))
    (fp_text value USB_OTG (at 0.3 3.45) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 1.8) (layer Dwgs.User))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 1 0.35) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at -2.5 -2.35) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at -0.65 -2.35) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.3 -2.35) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -2.35) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 -2.35) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -2.35) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 6 thru_hole circle (at 2.5 -2.35) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at -1 0.35) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad6)"))
    (pad 6 thru_hole oval (at -3.5 0.35 180) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad6)"))
    (pad 6 thru_hole oval (at 3.5 0.35) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 2.9 0.35) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at -2.9 0.35) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-Pad6)"))
    (model /home/rob/usb-example/Molex_Mirco_USB_105017-0001.wrl
      (at (xyz 0 0.09 -0.03))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 151.68 104.73) (end 151.68 105.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 151.99 104.91) (end 151.73 104.66) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 151.98 105.51) (end 152.26 105.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.29 104.72) (end 152.29 105.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.29 104.67) (end 145.29 105.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.98 105.46) (end 145.26 105.72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.99 104.86) (end 144.73 104.61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.68 104.68) (end 144.68 105.64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.78 105.41) (end 144.78 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.4 105.41) (end 153.67 105.41) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.4 100.33) (end 152.4 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.78 100.33) (end 143.51 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 106.68) (end 152.4 106.68) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 100.33) (end 153.67 105.41) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 99.06) (end 152.4 99.06) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.51 100.33) (end 143.51 105.41) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.51 99.06) (xy 153.67 99.06) (xy 153.67 106.68) (xy 143.51 106.68)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.51 99.06) (xy 153.67 99.06) (xy 153.67 106.68) (xy 143.51 106.68)
      )
    )
  )
)
