(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "SDP25 Schematic V2")
    (date "2024-11-08")
    (company "Team 14: Auditory-Vibration Assistant (AVA)")
    (comment 1 "Steven Huang")
    (comment 2 "Kishen Patil")
    (comment 3 "Kyle Auyeung")
    (comment 4 "Tyler Russel")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "G18")
  (net 3 "G19")
  (net 4 "3V")
  (net 5 "unconnected-(SW2-Pad1)")
  (net 6 "unconnected-(SW2-Pad2)")
  (net 7 "unconnected-(SW2-Pad5)")
  (net 8 "unconnected-(U1-EN-PadJ5_18)")
  (net 9 "unconnected-(U1-5V-PadJ5_1)")
  (net 10 "unconnected-(U1-SP-PadJ5_17)")
  (net 11 "unconnected-(U1-SN-PadJ5_16)")
  (net 12 "unconnected-(U1-G34-PadJ5_15)")
  (net 13 "unconnected-(U1-G35-PadJ5_14)")
  (net 14 "G32")
  (net 15 "G33")
  (net 16 "unconnected-(U1-SD2-PadJ5_4)")
  (net 17 "unconnected-(U1-SD3-PadJ5_3)")
  (net 18 "unconnected-(U1-CMD-PadJ5_2)")
  (net 19 "unconnected-(U1-CLK-PadJ4_19)")
  (net 20 "unconnected-(U1-SD0-PadJ4_18)")
  (net 21 "unconnected-(U1-SD1-PadJ4_17)")
  (net 22 "unconnected-(U1-G15-PadJ4_16)")
  (net 23 "unconnected-(U1-G21-PadJ4_6)")
  (net 24 "unconnected-(U1-RXD-PadJ4_5)")
  (net 25 "unconnected-(U1-TXD-PadJ4_4)")
  (net 26 "unconnected-(U1-G22-PadJ4_3)")
  (net 27 "unconnected-(U1-G23-PadJ4_2)")
  (net 28 "unconnected-(U1-GND_J4_1-PadJ4_1)")
  (net 29 "Net-(D1-A)")
  (net 30 "5V")
  (net 31 "GND")
  (net 32 "Net-(U2-+)")
  (net 33 "PA1")
  (net 34 "Net-(U3-+)")
  (net 35 "PA2")
  (net 36 "unconnected-(U1-GND_J4_7-PadJ4_7)")
  (net 37 "unconnected-(U1-G5-PadJ4_10)")
  (net 38 "unconnected-(U1-G17-PadJ4_11)")
  (net 39 "unconnected-(U1-G16-PadJ4_12)")
  (net 40 "unconnected-(U1-G4-PadJ4_13)")
  (net 41 "unconnected-(U1-G0-PadJ4_14)")
  (net 42 "unconnected-(U1-G2-PadJ4_15)")
  (net 43 "unconnected-(U1-G13-PadJ5_5)")
  (net 44 "unconnected-(U1-G12-PadJ5_7)")
  (net 45 "unconnected-(U1-G14-PadJ5_8)")
  (net 46 "unconnected-(U1-G27-PadJ5_9)")
  (net 47 "unconnected-(U1-G26-PadJ5_10)")
  (net 48 "unconnected-(U1-G25-PadJ5_11)")
  (net 49 "unconnected-(U2-GAIN-Pad1)")
  (net 50 "unconnected-(U2-BYPASS-Pad7)")
  (net 51 "unconnected-(U2-GAIN-Pad8)")
  (net 52 "unconnected-(U3-GAIN-Pad1)")
  (net 53 "unconnected-(U3-BYPASS-Pad7)")
  (net 54 "unconnected-(U3-GAIN-Pad8)")
  (net 55 "Net-(C7-Pad1)")
  (net 56 "Net-(C7-Pad2)")
  (net 57 "Net-(C9-Pad1)")
  (net 58 "Net-(C10-Pad2)")
  (footprint "digikey-footprints:PinHeader_1x3_P2.54_Drill1.1mm" (layer "F.Cu")
    (at 116.84 91.44 90)
    (property "Category" "Connectors, Interconnects")
    (property "DK_Datasheet_Link" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=640456&DocType=Customer+Drawing&DocLang=English")
    (property "DK_Detail_Page" "/product-detail/en/te-connectivity-amp-connectors/640456-3/A19470-ND/259010")
    (property "Description" "CONN HEADER VERT 3POS 2.54MM")
    (property "Digi-Key_PN" "A19470-ND")
    (property "Family" "Rectangular Connectors - Headers, Male Pins")
    (property "MPN" "640456-3")
    (property "Manufacturer" "TE Connectivity AMP Connectors")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (property "ki_description" "CONN HEADER VERT 3POS 2.54MM")
    (property "ki_keywords" "A19470-ND MTA-100")
    (attr through_hole)
    (fp_text reference "J2" (at 7.62 0 180) (layer "F.SilkS"))
    (fp_text value "Mic 1" (at 2.54 -2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 30 "5V") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 33 "PA1") (pintype "passive"))
  )
  (footprint "digikey-footprints:PinHeader_1x3_P2.54_Drill1.1mm" (layer "F.Cu")
    (at 176.53 102.87 90)
    (property "Category" "Connectors, Interconnects")
    (property "DK_Datasheet_Link" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=640456&DocType=Customer+Drawing&DocLang=English")
    (property "DK_Detail_Page" "/product-detail/en/te-connectivity-amp-connectors/640456-3/A19470-ND/259010")
    (property "Description" "CONN HEADER VERT 3POS 2.54MM")
    (property "Digi-Key_PN" "A19470-ND")
    (property "Family" "Rectangular Connectors - Headers, Male Pins")
    (property "MPN" "640456-3")
    (property "Manufacturer" "TE Connectivity AMP Connectors")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (property "ki_description" "CONN HEADER VERT 3POS 2.54MM")
    (property "ki_keywords" "A19470-ND MTA-100")
    (attr through_hole)
    (fp_text reference "J6" (at 7.62 0 180) (layer "F.SilkS"))
    (fp_text value "Motor Driver 1" (at 2.71 2.7 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "G18") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "G19") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 137.16 107.99 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C9" (at 7.58 0 -180) (layer "F.SilkS"))
    (fp_text value "50 nF" (at 2.5 2.85 -270) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 140.97 105.41 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 1.27 2.54 90) (layer "F.SilkS"))
    (fp_text value "27 ohm" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "G33") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 121.92 82.59 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 2.54 -270) (layer "F.SilkS"))
    (fp_text value "100 nF" (at 2.5 2.85 -270) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(U2-+)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "PA1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 140.97 99.06 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 1.27 2.54 90) (layer "F.SilkS"))
    (fp_text value "27 ohm" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "G33") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 152.4 69.85)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 1.27 -2.37) (layer "F.SilkS"))
    (fp_text value "43 ohm" (at 1.27 2.37) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 -2.37) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:PinHeader_1x2_P2.54mm" (layer "F.Cu")
    (at 132.08 71.12 -90)
    (property "Category" "Connectors, Interconnects")
    (property "DK_Datasheet_Link" "https://cdn.harwin.com/pdfs/M20-999.pdf")
    (property "DK_Detail_Page" "/product-detail/en/harwin-inc/M20-9990246/952-2262-ND/3728226")
    (property "Description" "CONN HEADER VERT 2POS 2.54MM")
    (property "Digi-Key_PN" "952-2262-ND")
    (property "Family" "Rectangular Connectors - Headers, Male Pins")
    (property "MPN" "M20-9990246")
    (property "Manufacturer" "Harwin Inc.")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (property "ki_description" "CONN HEADER VERT 2POS 2.54MM")
    (property "ki_keywords" "952-2262-ND M20")
    (attr through_hole)
    (fp_text reference "J1" (at -2.54 0 -180) (layer "F.SilkS"))
    (fp_text value "5V" (at 1.27 2.54 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0.02 270) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 161.29 69.85 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D1" (at 1.27 -3.96 270) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 146.05 69.85)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 1.27 -2.37) (layer "F.SilkS"))
    (fp_text value "3.4 ohm" (at 1.27 2.37) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 -2.37) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 128.31 78.74)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 -2.85) (layer "F.SilkS"))
    (fp_text value "10 uF" (at 2.5 2.85) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:PinHeader_1x3_P2.54_Drill1.1mm" (layer "F.Cu")
    (at 116.84 110.49 90)
    (property "Category" "Connectors, Interconnects")
    (property "DK_Datasheet_Link" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=640456&DocType=Customer+Drawing&DocLang=English")
    (property "DK_Detail_Page" "/product-detail/en/te-connectivity-amp-connectors/640456-3/A19470-ND/259010")
    (property "Description" "CONN HEADER VERT 3POS 2.54MM")
    (property "Digi-Key_PN" "A19470-ND")
    (property "Family" "Rectangular Connectors - Headers, Male Pins")
    (property "MPN" "640456-3")
    (property "Manufacturer" "TE Connectivity AMP Connectors")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (property "ki_description" "CONN HEADER VERT 3POS 2.54MM")
    (property "ki_keywords" "A19470-ND MTA-100")
    (attr through_hole)
    (fp_text reference "J3" (at 7.62 0 180) (layer "F.SilkS"))
    (fp_text value "Mic 2" (at 2.71 -2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 30 "5V") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 35 "PA2") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 140.97 111.76 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 1.27 2.54 90) (layer "F.SilkS"))
    (fp_text value "10 ohm" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(C9-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 140.97 92.71 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 1.27 2.54 90) (layer "F.SilkS"))
    (fp_text value "10 ohm" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(C7-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (at 125.74 102.88)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Low Voltage Audio Power Amplifier, DIP-8/SOIC-8/SSOP-8")
    (property "ki_keywords" "single Power opamp")
    (attr through_hole)
    (fp_text reference "U3" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "LM386" (at 3.81 9.95) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(U3-GAIN-Pad1)") (pinfunction "GAIN") (pintype "input+no_connect"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(U3-+)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(C10-Pad2)") (pintype "output"))
    (pad "6" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "5V") (pinfunction "V+") (pintype "power_in"))
    (pad "7" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(U3-BYPASS-Pad7)") (pinfunction "BYPASS") (pintype "input+no_connect"))
    (pad "8" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(U3-GAIN-Pad8)") (pinfunction "GAIN") (pintype "input+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (at 125.74 83.83)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Low Voltage Audio Power Amplifier, DIP-8/SOIC-8/SSOP-8")
    (property "ki_keywords" "single Power opamp")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "LM386" (at 3.81 9.95) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(U2-GAIN-Pad1)") (pinfunction "GAIN") (pintype "input+no_connect"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(U2-+)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(C7-Pad2)") (pintype "output"))
    (pad "6" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "5V") (pinfunction "V+") (pintype "power_in"))
    (pad "7" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(U2-BYPASS-Pad7)") (pinfunction "BYPASS") (pintype "input+no_connect"))
    (pad "8" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(U2-GAIN-Pad8)") (pinfunction "GAIN") (pintype "input+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 140.97 86.36 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 1.27 2.54 90) (layer "F.SilkS"))
    (fp_text value "27 ohm" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "G32") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 121.92 109.26 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 2.5 2.54 90) (layer "F.SilkS"))
    (fp_text value "68 nF" (at 2.5 2.85 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "PA2") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:200USP9T1A1M2RE_EWI" (layer "F.Cu")
    (at 137.16 73.66 90)
    (tags "200USP9T1A1M2RE ")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "200USP9T1A1M2RE")
    (attr through_hole)
    (fp_text reference "SW2" (at 5.08 2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "200USP9T1A1M2RE" (at 5.08 2.54 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 5 "unconnected-(SW2-Pad1)") (pinfunction "1") (pintype "unspecified+no_connect"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 6 "unconnected-(SW2-Pad2)") (pinfunction "2") (pintype "unspecified+no_connect"))
    (pad "4" thru_hole circle (at 2.54 2.54 90) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pad1)") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 0 5.08 90) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 7 "unconnected-(SW2-Pad5)") (pinfunction "5") (pintype "unspecified+no_connect"))
    (pad "6" thru_hole circle (at 2.54 5.08 90) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 30 "5V") (pinfunction "6") (pintype "unspecified"))
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 121.92 90.21 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 2.54 90) (layer "F.SilkS"))
    (fp_text value "68 nF" (at 2.5 2.85 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "PA1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 137.16 100.37 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C10" (at -2.54 -0.04 -180) (layer "F.SilkS"))
    (fp_text value "250 uF" (at 2.5 2.85 -270) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "G33") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 137.16 88.98 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at 7.54 -0.04 -180) (layer "F.SilkS"))
    (fp_text value "50 nF" (at 2.5 2.85 -270) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 128.31 97.79)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 2.5 -2.85) (layer "F.SilkS"))
    (fp_text value "10 uF" (at 2.5 2.85) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 137.16 81.32 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C8" (at -2.54 0 -180) (layer "F.SilkS"))
    (fp_text value "250 uF" (at 2.5 2.85 -270) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "G32") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 140.97 80.01 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 1.27 2.54 90) (layer "F.SilkS"))
    (fp_text value "27 ohm" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "G32") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ESP32_NODEMCU:MODULE_ESP32_NODEMCU" (layer "F.Cu")
    (at 159.05 100.33)
    (property "Availability" "Not in stock")
    (property "Check_prices" "https://www.snapeda.com/parts/ESP32%20NODEMCU/AZ-Delivery/view-part/?ref=eda")
    (property "Description" "\nNodeMCU is an open source loT platform. ESP32 is a series of low cost, low power\nsystem-on-chip (SoC) microcontrollers with integrated Wi-Fi & dual-mode Bluetooth.\n")
    (property "MANUFACTURER" "Espressif Systems")
    (property "MAXIMUM_PACKAGE_HEIGHT" "6.6 mm")
    (property "MF" "AZ Delivery")
    (property "MP" "ESP32 NODEMCU")
    (property "Package" "Package")
    (property "Price" "None")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/ESP32%20NODEMCU/AZ-Delivery/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "U1" (at 0.97 0) (layer "F.SilkS"))
    (fp_text value "ESP32_NODEMCU" (at -1.55 29.385) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -12.5 -26) (size 2.25 2.25) (drill 2.25) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at -12.5 26) (size 2.25 2.25) (drill 2.25) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 12.5 -26) (size 2.25 2.25) (drill 2.25) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 12.5 26) (size 2.25 2.25) (drill 2.25) (layers "*.Cu" "*.Mask"))
    (pad "J4_1" thru_hole rect (at 13 -22.86) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(U1-GND_J4_1-PadJ4_1)") (pinfunction "GND_J4_1") (pintype "power_in+no_connect") (solder_mask_margin 0.102))
    (pad "J4_2" thru_hole circle (at 13 -20.32) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(U1-G23-PadJ4_2)") (pinfunction "G23") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_3" thru_hole circle (at 13 -17.78) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(U1-G22-PadJ4_3)") (pinfunction "G22") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_4" thru_hole circle (at 13 -15.24) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(U1-TXD-PadJ4_4)") (pinfunction "TXD") (pintype "output+no_connect") (solder_mask_margin 0.102))
    (pad "J4_5" thru_hole circle (at 13 -12.7) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(U1-RXD-PadJ4_5)") (pinfunction "RXD") (pintype "input+no_connect") (solder_mask_margin 0.102))
    (pad "J4_6" thru_hole circle (at 13 -10.16) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(U1-G21-PadJ4_6)") (pinfunction "G21") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_7" thru_hole circle (at 13 -7.62) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(U1-GND_J4_7-PadJ4_7)") (pinfunction "GND_J4_7") (pintype "power_in+no_connect") (solder_mask_margin 0.102))
    (pad "J4_8" thru_hole circle (at 13 -5.08) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "G19") (pinfunction "G19") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_9" thru_hole circle (at 13 -2.54) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "G18") (pinfunction "G18") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_10" thru_hole circle (at 13 0) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(U1-G5-PadJ4_10)") (pinfunction "G5") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_11" thru_hole circle (at 13 2.54) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(U1-G17-PadJ4_11)") (pinfunction "G17") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_12" thru_hole circle (at 13 5.08) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 39 "unconnected-(U1-G16-PadJ4_12)") (pinfunction "G16") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_13" thru_hole circle (at 13 7.62) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 40 "unconnected-(U1-G4-PadJ4_13)") (pinfunction "G4") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_14" thru_hole circle (at 13 10.16) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(U1-G0-PadJ4_14)") (pinfunction "G0") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_15" thru_hole circle (at 13 12.7) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(U1-G2-PadJ4_15)") (pinfunction "G2") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_16" thru_hole circle (at 13 15.24) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(U1-G15-PadJ4_16)") (pinfunction "G15") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_17" thru_hole circle (at 13 17.78) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(U1-SD1-PadJ4_17)") (pinfunction "SD1") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_18" thru_hole circle (at 13 20.32) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(U1-SD0-PadJ4_18)") (pinfunction "SD0") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J4_19" thru_hole circle (at 13 22.86) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(U1-CLK-PadJ4_19)") (pinfunction "CLK") (pintype "input+no_connect") (solder_mask_margin 0.102))
    (pad "J5_1" thru_hole rect (at -13 22.86) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(U1-5V-PadJ5_1)") (pinfunction "5V") (pintype "power_in+no_connect") (solder_mask_margin 0.102))
    (pad "J5_2" thru_hole circle (at -13 20.32) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(U1-CMD-PadJ5_2)") (pinfunction "CMD") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_3" thru_hole circle (at -13 17.78) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(U1-SD3-PadJ5_3)") (pinfunction "SD3") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_4" thru_hole circle (at -13 15.24) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(U1-SD2-PadJ5_4)") (pinfunction "SD2") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_5" thru_hole circle (at -13 12.7) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(U1-G13-PadJ5_5)") (pinfunction "G13") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_6" thru_hole circle (at -13 10.16) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 31 "GND") (pinfunction "GND_J5_6") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "J5_7" thru_hole circle (at -13 7.62) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(U1-G12-PadJ5_7)") (pinfunction "G12") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_8" thru_hole circle (at -13 5.08) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(U1-G14-PadJ5_8)") (pinfunction "G14") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_9" thru_hole circle (at -13 2.54) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(U1-G27-PadJ5_9)") (pinfunction "G27") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_10" thru_hole circle (at -13 0) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(U1-G26-PadJ5_10)") (pinfunction "G26") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_11" thru_hole circle (at -13 -2.54) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(U1-G25-PadJ5_11)") (pinfunction "G25") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_12" thru_hole circle (at -13 -5.08) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "G33") (pinfunction "G33") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J5_13" thru_hole circle (at -13 -7.62) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "G32") (pinfunction "G32") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J5_14" thru_hole circle (at -13 -10.16) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(U1-G35-PadJ5_14)") (pinfunction "G35") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_15" thru_hole circle (at -13 -12.7) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(U1-G34-PadJ5_15)") (pinfunction "G34") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "J5_16" thru_hole circle (at -13 -15.24) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(U1-SN-PadJ5_16)") (pinfunction "SN") (pintype "input+no_connect") (solder_mask_margin 0.102))
    (pad "J5_17" thru_hole circle (at -13 -17.78) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(U1-SP-PadJ5_17)") (pinfunction "SP") (pintype "input+no_connect") (solder_mask_margin 0.102))
    (pad "J5_18" thru_hole circle (at -13 -20.32) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(U1-EN-PadJ5_18)") (pinfunction "EN") (pintype "input+no_connect") (solder_mask_margin 0.102))
    (pad "J5_19" thru_hole circle (at -13 -22.86) (size 1.35 1.35) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "3V") (pinfunction "3V3") (pintype "power_in") (solder_mask_margin 0.102))
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 121.92 101.6 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SDP25.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 2.5 2.54 -270) (layer "F.SilkS"))
    (fp_text value "100 nF" (at 2.5 2.85 -270) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(U3-+)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "PA2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 114.3 64.77) (end 179.07 129.54)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "SDP25\nTeam 14\nSteven Huang\nKishen Patil\nKyle Auyeung\nTyler Russel" (at 162.56 95.25) (layer "B.SilkS"))
  (zone (net 31) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 115.57 66.04)
        (xy 115.57 128.27)
        (xy 177.8 128.27)
        (xy 177.8 66.04)
      )
    )
  )
)
