(kicad_pcb (version 20171130) (host pcbnew "(5.1.0-rc1-17-gb4eda32f8)")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 29)
    (zones 0)
    (modules 2)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 51 50)
    (grid_origin 59 50)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.050000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 SDA)
  (net 3 SCL)
  (net 4 ADC0)
  (net 5 ADC1)
  (net 6 +3V3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net ADC0)
    (add_net ADC1)
    (add_net GND)
    (add_net SCL)
    (add_net SDA)
  )
  (module badgelife_sao_v169bis:Badgelife-SAOv169-BADGE-2x3 (layer F.Cu) (tedit 5CB6F2DE)
    (at 59 57.62)
    (descr "Through hole straight IDC box header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x03 2.54mm double row")
    (fp_text reference X1 (at 0 -5.842) (layer F.SilkS) hide)
    (fp_text value Badgelife_sao_connector_v169bis (at 0 -8.509) (layer F.Fab))
    (fp_text user %R (at 0.06 0.02 270) (layer F.Fab))
    (fp_text user VCC (at -2.54 -2.794) (layer B.SilkS))
    (fp_text user GND (at -2.54 3.048) (layer B.SilkS))
    (fp_text user SDA (at 0 -2.794) (layer B.SilkS))
    (fp_text user SCL (at 0 3.048) (layer B.SilkS))
    (fp_text user ADC1 (at 2.6 3.03) (layer B.SilkS))
    (fp_text user ADC0 (at 2.6 -2.794) (layer B.SilkS))
    (pad 5 thru_hole circle (at 2.6 -1.25 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 ADC0))
    (pad 6 thru_hole circle (at 2.6 1.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 ADC1))
    (pad 3 thru_hole oval (at 0.06 -1.25 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 SDA))
    (pad 4 thru_hole oval (at 0.06 1.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 SCL))
    (pad 1 thru_hole oval (at -2.48 -1.25 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (pad 2 thru_hole circle (at -2.48 1.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_2x07_Pitch2.54mm (layer F.Cu) (tedit 5CB6F199)
    (at 57.73 71.59)
    (descr "Through hole straight pin header, 2x07, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value KiCon_Badge_Expansion (at 1.27 17.57) (layer F.Fab))
    (fp_text user %R (at 1.27 7.62 90) (layer F.Fab))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 2.3 1.9) (drill 1.3 (offset 0.2 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 15.24) (size 2.3 1.9) (drill 1.3 (offset -0.2 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 2.3 1.9) (drill 1.3 (offset 0.2 0)) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7) (size 2.3 1.9) (drill 1.3 (offset -0.2 0)) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 2.3 1.9) (drill 1.3 (offset 0.2 0)) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16) (size 2.3 1.9) (drill 1.3 (offset -0.2 0)) (layers *.Cu *.Mask)
      (net 2 SDA))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 2.3 1.9) (drill 1.3 (offset 0.2 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62) (size 2.3 1.9) (drill 1.3 (offset -0.2 0)) (layers *.Cu *.Mask)
      (net 3 SCL))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 2.3 1.9) (drill 1.3 (offset 0.2 0)) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08) (size 2.3 1.9) (drill 1.3 (offset -0.2 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 2.3 1.9) (drill 1.3 (offset 0.2 0)) (layers *.Cu *.Mask)
      (net 4 ADC0))
    (pad 3 thru_hole oval (at 0 2.54) (size 2.3 1.9) (drill 1.3 (offset -0.2 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.3 1.9) (drill 1.3 (offset 0.2 0)) (layers *.Cu *.Mask)
      (net 5 ADC1))
    (pad 1 thru_hole rect (at 0 0) (size 2.3 1.9) (drill 1.3 (offset -0.2 0)) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "#badgelife" (at 59 52.75) (layer F.SilkS))
  (gr_text v1.69bis (at 60.3 65.95 90) (layer B.SilkS))
  (gr_text "#badgelife" (at 57.65 65.8 90) (layer B.SilkS))
  (gr_line (start 63.760176 63.57022) (end 63.330763 63.982764) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 64.587999 65.24) (end 62.810001 65.24) (angle 45) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 54.239824 63.57022) (end 54.669236 63.982764) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 53.412 65.24) (end 55.19 65.24) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 55.19 86.83) (end 55.19 65.24) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 62.81 86.83) (end 62.81 65.24) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 59 86.83) (end 55.19 86.83) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 59 57.62) (end 66.62 57.62) (angle 51.34019175) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 59 57.62) (end 51.38 57.62) (angle -51.34019175) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 59 57.62) (end 66.62 57.62) (angle -180) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 50) (xy 67 50) (xy 67 91) (xy 51 91)
      )
    )
  )
)
