(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 46)
    (no_connects 0)
    (area 60.394999 84.446901 145.34687 127.050001)
    (thickness 1.6)
    (drawings 33)
    (tracks 311)
    (zones 0)
    (modules 5)
    (nets 61)
  )
  (page A4)
  (title_block
    (title "Acorn Electron cartridge breakout")
    (date 2017-02-16)
    (comment 2 "See: http://hgweb.boddie.org.uk/AcornElectronCartridge")
    (comment 3 "Design licensed under the terms of the GNU General Public License version 3 or later.")
    (comment 4 "A prototyping/breakout cartridge for the Acorn Electron Plus 1 expansion unit.")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.15)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 102.87 127)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 /nRST)
  (net 2 /nOE)
  (net 3 /CSRW)
  (net 4 /A8)
  (net 5 /A13)
  (net 6 /A12)
  (net 7 /PHI2)
  (net 8 /-5V)
  (net 9 /READY)
  (net 10 /nNMI)
  (net 11 /nIRQ)
  (net 12 /nINFC)
  (net 13 /nINFD)
  (net 14 /ROMQA)
  (net 15 /CLOCK)
  (net 16 /nROMSTB)
  (net 17 /ADOUT)
  (net 18 /AGND)
  (net 19 /ADIN)
  (net 20 /D3)
  (net 21 /A10)
  (net 22 /A11)
  (net 23 /A9)
  (net 24 /D7)
  (net 25 /D6)
  (net 26 /D5)
  (net 27 /D4)
  (net 28 /nOE2)
  (net 29 /BA7)
  (net 30 /BA6)
  (net 31 /BA5)
  (net 32 /BA4)
  (net 33 /BA3)
  (net 34 /BA2)
  (net 35 /BA1)
  (net 36 /BA0)
  (net 37 /D0)
  (net 38 /D2)
  (net 39 /D1)
  (net 40 /NC)
  (net 41 VCC)
  (net 42 GND)
  (net 43 /OE#)
  (net 44 /OE)
  (net 45 /A14)
  (net 46 /CE#)
  (net 47 "Net-(Flash1-Pad1)")
  (net 48 "Net-(Flash1-Pad30)")
  (net 49 /A15)
  (net 50 "Net-(FLIP1-Pad10)")
  (net 51 "Net-(FLIP1-Pad11)")
  (net 52 "Net-(FLIP1-Pad12)")
  (net 53 /A16)
  (net 54 "Net-(FLIP1-Pad13)")
  (net 55 "Net-(FLIP1-Pad6)")
  (net 56 "Net-(FLIP1-Pad14)")
  (net 57 "Net-(FLIP1-Pad7)")
  (net 58 "Net-(FLIP1-Pad15)")
  (net 59 /+5V_B)
  (net 60 /0V_A)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+5V_B)
    (add_net /-5V)
    (add_net /0V_A)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A8)
    (add_net /A9)
    (add_net /ADIN)
    (add_net /ADOUT)
    (add_net /AGND)
    (add_net /BA0)
    (add_net /BA1)
    (add_net /BA2)
    (add_net /BA3)
    (add_net /BA4)
    (add_net /BA5)
    (add_net /BA6)
    (add_net /BA7)
    (add_net /CE#)
    (add_net /CLOCK)
    (add_net /CSRW)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /NC)
    (add_net /OE)
    (add_net /OE#)
    (add_net /PHI2)
    (add_net /READY)
    (add_net /ROMQA)
    (add_net /nINFC)
    (add_net /nINFD)
    (add_net /nIRQ)
    (add_net /nNMI)
    (add_net /nOE)
    (add_net /nOE2)
    (add_net /nROMSTB)
    (add_net /nRST)
    (add_net GND)
    (add_net "Net-(FLIP1-Pad10)")
    (add_net "Net-(FLIP1-Pad11)")
    (add_net "Net-(FLIP1-Pad12)")
    (add_net "Net-(FLIP1-Pad13)")
    (add_net "Net-(FLIP1-Pad14)")
    (add_net "Net-(FLIP1-Pad15)")
    (add_net "Net-(FLIP1-Pad6)")
    (add_net "Net-(FLIP1-Pad7)")
    (add_net "Net-(Flash1-Pad1)")
    (add_net "Net-(Flash1-Pad30)")
    (add_net VCC)
  )
  (net_class OSHPark ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (module Housings_DIP:DIP-32_W15.24mm_Socket (layer F.Cu) (tedit 59C78D6C)
    (at 87.63 106.68 90)
    (descr "32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
    (fp_text reference Flash1 (at 7.62 -2.33 90) (layer F.SilkS))
    (fp_text value SST39SF010 (at 7.62 40.43 90) (layer F.Fab))
    (fp_text user %R (at 7.62 19.05 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(Flash1-Pad1)"))
    (pad 17 thru_hole oval (at 15.24 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /D3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /A16))
    (pad 18 thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /D4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /A15))
    (pad 19 thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /D5))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /A12))
    (pad 20 thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /D6))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /BA7))
    (pad 21 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /D7))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /BA6))
    (pad 22 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /CE#))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /BA5))
    (pad 23 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /A10))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /BA4))
    (pad 24 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /OE#))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /BA3))
    (pad 25 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /A11))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /BA2))
    (pad 26 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /A9))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /BA1))
    (pad 27 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /A8))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /BA0))
    (pad 28 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /A13))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /D0))
    (pad 29 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /A14))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /D1))
    (pad 30 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(Flash1-Pad30)"))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /D2))
    (pad 31 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /CSRW))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 32 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-32_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm_Socket (layer F.Cu) (tedit 59D805FF)
    (at 133.985 91.44)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference FLIP1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74LS174 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /nRST))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /nROMSTB))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /A15))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(FLIP1-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /D0))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(FLIP1-Pad11)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /D1))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(FLIP1-Pad12)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /A16))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(FLIP1-Pad13)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(FLIP1-Pad6)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(FLIP1-Pad14)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(FLIP1-Pad7)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(FLIP1-Pad15)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Acorn_Electron:Acorn_Electron_cartridge_edge_connector_rear (layer F.Cu) (tedit 59D7B679)
    (at 102.87 113.03)
    (tags "Acorn Electron cartridge edge connector rear")
    (fp_text reference CONN1 (at 0 -43.18) (layer F.SilkS) hide)
    (fp_text value Acorn_Electron_cartridge_edge_connector_rear_side_A (at 0 -49.53) (layer F.Fab) hide)
    (pad 1 connect rect (at -26.67 6.62) (size 1.27 10.7) (layers F.Cu F.Mask)
      (net 41 VCC))
    (pad 2 connect rect (at -24.13 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 2 /nOE))
    (pad 3 connect rect (at -21.59 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 1 /nRST))
    (pad 4 connect rect (at -19.05 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 3 /CSRW))
    (pad 5 connect rect (at -16.51 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 4 /A8))
    (pad 6 connect rect (at -13.97 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 5 /A13))
    (pad 7 connect rect (at -11.43 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 6 /A12))
    (pad 8 connect rect (at -8.89 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 7 /PHI2))
    (pad 9 connect rect (at -6.35 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 8 /-5V))
    (pad 10 connect rect (at -3.81 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 40 /NC))
    (pad 11 connect rect (at -1.27 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 9 /READY))
    (pad 12 connect rect (at 1.27 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 10 /nNMI))
    (pad 13 connect rect (at 3.81 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 11 /nIRQ))
    (pad 14 connect rect (at 6.35 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 12 /nINFC))
    (pad 15 connect rect (at 8.89 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 13 /nINFD))
    (pad 16 connect rect (at 11.43 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 14 /ROMQA))
    (pad 17 connect rect (at 13.97 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 15 /CLOCK))
    (pad 18 connect rect (at 16.51 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 16 /nROMSTB))
    (pad 19 connect rect (at 19.05 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 17 /ADOUT))
    (pad 20 connect rect (at 21.59 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 18 /AGND))
    (pad 21 connect rect (at 24.13 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 19 /ADIN))
    (pad 22 connect rect (at 26.67 7.62) (size 1.27 12.7) (layers F.Cu F.Mask)
      (net 60 /0V_A))
  )
  (module Acorn_Electron:Acorn_Electron_cartridge_edge_connector_front (layer B.Cu) (tedit 59D7B67C)
    (at 102.87 113.03)
    (tags "Acorn Electron cartridge edge connector front")
    (fp_text reference CONN2 (at 0 -43.18) (layer B.SilkS) hide)
    (fp_text value Acorn_Electron_cartridge_edge_connector_front_side_B (at 0 -49.53) (layer B.Fab) hide)
    (pad 1 connect rect (at -26.67 6.62) (size 1.27 10.7) (layers B.Cu B.Mask)
      (net 59 /+5V_B))
    (pad 2 connect rect (at -24.13 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 21 /A10))
    (pad 3 connect rect (at -21.59 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 20 /D3))
    (pad 4 connect rect (at -19.05 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 22 /A11))
    (pad 5 connect rect (at -16.51 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 23 /A9))
    (pad 6 connect rect (at -13.97 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 24 /D7))
    (pad 7 connect rect (at -11.43 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 25 /D6))
    (pad 8 connect rect (at -8.89 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 26 /D5))
    (pad 9 connect rect (at -6.35 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 27 /D4))
    (pad 10 connect rect (at -3.81 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 28 /nOE2))
    (pad 11 connect rect (at -1.27 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 29 /BA7))
    (pad 12 connect rect (at 1.27 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 30 /BA6))
    (pad 13 connect rect (at 3.81 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 31 /BA5))
    (pad 14 connect rect (at 6.35 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 32 /BA4))
    (pad 15 connect rect (at 8.89 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 33 /BA3))
    (pad 16 connect rect (at 11.43 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 34 /BA2))
    (pad 17 connect rect (at 13.97 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 35 /BA1))
    (pad 18 connect rect (at 16.51 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 36 /BA0))
    (pad 19 connect rect (at 19.05 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 37 /D0))
    (pad 20 connect rect (at 21.59 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 38 /D2))
    (pad 21 connect rect (at 24.13 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 39 /D1))
    (pad 22 connect rect (at 26.67 7.62) (size 1.27 12.7) (layers B.Cu B.Mask)
      (net 42 GND))
  )
  (module Housings_DIP:DIP-14_W7.62mm_Socket (layer F.Cu) (tedit 59C78D6B)
    (at 71.12 108.585 180)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference NAND1 (at 3.81 -2.33 180) (layer F.SilkS))
    (fp_text value 74HC00 (at 3.81 17.57 180) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /nOE))
    (pad 8 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /OE#))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /nOE))
    (pad 9 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /CSRW))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /OE))
    (pad 10 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /CSRW))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /OE))
    (pad 11 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /A14))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /PHI2))
    (pad 12 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /ROMQA))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /CE#))
    (pad 13 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /ROMQA))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 GND))
    (pad 14 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "This side to front" (at 137.795 86.36) (layer B.SilkS))
  (gr_line (start 145.296869 84.496902) (end 145.296869 84.496902) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.445 84.496902) (end 145.296869 84.496902) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.445 115.146554) (end 60.445 84.496902) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.524236 115.146554) (end 60.445 115.146554) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.745636 115.169132) (end 73.524236 115.146554) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.951386 115.233506) (end 73.745636 115.169132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.137213 115.335332) (end 73.951386 115.233506) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.29884 115.470093) (end 74.137213 115.335332) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.431993 115.633331) (end 74.29884 115.470093) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.532395 115.820585) (end 74.431993 115.633331) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.595772 116.027341) (end 74.532395 115.820585) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.617847 116.249111) (end 74.595772 116.027341) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.617847 127) (end 74.617847 116.249111) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.124027 127) (end 74.617847 127) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.124027 116.249111) (end 131.124027 127) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.146097 116.027341) (end 131.124027 116.249111) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.209473 115.820585) (end 131.146097 116.027341) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.309876 115.633331) (end 131.209473 115.820585) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.443029 115.470093) (end 131.309876 115.633331) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.604655 115.335332) (end 131.443029 115.470093) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.790481 115.233506) (end 131.604655 115.335332) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.996232 115.169132) (end 131.790481 115.233506) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.217633 115.146554) (end 131.996232 115.169132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.296869 115.146554) (end 132.217633 115.146554) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.296869 84.496902) (end 145.296869 115.146554) (layer Edge.Cuts) (width 0.1))
  (gr_text "(C) 2017 David Boddie   Licensed under GPLv3 or later\nElectron Flash ROM Cart Revision S4" (at 127 86.995) (layer F.SilkS))
  (gr_text B22 (at 129.54 113.665 270) (layer B.SilkS))
  (gr_text B1 (at 76.2 113.665 270) (layer B.SilkS))
  (gr_text A22 (at 129.54 113.665 90) (layer F.SilkS))
  (gr_text A1 (at 76.2 113.665 90) (layer F.SilkS))
  (gr_text "This side to rear" (at 136.525 86.36) (layer F.SilkS))
  (gr_text "F.Cu (front copper) layer is rear side of cartridge board.\nB.Cu (back copper) layer is front side of cartridge board.\n74HC00 is attached to the front side of the board.\nFlash ROM is attached to the rear side." (at 102.87 57.15) (layer Cmts.User))
)
