(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 99)
    (zones 0)
    (modules 16)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /FIRE)
  (net 3 /DOWN)
  (net 4 /LEFT)
  (net 5 /RIGHT)
  (net 6 /UP)
  (net 7 /POTY)
  (net 8 /5V)
  (net 9 /POTX)
  (net 10 "Net-(R1-Pad2)")
  (net 11 "Net-(R2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /5V)
    (add_net /DOWN)
    (add_net /FIRE)
    (add_net /GND)
    (add_net /LEFT)
    (add_net /POTX)
    (add_net /POTY)
    (add_net /RIGHT)
    (add_net /UP)
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
  )
  (module digikey-footprints:DSUB-9_Jack_5747840-3 locked (layer F.Cu) (tedit 5AD0FBDD)
    (at 158.5 92.25)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=5747840&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference J1 (at 0 6.25) (layer F.SilkS))
    (fp_text value 5747840-3 (at 0 4.75) (layer F.Fab))
    (fp_text user %R (at 0 -7.5) (layer F.Fab))
    (pad 5 thru_hole circle (at -5.48 1.42) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 7 /POTY))
    (pad 9 thru_hole circle (at -4.11 -1.42) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 9 /POTX))
    (pad 4 thru_hole circle (at -2.74 1.42) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 5 /RIGHT))
    (pad 8 thru_hole circle (at -1.37 -1.42) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 3 thru_hole circle (at 0 1.42) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 4 /LEFT))
    (pad 7 thru_hole circle (at 1.37 -1.42) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 8 /5V))
    (pad 2 thru_hole circle (at 2.74 1.42) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 /DOWN))
    (pad 6 thru_hole circle (at 4.11 -1.42) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 2 /FIRE))
    (pad 1 thru_hole circle (at 5.48 1.42) (size 2 2) (drill 1.04) (layers *.Cu *.Mask)
      (net 6 /UP))
    (pad 10 thru_hole circle (at 12.495 0) (size 3.5 3.5) (drill 3.17) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 10 thru_hole circle (at -12.495 0) (size 3.5 3.5) (drill 3.17) (layers *.Cu *.Mask)
      (net 1 /GND))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 213.75 99.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 330 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 204 91 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 330 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /5V))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Tactile_THT_B3F-1xxx (layer F.Cu) (tedit 5AF34B0A)
    (at 203.2488 96.7394)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S8 (at 3.2512 -2.2094) (layer F.SilkS))
    (fp_text value FIRE3 (at 3.2512 7.1006) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(R2-Pad2)"))
    (pad 3 thru_hole circle (at 0.0012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(R2-Pad2)"))
    (pad 2 thru_hole circle (at 6.5012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /POTY))
    (pad 1 thru_hole rect (at 0.0012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /POTY))
  )
  (module digikey-footprints:Switch_Tactile_THT_B3F-1xxx (layer F.Cu) (tedit 5AF34B0A)
    (at 193.2488 88.2394)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S6 (at 3.2512 -2.2094) (layer F.SilkS))
    (fp_text value FIRE2 (at 3.2512 7.1006) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606) (layer F.Fab))
    (pad 1 thru_hole rect (at 0.0012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 /POTX))
    (pad 2 thru_hole circle (at 6.5012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 /POTX))
    (pad 3 thru_hole circle (at 0.0012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 4 thru_hole circle (at 6.5012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
  )
  (module digikey-footprints:Switch_Tactile_THT_B3F-1xxx (layer F.Cu) (tedit 5AF34B0A)
    (at 193.2488 105.2394)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S7 (at 3.2512 -2.2094) (layer F.SilkS))
    (fp_text value JUMP (at 3.2512 7.1006) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606) (layer F.Fab))
    (pad 1 thru_hole rect (at 0.0012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 6.5012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 3 thru_hole circle (at 0.0012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /UP))
    (pad 4 thru_hole circle (at 6.5012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /UP))
    (model "${KIPRJMOD}/Omron B3F-1000.step"
      (offset (xyz 3.25 -2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Tactile_THT_B3F-1xxx (layer F.Cu) (tedit 5AF34B0A)
    (at 117.2488 88.2394)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S5 (at 3.2512 -2.2094) (layer F.SilkS))
    (fp_text value UP (at 3.2512 7.1006) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /UP))
    (pad 3 thru_hole circle (at 0.0012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /UP))
    (pad 2 thru_hole circle (at 6.5012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole rect (at 0.0012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model "${KIPRJMOD}/Omron B3F-1000.step"
      (offset (xyz 3.25 -2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Tactile_THT_B3F-1xxx (layer F.Cu) (tedit 5AF34B0A)
    (at 127.2488 96.7394)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S4 (at 3.2512 -2.2094) (layer F.SilkS))
    (fp_text value RIGHT (at 3.2512 7.1006) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RIGHT))
    (pad 3 thru_hole circle (at 0.0012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RIGHT))
    (pad 2 thru_hole circle (at 6.5012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole rect (at 0.0012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model "${KIPRJMOD}/Omron B3F-1000.step"
      (offset (xyz 3.25 -2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Tactile_THT_B3F-1xxx (layer F.Cu) (tedit 5AF34B0A)
    (at 107.25 96.75)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S3 (at 3.2512 -2.2094) (layer F.SilkS))
    (fp_text value LEFT (at 3.2512 7.1006) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606) (layer F.Fab))
    (pad 1 thru_hole rect (at 0.0012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 6.5012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 3 thru_hole circle (at 0.0012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /LEFT))
    (pad 4 thru_hole circle (at 6.5012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /LEFT))
    (model "${KIPRJMOD}/Omron B3F-1000.step"
      (offset (xyz 3.25 -2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Tactile_THT_B3F-1xxx (layer F.Cu) (tedit 5AF34B0A)
    (at 117.25 105.25)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S2 (at 3.2512 -2.2094) (layer F.SilkS))
    (fp_text value DOWN (at 3.2512 7.1006) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606) (layer F.Fab))
    (pad 4 thru_hole circle (at 6.5012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 /DOWN))
    (pad 3 thru_hole circle (at 0.0012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 /DOWN))
    (pad 2 thru_hole circle (at 6.5012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 1 thru_hole rect (at 0.0012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model "${KIPRJMOD}/Omron B3F-1000.step"
      (offset (xyz 3.25 -2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Tactile_THT_B3F-1xxx (layer F.Cu) (tedit 5AF34B0A)
    (at 183.2488 96.7394)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference S1 (at 3.2512 -2.2094) (layer F.SilkS))
    (fp_text value FIRE (at 3.2512 7.1006) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606) (layer F.Fab))
    (pad 1 thru_hole rect (at 0.0012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 6.5012 0.0106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 3 thru_hole circle (at 0.0012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 /FIRE))
    (pad 4 thru_hole circle (at 6.5012 4.5106) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 /FIRE))
    (model "${KIPRJMOD}/Omron B3F-1000.step"
      (offset (xyz 3.25 -2.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 5CB95F73)
    (at 106 86.5)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference 3mm_UL (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 5CB95F8D)
    (at 106 111.5)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference 3mm_LL (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 5CB95F9D)
    (at 211 86.5)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference 3mm_UR (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3mm (layer F.Cu) (tedit 5CB95FC1)
    (at 211 111.5)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (attr virtual)
    (fp_text reference 3mm_LR (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_6mm (layer F.Cu) (tedit 5CB95FD2)
    (at 158.5 111.5)
    (descr "Mounting Hole 6mm, no annular")
    (tags "mounting hole 6mm no annular")
    (attr virtual)
    (fp_text reference 6mm_C (at 0 -7) (layer F.SilkS) hide)
    (fp_text value MountingHole_6mm (at 0 7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6 6) (drill 6) (layers *.Cu *.Mask))
  )
  (gr_text "Open Source Hardware" (at 158.5 100) (layer B.SilkS))
  (gr_text http://github.com/jtgans/RetroPad (at 158.5 102.75) (layer B.SilkS))
  (dimension 10 (width 0.3) (layer Dwgs.User)
    (gr_text "10.000 mm" (at 101 125.6) (layer Dwgs.User))
    (feature1 (pts (xy 96 111.5) (xy 96 124.086421)))
    (feature2 (pts (xy 106 111.5) (xy 106 124.086421)))
    (crossbar (pts (xy 106 123.5) (xy 96 123.5)))
    (arrow1a (pts (xy 96 123.5) (xy 97.126504 122.913579)))
    (arrow1b (pts (xy 96 123.5) (xy 97.126504 124.086421)))
    (arrow2a (pts (xy 106 123.5) (xy 104.873496 122.913579)))
    (arrow2b (pts (xy 106 123.5) (xy 104.873496 124.086421)))
  )
  (dimension 52.5 (width 0.3) (layer Dwgs.User)
    (gr_text "52.500 mm" (at 184.75 64.4) (layer Dwgs.User))
    (feature1 (pts (xy 158.5 79.5) (xy 158.5 65.913579)))
    (feature2 (pts (xy 211 79.5) (xy 211 65.913579)))
    (crossbar (pts (xy 211 66.5) (xy 158.5 66.5)))
    (arrow1a (pts (xy 158.5 66.5) (xy 159.626504 65.913579)))
    (arrow1b (pts (xy 158.5 66.5) (xy 159.626504 67.086421)))
    (arrow2a (pts (xy 211 66.5) (xy 209.873496 65.913579)))
    (arrow2b (pts (xy 211 66.5) (xy 209.873496 67.086421)))
  )
  (dimension 12.5 (width 0.3) (layer Dwgs.User)
    (gr_text "12.500 mm" (at 92.4 105.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 99 99) (xy 93.913579 99)))
    (feature2 (pts (xy 99 111.5) (xy 93.913579 111.5)))
    (crossbar (pts (xy 94.5 111.5) (xy 94.5 99)))
    (arrow1a (pts (xy 94.5 99) (xy 95.086421 100.126504)))
    (arrow1b (pts (xy 94.5 99) (xy 93.913579 100.126504)))
    (arrow2a (pts (xy 94.5 111.5) (xy 95.086421 110.373496)))
    (arrow2b (pts (xy 94.5 111.5) (xy 93.913579 110.373496)))
  )
  (dimension 105 (width 0.3) (layer Dwgs.User)
    (gr_text "105.000 mm" (at 158.5 68.9) (layer Dwgs.User))
    (feature1 (pts (xy 211 79.5) (xy 211 70.413579)))
    (feature2 (pts (xy 106 79.5) (xy 106 70.413579)))
    (crossbar (pts (xy 106 71) (xy 211 71)))
    (arrow1a (pts (xy 211 71) (xy 209.873496 71.586421)))
    (arrow1b (pts (xy 211 71) (xy 209.873496 70.413579)))
    (arrow2a (pts (xy 106 71) (xy 107.126504 71.586421)))
    (arrow2b (pts (xy 106 71) (xy 107.126504 70.413579)))
  )
  (dimension 25 (width 0.3) (layer Dwgs.User)
    (gr_text "25.000 mm" (at 87.65 99 270) (layer Dwgs.User))
    (feature1 (pts (xy 99 111.5) (xy 89.163579 111.5)))
    (feature2 (pts (xy 99 86.5) (xy 89.163579 86.5)))
    (crossbar (pts (xy 89.75 86.5) (xy 89.75 111.5)))
    (arrow1a (pts (xy 89.75 111.5) (xy 89.163579 110.373496)))
    (arrow1b (pts (xy 89.75 111.5) (xy 90.336421 110.373496)))
    (arrow2a (pts (xy 89.75 86.5) (xy 89.163579 87.626504)))
    (arrow2b (pts (xy 89.75 86.5) (xy 90.336421 87.626504)))
  )
  (gr_text "RetroPad v2.0 by June Tate-Gans" (at 158.5 102.25) (layer F.SilkS))
  (gr_line (start 96 84) (end 103.5 76.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.5 121.5) (end 96 114) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 221 114) (end 213.5 121.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.5 76.5) (end 221 84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96 114) (end 96 84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.5 121.5) (end 103.5 121.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 221 84) (end 221 114) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.5 76.5) (end 213.5 76.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99 86.5) (xy 106 79.5) (xy 211 79.5) (xy 218 86.5) (xy 218 111.5)
        (xy 211.25 118.5) (xy 106 118.5) (xy 99 111.75)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99 111.5) (xy 99 86.5) (xy 106 79.5) (xy 211 79.5) (xy 218 86.5)
        (xy 218 111.5) (xy 211.25 118.5) (xy 106 118.5)
      )
    )
  )
)
