(kicad_pcb (version 20171130) (host pcbnew 5.0.1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 91)
    (zones 0)
    (modules 23)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.25)
    (user_trace_width 1.5)
    (user_trace_width 1.75)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2.6)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "elcrow/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 /TRIG)
  (net 4 VCC)
  (net 5 /PWM_OUT)
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(D2-Pad1)")
  (net 8 +12V)
  (net 9 /FAN_RPM)
  (net 10 "Net-(J1-Pad4)")
  (net 11 "Net-(R1-Pad2)")
  (net 12 "Net-(J2-Pad4)")
  (net 13 /12V_OUT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /12V_OUT)
    (add_net /FAN_RPM)
    (add_net /PWM_OUT)
    (add_net /TRIG)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(R1-Pad2)")
    (add_net VCC)
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 148.336 131.064 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J3 (at -0.254 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /12V_OUT))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 +12V))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C2071C0)
    (at 143.002 93.472)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C2071C4)
    (at 170.942 93.472)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C2071C9)
    (at 170.942 130.81)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 145.542 99.822 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C5 (at 0.762 3.556 180) (layer F.SilkS))
    (fp_text value .33uF (at 1 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +12V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /usr/share/kicad/modules/Capacitor_THT.pretty/CP_Radial_D5.0mm_P2.00mm.kicad_mod
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 141.986 109.474)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 2.286 0) (layer F.SilkS))
    (fp_text value .1uF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 143.51 105.664)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U1 (at -2.286 0) (layer F.SilkS))
    (fp_text value MC78L05_TO92 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 +12V))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59D29AB8)
    (at 150.368 119.634 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.556 3.556 90) (layer F.SilkS))
    (fp_text value NE555 (at 3.81 8.128 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /TRIG))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /TRIG))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W4.4mm_P5.00mm (layer F.Cu) (tedit 59D29AB1)
    (at 154.94 108.204 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*4.4mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 4.4mm Capacitor")
    (fp_text reference C1 (at 2.286 0 180) (layer F.SilkS))
    (fp_text value .01uF (at 2.794 -1.524 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W4.4mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /usr/share/kicad/modules/Capacitor_THT.pretty/C_Disc_D7.5mm_W4.4mm_P5.00mm.kicad_mod
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 59D29AA4)
    (at 147.066 117.348 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C2 (at -0.254 -2.286 90) (layer F.SilkS))
    (fp_text value 470pF (at 2.286 0 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /TRIG))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 59D29AA9)
    (at 142.24 114.3)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C3 (at 0 3.048) (layer F.SilkS))
    (fp_text value 10uF (at 0.762 2.794) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 59D29AD3)
    (at 145.796 124.714 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.5 -2.56 90) (layer F.SilkS))
    (fp_text value .1uF (at 2.426 0.05 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 59E8BCF8)
    (at 170.942 119.38 180)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 5.334 1.778 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.08 0 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /PWM_OUT))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 59E8BCEE)
    (at 163.068 132.08 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 5.08 -1.778 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.08 0 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /PWM_OUT))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-04_04x2.54mm_Straight (layer F.Cu) (tedit 5A541355)
    (at 157.988 101.854 180)
    (descr "Connector Headers with Friction Lock, 22-27-2041, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2041")
    (fp_text reference J1 (at -0.762 -4.064 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 4.064 2.286 180) (layer F.Fab))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 +12V))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /FAN_RPM))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-04_04x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-04_04x2.54mm_Straight (layer F.Cu) (tedit 59E82E2C)
    (at 149.6 124.4)
    (descr "Connector Headers with Friction Lock, 22-27-2041, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2041")
    (fp_text reference J2 (at -2.026 3.87) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 3.562 2.346) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 /12V_OUT))
    (pad 3 thru_hole oval (at 5.08 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /FAN_RPM))
    (pad 4 thru_hole oval (at 7.62 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-04_04x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 59E8BCF3)
    (at 165.862 121.92 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 6.604 -2.286 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /PWM_OUT))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_PTV09A-1_Horizontal (layer F.Cu) (tedit 59D29A8A)
    (at 161.29 113.792)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, http://www.bourns.com/docs/Product-Datasheets/ptv09.pdf")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single")
    (fp_text reference RV1 (at 3.048 -2.54 90) (layer F.SilkS))
    (fp_text value 100k (at 3.048 0.254) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 /TRIG))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 0 np_thru_hole circle (at 7 -6.9) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad 0 np_thru_hole circle (at 7 1.9) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_PTV09A-1_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 59D29AC9)
    (at 171.45 102.87 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 6.096 -2.286 180) (layer F.SilkS))
    (fp_text value 4.7K (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 59E82E24)
    (at 158.242 130.556 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U3 (at -1.016 2.286 180) (layer F.SilkS))
    (fp_text value 74AHC1G14 (at 0.254 -2.032 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.35 0 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /PWM_OUT))
    (pad 3 smd rect (at -1.35 0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.35 0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at 1.35 -0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:KiCad-Logo2_8mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 156.464 93.98)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_8mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 171.196 125.222 90)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 90) (layer F.Fab) hide)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C2071BD)
    (at 143.002 130.81)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "Jumper for Motherboard Power" (at 149.098 133.096) (layer F.SilkS))
  (gr_text "To Motherboard" (at 164.084 99.568) (layer F.SilkS))
  (gr_text "To Fans" (at 153.67 128.27) (layer F.SilkS))
  (gr_text https://github.com/mtreinish/pwmcontroller (at 165.608 133.604) (layer F.SilkS))
  (gr_text "PWM Controller v3.0\nMatthew Treinish" (at 141.224 121.666 90) (layer F.SilkS))
  (gr_line (start 174.498 89.916) (end 174.244 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.446 89.916) (end 174.498 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.446 134.366) (end 139.446 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.498 134.366) (end 139.446 134.366) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.498 89.916) (end 174.498 134.366) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.244 134.112) (xy 139.7 134.112) (xy 139.7 90.17) (xy 174.244 90.17)
      )
    )
  )
  (zone (net 4) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.244 134.112) (xy 139.7 134.112) (xy 139.7 90.17) (xy 174.244 90.17)
      )
    )
  )
)
