(kicad_pcb (version 20171130) (host pcbnew 5.0.1)
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 41)
    (zones 0)
    (modules 4)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FEFFB63F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /SHLD)
  (net 2 GND)
  (net 3 "Net-(J1-Pad4)")
  (net 4 /DP)
  (net 5 /DN)
  (net 6 "Net-(J2-Pad4)")
  (net 7 /5VA)
  (net 8 /5VB)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /5VA)
    (add_net /5VB)
    (add_net /DN)
    (add_net /DP)
    (add_net /SHLD)
    (add_net GND)
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad4)")
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 5BE49408)
    (at 150.114 101.346)
    (fp_text reference TP2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value 5VTB (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /5VB))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer B.Cu) (tedit 5BE493A9)
    (at 150.114 101.346)
    (fp_text reference TP1 (at 0 3.81) (layer B.SilkS) hide)
    (fp_text value 5VTA (at -1.905 -3.175) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 7 /5VA))
  )
  (module handy:USB_Micro-B (layer F.Cu) (tedit 58F7730C)
    (at 146.558 103.886 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J2 (at 0 -3.24 270) (layer F.SilkS) hide)
    (fp_text value USB_B_Micro (at 0 5.01 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /5VB))
    (pad 2 smd rect (at -0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /DN))
    (pad 3 smd rect (at 0 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /DP))
    (pad 4 smd rect (at 0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.5 -1.35) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 /SHLD))
    (pad 6 thru_hole circle (at 2.5 -1.35) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 /SHLD))
    (pad 6 thru_hole circle (at -3.5 1.35) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask)
      (net 1 /SHLD))
    (pad 6 thru_hole circle (at 3.5 1.35) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask)
      (net 1 /SHLD))
  )
  (module handy:USB_Micro-B (layer B.Cu) (tedit 58F7730C)
    (at 153.67 103.886 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at 0 3.24 270) (layer B.SilkS) hide)
    (fp_text value USB_B_Micro (at 0 -5.01 270) (layer B.Fab))
    (pad 6 thru_hole circle (at 3.5 -1.35 180) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask)
      (net 1 /SHLD))
    (pad 6 thru_hole circle (at -3.5 -1.35 180) (size 1.55 1.55) (drill 1.15) (layers *.Cu *.Mask)
      (net 1 /SHLD))
    (pad 6 thru_hole circle (at 2.5 1.35 180) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 /SHLD))
    (pad 6 thru_hole circle (at -2.5 1.35 180) (size 1.25 1.25) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 /SHLD))
    (pad 5 smd rect (at 1.3 1.35 180) (size 1.35 0.4) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 1.35 180) (size 1.35 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 1.35 180) (size 1.35 0.4) (layers B.Cu B.Paste B.Mask)
      (net 4 /DP))
    (pad 2 smd rect (at -0.65 1.35 180) (size 1.35 0.4) (layers B.Cu B.Paste B.Mask)
      (net 5 /DN))
    (pad 1 smd rect (at -1.3 1.35 180) (size 1.35 0.4) (layers B.Cu B.Paste B.Mask)
      (net 7 /5VA))
  )
  (gr_text 5 (at 150.114 99.7585 270) (layer F.Mask))
  (gr_text 5 (at 150.114 99.7585 270) (layer B.Mask))
  (gr_text GCNP (at 154.94 103.886 270) (layer B.Mask))
  (gr_text GN (at 147.828 103.886 270) (layer B.Mask))
  (gr_text SH (at 152.654 103.886 270) (layer F.Mask))
  (dimension 10.668 (width 0.3) (layer Cmts.User)
    (gr_text "10.668 mm" (at 136.076 103.886 270) (layer Cmts.User))
    (feature1 (pts (xy 140.716 109.22) (xy 137.589579 109.22)))
    (feature2 (pts (xy 140.716 98.552) (xy 137.589579 98.552)))
    (crossbar (pts (xy 138.176 98.552) (xy 138.176 109.22)))
    (arrow1a (pts (xy 138.176 109.22) (xy 137.589579 108.093496)))
    (arrow1b (pts (xy 138.176 109.22) (xy 138.762421 108.093496)))
    (arrow2a (pts (xy 138.176 98.552) (xy 137.589579 99.678504)))
    (arrow2b (pts (xy 138.176 98.552) (xy 138.762421 99.678504)))
  )
  (dimension 12.7 (width 0.3) (layer Cmts.User)
    (gr_text "12.700 mm" (at 150.114 94.928) (layer Cmts.User))
    (feature1 (pts (xy 156.464 98.044) (xy 156.464 96.441579)))
    (feature2 (pts (xy 143.764 98.044) (xy 143.764 96.441579)))
    (crossbar (pts (xy 143.764 97.028) (xy 156.464 97.028)))
    (arrow1a (pts (xy 156.464 97.028) (xy 155.337496 97.614421)))
    (arrow1b (pts (xy 156.464 97.028) (xy 155.337496 96.441579)))
    (arrow2a (pts (xy 143.764 97.028) (xy 144.890504 97.614421)))
    (arrow2b (pts (xy 143.764 97.028) (xy 144.890504 96.441579)))
  )
  (gr_line (start 144.272 98.552) (end 143.764 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.956 98.552) (end 144.272 98.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.464 99.06) (end 155.956 98.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.464 108.712) (end 156.464 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.956 109.22) (end 156.464 108.712) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.272 109.22) (end 155.956 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.764 108.712) (end 144.272 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.764 108.712) (end 143.764 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.272 109.22) (xy 155.956 109.22) (xy 156.464 108.712) (xy 156.464 99.06) (xy 155.956 98.552)
        (xy 144.272 98.552) (xy 143.764 99.06) (xy 143.764 108.712)
      )
    )
  )
  (zone (net 1) (net_name /SHLD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.272 109.22) (xy 155.956 109.22) (xy 156.464 108.712) (xy 156.464 99.06) (xy 155.956 98.552)
        (xy 144.272 98.552) (xy 143.764 99.06) (xy 143.764 108.712)
      )
    )
  )
)
