<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="64.5035" x2="0" y2="1" width="0" layer="20"/>
<wire x1="0" y1="1" x2="1" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1" y1="0" x2="82.1088" y2="0" width="0" layer="20"/>
<wire x1="82.1088" y1="0" x2="83.1088" y2="1" width="0" layer="20" curve="90"/>
<wire x1="83.1088" y1="1" x2="83.1088" y2="64.5035" width="0" layer="20"/>
<wire x1="83.1088" y1="64.5035" x2="81.8388" y2="65.7735" width="0" layer="20" curve="90"/>
<wire x1="81.8388" y1="65.7735" x2="1.27" y2="65.7735" width="0" layer="20"/>
<wire x1="1.27" y1="65.7735" x2="0" y2="64.5035" width="0" layer="20" curve="90"/>
<text>Barbouri 2022</text>
<text>HP 5300 A/B
Display Module
Test Card
Rev. B</text>
<text>Open Hardware</text>
<text>1--Hz
2--M
3--S
4--K
5--u
6--DP1
7--DP2
8--DP3
9--DP5
10-N/C</text>
<text>DP4</text>
<text>GND</text>
<text>POWER
SUPPLY</text>
<text>50</text>
<text>25</text>
<text>Test 1:
(4-1)-(42)
(36)-(45)
(38)-(44)
(40)-(43)
Power</text>
<text>Test 2:
(36)-(45)
(38-1)-(43)
(38-2)-(44)
(40)-(42)
Power</text>
<text>Test 3:
(36)-(43)
(38)-(44)
(40)-(45)
Power</text>
<text>Test 4:
(4-1)-(9)
(4-2)-(41)
(4-3)-(20)
(4-4)-(19)
(38)-(5)
Power</text>
<text>Test 6:
(4-1)-(9)
(4-3)-(20)
(4-4)-(19)
(5-1)-(13)
(7) - (16)
(36)-(37)
(38)-(39)
(40)-(41)
Power</text>
<text>Test 7:
(1) - (6)
(4-1)-(27)
(4-2)-(28)
(4-3)-(22)
(4-4)-(23)
(4-5)-(47)
(5-1)- (7)
(5-2)-(16)
(17)-(18)
(36)-(37)
(38)-(39)
(40)-(41)
Power</text>
<text>Test 8:
(4-1)-(42)
(36)-(45)
(38)-(44)
(40)-(43)
Power
Switch to
Hz
M
S
K
u
DP1
DP2
DP3
DP5
|
(4-2)-(47)
DP4</text>
<text>Test 9:
(4-1)- (9)
(4-2)-(20)
(4-3)-(19)
(5-1)-(18)
(7) -(16)
(36)-(37)
(38)-(39)
(40)-(41)
Power</text>
<text>Test 10:
(4-4)-(22)
Test 11:
(4-4)-(23)
Test 12:
(4-4)-(22)
(4-5)-(23)
Test 13:
(4-4)-(24)
Test 14:
(4-4)-(22)
(4-5)-(24)</text>
<text>Test 10-16
 Use same
 base
 settings
 as Test 9</text>
<text>Test 15:
(4-4)-(23)
(4-5)-(24)</text>
<text>Test 16:
(4-4)-(22)
(4-5)-(23)
(4-6)-(24)</text>
<text>(CC BY-SA 4.0)</text>
<text>Hewlett Packard 5300 series</text>
<text>Operating and Service Manual</text>
<text>Table 5-2,5-3,5-4</text>
<text>Test 5:
(4-1)-(9)
(4-2)-(20)
(4-3)-(19)
(4-4)-(22)</text>
<text>(4-5)-(37)
(4-6)-(39)
(4-7)-(41)
(5-1)-(16)
(17) -(18)</text>
<text>(43) -(21)
Power</text>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,17/1,3">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-champ">
<description>&lt;b&gt;IEEE488 (Centronics) Connectors from AMP&lt;/b&gt;&lt;p&gt;
Source: AMP Catalog&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="50H">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
horizontal with mounting hole</description>
</package>
</packages>
</library>
<library name="switch-grayhill">
<description>&lt;b&gt;Grayhill Rotary Switches&lt;/b&gt;&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2011, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="71-10-1D-1C">
<description>&lt;b&gt;Grayhill 71 Series&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TL3XPO">
<description>&lt;b&gt;TINY SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/700000-724999/705152-da-01-de-Subminiaturschalter_TL_36YO.pdf</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-17">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M_COPPER">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Top Copper&lt;/h3&gt;
&lt;p&gt;Exposed copper logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="+22" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="2110-2-00-80-00-00-07-0"/>
<attribute name="MFG" value="Mill-Max"/>
<attribute name="DESC" value="TERM TURRET SINGLE L=5.84mm Mt-Hole=1.3mm TIN"/>
</element>
<element name="-5" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="2110-2-00-80-00-00-07-0"/>
<attribute name="MFG" value="Mill-Max"/>
<attribute name="DESC" value="TERM TURRET SINGLE L=5.84mm Mt-Hole=1.3mm TIN"/>
</element>
<element name="+5" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="2110-2-00-80-00-00-07-0"/>
<attribute name="MFG" value="Mill-Max"/>
<attribute name="DESC" value="TERM TURRET SINGLE L=5.84mm Mt-Hole=1.3mm TIN"/>
</element>
<element name="-17" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="2110-2-00-80-00-00-07-0"/>
<attribute name="MFG" value="Mill-Max"/>
<attribute name="DESC" value="TERM TURRET SINGLE L=5.84mm Mt-Hole=1.3mm TIN"/>
</element>
<element name="+17" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="2110-2-00-80-00-00-07-0"/>
<attribute name="MFG" value="Mill-Max"/>
<attribute name="DESC" value="TERM TURRET SINGLE L=5.84mm Mt-Hole=1.3mm TIN"/>
</element>
<element name="PL1" library="con-amp-champ" package="50H" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
<attribute name="DESC" value="CONN SCSI RCPT 50POS R/A SOLDER"/>
<attribute name="MFG" value="NorComp Inc."/>
<attribute name="PN" value="112-050-213R001"/>
</element>
<element name="RST" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Mill-Max"/>
<attribute name="PN" value="2110-2-00-80-00-00-07-0"/>
<attribute name="DESC" value="TERM TURRET SINGLE L=5.84mm Mt-Hole=1.3mm TIN"/>
</element>
<element name="S1" library="switch-grayhill" package="71-10-1D-1C" value="71-10SP-1D">
<attribute name="LABEL" value=""/>
<attribute name="DESC" value="SWITCH ROTARY 2-10POS 250MA 115V"/>
<attribute name="MFG" value="Grayhill"/>
<attribute name="PN" value="71BDF36-01-1-AJN"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="switch" package="TL3XPO" value="POWER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="SWITCH TOGGLE SPST 0.4VA 28V Through Hole"/>
<attribute name="MFG" value="NKK Switches"/>
<attribute name="PN" value="A11JP"/>
</element>
<element name="PAD1" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5-1" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5-2" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="6" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="7" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="9" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="13" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="16" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="17" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="18" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="19" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="20" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="22" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="23" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="24" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="27" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="28" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="36" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="37" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="38-1" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="38-2" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="39" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="40" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="41" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="42" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="43" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="44" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="45" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="47" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="Pin Receptacle Connector 0.020&quot; ~ 0.032&quot; Mtg-hole=1.45mm"/>
<attribute name="MFG" value="Mill-Max"/>
<attribute name="PN" value="0338-0-15-15-15-27-10-0"/>
</element>
<element name="4-1" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="4-2" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="4-3" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="4-4" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="4-5" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="2110-2-00-80-00-00-07-0"/>
<attribute name="MFG" value="Mill-Max"/>
<attribute name="DESC" value="TERM TURRET SINGLE L=5.84mm Mt-Hole=1.3mm TIN"/>
</element>
<element name="U$2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M_COPPER" value=""/>
<element name="1" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="DESC" value="Pin Receptacle Connector 0.020&quot; ~ 0.032&quot; Mtg-hole=1.45mm"/>
<attribute name="PN" value="0338-0-15-15-15-27-10-0"/>
<attribute name="MFG" value="Mill-Max"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="4-6" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="4-7" library="testpad" package="P1-17" value="TPPAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="HOLD">
<contactref element="PL1" pad="19"/>
<contactref element="19" pad="TP"/>
</signal>
<signal name="TBSELA">
<contactref element="PL1" pad="22"/>
<contactref element="22" pad="TP"/>
</signal>
<signal name="1MHZIN">
<contactref element="PL1" pad="21"/>
</signal>
<signal name="DP4">
<contactref element="PL1" pad="47"/>
<contactref element="47" pad="TP"/>
</signal>
<signal name="DP3">
<contactref element="PL1" pad="46"/>
<contactref element="S1" pad="A8"/>
</signal>
<signal name="DP2">
<contactref element="PL1" pad="34"/>
<contactref element="S1" pad="A7"/>
</signal>
<signal name="DP1">
<contactref element="PL1" pad="33"/>
<contactref element="S1" pad="A6"/>
</signal>
<signal name="INHIBIT">
<contactref element="PL1" pad="8"/>
</signal>
<signal name="R/L">
<contactref element="PL1" pad="35"/>
</signal>
<signal name="EXPONENT">
<contactref element="PL1" pad="13"/>
<contactref element="13" pad="TP"/>
</signal>
<signal name="+5V">
<contactref element="PL1" pad="1"/>
<contactref element="+5" pad="1"/>
<contactref element="1" pad="TP"/>
</signal>
<signal name="-5V">
<contactref element="PL1" pad="2"/>
<contactref element="-5" pad="1"/>
</signal>
<signal name="-17V">
<contactref element="PL1" pad="3"/>
<contactref element="-17" pad="1"/>
</signal>
<signal name="GND">
<contactref element="PL1" pad="4"/>
<contactref element="S1" pad="A-COM"/>
<contactref element="4-1" pad="TP"/>
<contactref element="4-2" pad="TP"/>
<contactref element="4-3" pad="TP"/>
<contactref element="4-4" pad="TP"/>
<contactref element="4-5" pad="TP"/>
<contactref element="GND" pad="1"/>
<contactref element="PAD1" pad="1"/>
<contactref element="PAD2" pad="1"/>
<contactref element="4-6" pad="TP"/>
<contactref element="PL1" pad="49"/>
<contactref element="4-7" pad="TP"/>
</signal>
<signal name="F1">
<contactref element="PL1" pad="5"/>
<contactref element="5-1" pad="TP"/>
<contactref element="5-2" pad="TP"/>
</signal>
<signal name="F2">
<contactref element="PL1" pad="7"/>
<contactref element="7" pad="TP"/>
</signal>
<signal name="OPEN">
<contactref element="PL1" pad="9"/>
<contactref element="9" pad="TP"/>
</signal>
<signal name="CLOSE">
<contactref element="PL1" pad="10"/>
</signal>
<signal name="LOG">
<contactref element="PL1" pad="11"/>
</signal>
<signal name="MGFF">
<contactref element="PL1" pad="12"/>
</signal>
<signal name="OVERFLOW">
<contactref element="PL1" pad="14"/>
</signal>
<signal name="RESET">
<contactref element="PL1" pad="15"/>
<contactref element="RST" pad="1"/>
</signal>
<signal name="CLOCK">
<contactref element="PL1" pad="16"/>
<contactref element="16" pad="TP"/>
</signal>
<signal name="MAXTIME">
<contactref element="PL1" pad="17"/>
<contactref element="17" pad="TP"/>
</signal>
<signal name="TBOUTPUT">
<contactref element="PL1" pad="18"/>
<contactref element="18" pad="TP"/>
</signal>
<signal name="TRANSFER">
<contactref element="PL1" pad="20"/>
<contactref element="20" pad="TP"/>
</signal>
<signal name="TBSELB">
<contactref element="PL1" pad="23"/>
<contactref element="23" pad="TP"/>
</signal>
<signal name="TBSELC">
<contactref element="PL1" pad="24"/>
<contactref element="24" pad="TP"/>
</signal>
<signal name="+22V">
<contactref element="PL1" pad="25"/>
<contactref element="+22" pad="1"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="+17V">
<contactref element="PL1" pad="26"/>
<contactref element="+17" pad="1"/>
</signal>
<signal name="HZ">
<contactref element="PL1" pad="27"/>
<contactref element="S1" pad="A1"/>
<contactref element="27" pad="TP"/>
</signal>
<signal name="M">
<contactref element="PL1" pad="28"/>
<contactref element="S1" pad="A2"/>
<contactref element="28" pad="TP"/>
</signal>
<signal name="S">
<contactref element="PL1" pad="29"/>
<contactref element="S1" pad="A3"/>
</signal>
<signal name="K">
<contactref element="PL1" pad="30"/>
<contactref element="S1" pad="A4"/>
</signal>
<signal name="U">
<contactref element="PL1" pad="31"/>
<contactref element="S1" pad="A5"/>
</signal>
<signal name="MANRST">
<contactref element="PL1" pad="32"/>
</signal>
<signal name="DIGADRX">
<contactref element="PL1" pad="36"/>
<contactref element="36" pad="TP"/>
</signal>
<signal name="DIGSELX">
<contactref element="PL1" pad="37"/>
<contactref element="37" pad="TP"/>
</signal>
<signal name="DIGADRY">
<contactref element="PL1" pad="38"/>
<contactref element="38-1" pad="TP"/>
<contactref element="38-2" pad="TP"/>
</signal>
<signal name="DIGSELY">
<contactref element="PL1" pad="39"/>
<contactref element="39" pad="TP"/>
</signal>
<signal name="DIGADRZ">
<contactref element="PL1" pad="40"/>
<contactref element="40" pad="TP"/>
</signal>
<signal name="DIGSELZ">
<contactref element="PL1" pad="41"/>
<contactref element="41" pad="TP"/>
</signal>
<signal name="DATA-D">
<contactref element="PL1" pad="42"/>
<contactref element="42" pad="TP"/>
</signal>
<signal name="DATA-C">
<contactref element="PL1" pad="43"/>
<contactref element="43" pad="TP"/>
</signal>
<signal name="DATA-B">
<contactref element="PL1" pad="44"/>
<contactref element="44" pad="TP"/>
</signal>
<signal name="DATA-A">
<contactref element="PL1" pad="45"/>
<contactref element="45" pad="TP"/>
</signal>
<signal name="DP5">
<contactref element="PL1" pad="48"/>
<contactref element="S1" pad="A9"/>
</signal>
<signal name="9%">
<contactref element="PL1" pad="6"/>
<contactref element="6" pad="TP"/>
</signal>
<signal name="PWR-IN">
<contactref element="PL1" pad="50"/>
<contactref element="S2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
