(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 59)
    (zones 0)
    (modules 9)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.3048)
    (user_via 0.6858 0.3302)
    (user_via 0.8128 0.4064)
    (user_via 1.2192 0.6096)
    (user_via 1.4224 0.8128)
    (blind_buried_vias_allowed yes)
    (uvia_size 0.3302)
    (uvia_drill 0.2032)
    (uvias_allowed yes)
    (uvia_min_size 0.2032)
    (uvia_min_drill 0.1016)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.8 0.8)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFFEFF)
    (pcbplotparams
      (layerselection 0x010fc_fffffff9)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerbers"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VinA)
  (net 3 /VdivA)
  (net 4 /anode)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3302)
    (uvia_drill 0.2032)
    (add_net /VdivA)
    (add_net /VinA)
    (add_net /anode)
    (add_net GND)
    (add_net "Net-(JS1-Pad1)")
    (add_net "Net-(JS1-Pad11)")
    (add_net "Net-(JS1-Pad12)")
    (add_net "Net-(JS1-Pad17)")
    (add_net "Net-(JS1-Pad18)")
    (add_net "Net-(JS1-Pad2)")
    (add_net "Net-(JS1-Pad7)")
    (add_net "Net-(JS1-Pad8)")
  )
  (net_class 10mil ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.2032)
  )
  (net_class 15mil ""
    (clearance 0.1524)
    (trace_width 0.381)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.2032)
  )
  (net_class 20mil ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 1.2192)
    (via_drill 0.6096)
    (uvia_dia 0.3302)
    (uvia_drill 0.2032)
  )
  (net_class 25mil ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 1.4224)
    (via_drill 0.8128)
    (uvia_dia 0.3302)
    (uvia_drill 0.2032)
  )
  (net_class 6mil ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3302)
    (uvia_drill 0.2032)
  )
  (net_class 8mil ""
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3302)
    (uvia_drill 0.2032)
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer F.Cu) (tedit 5C5B15B8)
    (at 0 -1.524 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.27 1.4605) (layer F.SilkS))
    (fp_text value 1.2nF (at 0 0.35) (layer F.Fab))
    (fp_text user %R (at 0.15 -0.2) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /anode))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm_numbers (layer F.Cu) (tedit 60101B89)
    (at -1.3462 7.0866 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 2.1971 -0.2413 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user 2 (at -1.905 2.54 90) (layer F.SilkS))
    (fp_text user 1 (at -1.905 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VinA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer F.Cu) (tedit 5C5B15B8)
    (at 0 1.524 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 1.3335 -1.651) (layer F.SilkS))
    (fp_text value 1.2nF (at 0 0.35) (layer F.Fab))
    (fp_text user %R (at 0.15 -0.2) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /anode))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:SSMB_TH (layer F.Cu) (tedit 60820D74)
    (at -0.0254 -8.4074)
    (descr "SSMB Jack Thru-Hole Connector .026\" Round Contact")
    (tags "SSMB ")
    (fp_text reference J1 (at -1.4986 3.1369 180) (layer F.SilkS))
    (fp_text value BNC (at 5.588 0.508) (layer F.Fab))
    (fp_text user %R (at 4.318 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 /VinA))
    (pad 2 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG}/MSAG_KiCad3d/ssmb_straight_7209-1511-050.STEP
      (offset (xyz 0 0 6.7))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer F.Cu) (tedit 5C5B175C)
    (at 3.429 1.397 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -1.397 1.778) (layer F.SilkS))
    (fp_text value 10 (at 0 0.35 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /VdivA))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer F.Cu) (tedit 5C5B175C)
    (at 3.429 -3.476 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -0.127 1.8415 180) (layer F.SilkS))
    (fp_text value 2.7k (at 0 0.35 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /VdivA))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /VinA))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer F.Cu) (tedit 5C5B175C)
    (at 3.429 -8.382 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.175 -1.778 180) (layer F.SilkS))
    (fp_text value 49.9 (at 0 0.35 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /VinA))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer F.Cu) (tedit 5C5B15B8)
    (at 3.429 6.223 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference Cq1 (at -1.778 1.905 270) (layer F.SilkS))
    (fp_text value 130pF_NP0 (at 0 0.35 90) (layer F.Fab))
    (fp_text user %R (at 0.15 -0.2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /anode))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VdivA))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:CLP-109-02-F-D-A (layer B.Cu) (tedit 5DCFF754)
    (at 0 0 180)
    (descr "surface-mounted straight pin header, 2x08, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x08 1.27mm double row")
    (attr smd)
    (fp_text reference JS1 (at -1.46812 4.38658) (layer B.SilkS) hide)
    (fp_text value CLP-109-02-F-D-A (at 0 -6.775) (layer B.Fab))
    (fp_text user %R (at 0 0.635 270) (layer B.Fab))
    (pad 18 smd rect (at -1.6129 -5.08 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd rect (at -1.6129 -3.81 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask)
      (net 4 /anode))
    (pad 14 smd rect (at -1.6129 -2.54 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask)
      (net 4 /anode))
    (pad 12 smd rect (at -1.6129 -1.27 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd rect (at 1.6129 -5.08 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 1.6129 -3.81 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask)
      (net 4 /anode))
    (pad 13 smd rect (at 1.6129 -2.54 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask)
      (net 4 /anode))
    (pad 11 smd rect (at 1.6129 -1.27 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at 1.6129 5.08 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 1.6129 0 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.6129 3.81 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask)
      (net 4 /anode))
    (pad 5 smd rect (at 1.6129 2.54 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask)
      (net 4 /anode))
    (pad 7 smd rect (at 1.6129 1.27 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at -1.6129 0 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -1.6129 1.27 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -1.6129 2.54 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask)
      (net 4 /anode))
    (pad 4 smd rect (at -1.6129 3.81 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask)
      (net 4 /anode))
    (pad 2 smd rect (at -1.6129 5.08 180) (size 1.4732 0.7366) (layers B.Cu B.Paste B.Mask))
    (pad 20 thru_hole circle (at 0 4.445 180) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 0 -4.445 180) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (model ${MSAG}/MSAG_KiCad3d/CLP-109-02-F-D-A.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (gr_line (start 4.953 9.5885) (end 4.953 -10.922) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -2.7305 -4.445) (end -2.7305 -10.922) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -2.7305 9.5885) (end -2.7305 -4.445) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 4.953 9.5885) (end -2.7305 9.5885) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -2.7305 -10.922) (end 4.953 -10.922) (layer Edge.Cuts) (width 0.15))
)
