(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 9)
    (no_connects 0)
    (area 125.654999 78.156999 187.019001 102.818001)
    (thickness 1.6)
    (drawings 20)
    (tracks 0)
    (zones 0)
    (modules 5)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /pwr_a)
  (net 2 /pwr_b)
  (net 3 /gnd)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /gnd)
    (add_net /pwr_a)
    (add_net /pwr_b)
  )
  (module Connectors_Molex:Molex_MegaFit_2x02x5.70mm_Angled (layer F.Cu) (tedit 58A287C1)
    (at 153.416 94.488)
    (descr "Molex MegaFit, dual row, side entry type, through hole")
    (tags "connector molex mega-fit 76825-0004 172064-0004 172064-1004")
    (fp_text reference J1 (at 2.85 9) (layer F.SilkS))
    (fp_text value Break (at 2.85 10.5) (layer F.Fab))
    (fp_text user %R (at 2.85 -11) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 1 /pwr_a))
    (pad 2 thru_hole circle (at 5.7 0) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 1 /pwr_a))
    (pad 3 thru_hole circle (at 0 5.5) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /pwr_b))
    (pad 4 thru_hole circle (at 5.7 5.5) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /pwr_b))
    (pad "" np_thru_hole circle (at 2.85 -7.3) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_MegaFit_2x02x5.70mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MegaFit_2x02x5.70mm_Angled (layer F.Cu) (tedit 58A287C1)
    (at 141.986 98.552 90)
    (descr "Molex MegaFit, dual row, side entry type, through hole")
    (tags "connector molex mega-fit 76825-0004 172064-0004 172064-1004")
    (fp_text reference J2 (at 2.85 9 90) (layer F.SilkS))
    (fp_text value Pwr_Out (at 2.85 10.5 90) (layer F.Fab))
    (fp_text user %R (at 2.85 -11 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /pwr_b))
    (pad 2 thru_hole circle (at 5.7 0 90) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /pwr_b))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /gnd))
    (pad 4 thru_hole circle (at 5.7 5.5 90) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /gnd))
    (pad "" np_thru_hole circle (at 2.85 -7.3 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_MegaFit_2x02x5.70mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MegaFit_2x02x5.70mm_Angled (layer F.Cu) (tedit 58A287C1)
    (at 170.688 92.964 270)
    (descr "Molex MegaFit, dual row, side entry type, through hole")
    (tags "connector molex mega-fit 76825-0004 172064-0004 172064-1004")
    (fp_text reference J3 (at 2.85 9 270) (layer F.SilkS))
    (fp_text value Pwr_In (at 2.85 10.5 270) (layer F.Fab))
    (fp_text user %R (at 2.85 -11 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 1 /pwr_a))
    (pad 2 thru_hole circle (at 5.7 0 270) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 1 /pwr_a))
    (pad 3 thru_hole circle (at 0 5.5 270) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /gnd))
    (pad 4 thru_hole circle (at 5.7 5.5 270) (size 3.75 3.75) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /gnd))
    (pad "" np_thru_hole circle (at 2.85 -7.3 270) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_MegaFit_2x02x5.70mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO14580 (layer F.Cu) (tedit 5AD5766C)
    (at 147.32 86.614)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO14580")
    (tags "mounting hole 2.7mm no annular m2.5 iso14580")
    (attr virtual)
    (fp_text reference "" (at 0 -3.25) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5_ISO14580 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO14580 (layer F.Cu) (tedit 5AD57675)
    (at 165.354 86.614)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO14580")
    (tags "mounting hole 2.7mm no annular m2.5 iso14580")
    (attr virtual)
    (fp_text reference "" (at 0 -3.25) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5_ISO14580 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_text B (at 156.337 94.869) (layer F.SilkS))
  (gr_text A (at 156.21 100.076) (layer F.SilkS))
  (gr_text gnd (at 165.227 95.631) (layer F.SilkS))
  (gr_text Vin (at 169.926 95.885) (layer F.SilkS))
  (gr_text Vin (at 143.002 95.758) (layer F.SilkS))
  (gr_text gnd (at 147.574 95.504) (layer F.SilkS))
  (gr_line (start 186.944 102.743) (end 186.944 102.362) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 102.743) (end 125.73 102.362) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.894 89.154) (end 186.944 89.154) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.814 78.232) (end 162.814 84.074) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.894 84.074) (end 162.814 84.074) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.894 89.154) (end 167.894 84.074) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 84.074) (end 149.86 78.232) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 84.074) (end 149.86 84.074) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 89.154) (end 144.78 84.074) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 89.154) (end 144.78 89.154) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 89.154) (end 125.73 102.362) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.814 78.232) (end 149.86 78.232) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.944 102.362) (end 186.944 89.154) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 102.743) (end 186.944 102.743) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name /gnd) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 3))
    (polygon
      (pts
        (xy 174.498 101.346) (xy 136.906 101.346) (xy 136.906 89.916) (xy 174.498 89.916)
      )
    )
  )
  (zone (net 2) (net_name /pwr_b) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 3))
    (polygon
      (pts
        (xy 149.987 97.409) (xy 162.052 97.409) (xy 162.052 102.616) (xy 138.684 102.616) (xy 138.684 89.916)
        (xy 149.987 89.916)
      )
    )
  )
  (zone (net 1) (net_name /pwr_a) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 3))
    (polygon
      (pts
        (xy 150.749 90.805) (xy 150.749 96.901) (xy 162.687 96.901) (xy 162.687 101.854) (xy 173.99 101.854)
        (xy 173.99 89.662) (xy 150.749 89.662)
      )
    )
  )
)
