<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.165" y2="0" width="0" layer="20"/>
<wire x1="50.165" y1="0" x2="50.165" y2="28.575" width="0" layer="20"/>
<wire x1="50.165" y1="28.575" x2="0" y2="28.575" width="0" layer="20"/>
<wire x1="0" y1="28.575" x2="0" y2="0" width="0" layer="20"/>
<text>BLK</text>
<text>RF Radio</text>
<text>1</text>
<text>GRN</text>
<text>R</text>
<text>Y</text>
<text>G</text>
<text>+</text>
<text>-</text>
<text>RF RAS node Ver 1</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="FTDI_BASIC">
</package>
<package name="2X4">
</package>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="atmega8">
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
</packages>
</library>
<library name="JC">
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-omron">
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="breakout-board">
<packages>
<package name=".6X.6">
<description>0.6 x 0.6 inch Board Step-Up Voltage</description>
</package>
</packages>
</library>
<library name="RHT03_DHT-22_AM2302">
<description>&lt;h1&gt;RHT03 / DHT-22 / AM2302 library&lt;/h1&gt;
&lt;p&gt;
Library with devices (schematic symbol and packages) for the RHT03 / DHT-22 / AM2302 digital relative humidity and tempearture sensor.&lt;br /&gt;
Warning: Package does not include tKeepout areas so that the part may optionally be placed on a riser with components underneath.  Please keep the package outline and bent-pin space in mind.
&lt;/p&gt;</description>
<packages>
<package name="RHT03_DHT-22">
<description>&lt;h1&gt;RHT03 / DHT-22&lt;/h1&gt;
&lt;p&gt;
Package for the RHT03 / DHT-22 relative humidity and temperature sensor.
&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="resistor" package="C025-025X050" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="resistor" package="C025-025X050" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="resistor" package="C025-025X050" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="atmega8" package="DIL28-3" value="ATMEGA328">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="R1" library="resistor" package="0204V" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun" package="FTDI_BASIC" value="FTDI_BASICPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun" package="1X02_LOCK" value="EXTPWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun" package="2X4" value="RADIO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="crystal" package="HC49/S" value="8MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="resistor" package="C025-025X050" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="resistor" package="C025-025X050" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="JC" package="TO-92" value="MCP9700">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="0204V" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor" package="0204V" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="resistor" package="C025-025X050" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP8" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP9" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="S1" library="switch-omron" package="B3F-10XX" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED_R" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED_Y" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED_G" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistor" package="0204V" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="resistor" package="0204V" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="resistor" package="0204V" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="resistor" package="C025-025X050" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun" package="1X02_LOCK" value="EXTPWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun" package="1X02_LOCK" value="EXTPWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="breakout-board" package=".6X.6" value="PRT-09216">
<attribute name="NAME"/>
</element>
<element name="IC4" library="RHT03_DHT-22_AM2302" package="RHT03_DHT-22" value="">
<attribute name="PROD_ID" value="SEN-10167"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="resistor" package="0204V" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="resistor" package="0204V" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="resistor" package="0204V" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="22"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="JP7" pad="GND"/>
<contactref element="JP7" pad="CTS"/>
<contactref element="U$2" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="LED_Y" pad="K"/>
<contactref element="LED_R" pad="K"/>
<contactref element="LED_G" pad="K"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="C7" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC4" pad="GND"/>
<contactref element="IC4" pad="NULL"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="C3" pad="1"/>
<contactref element="JP7" pad="DTR"/>
</signal>
<signal name="RED_LED">
<contactref element="IC2" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="GRN_LED">
<contactref element="IC2" pad="11"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="S1">
<contactref element="IC2" pad="12"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="IC2" pad="28"/>
<contactref element="JP5" pad="4"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="IC2" pad="27"/>
<contactref element="JP5" pad="3"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="VOLTAGE">
<contactref element="IC2" pad="26"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="RXI">
<contactref element="IC2" pad="2"/>
<contactref element="JP7" pad="TXO"/>
</signal>
<signal name="TXO">
<contactref element="IC2" pad="3"/>
<contactref element="JP7" pad="RXI"/>
</signal>
<signal name="AREF">
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="RESET">
<contactref element="IC2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="U$2" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="C6" pad="2"/>
<contactref element="IC2" pad="20"/>
<contactref element="R1" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="JP7" pad="VCC"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC4" pad="VDD"/>
<contactref element="R7" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="UC10">
<contactref element="IC2" pad="16"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="6"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="7"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="5"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="DATA">
<contactref element="IC4" pad="DATA"/>
<contactref element="R7" pad="2"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="UCA1">
<contactref element="IC2" pad="24"/>
</signal>
<signal name="RFCE">
<contactref element="U$2" pad="3"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="RFCSN">
<contactref element="U$2" pad="4"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="RFIRQ">
<contactref element="U$2" pad="8"/>
</signal>
<signal name="XTAL1">
<contactref element="Q1" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="XTAL2">
<contactref element="Q1" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="TEMP">
<contactref element="IC3" pad="2"/>
<contactref element="IC2" pad="25"/>
</signal>
<signal name="N$2">
<contactref element="LED_R" pad="A"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LED_Y" pad="A"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LED_G" pad="A"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="YEL_LED">
<contactref element="R5" pad="2"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="EXTPWR">
<contactref element="JP6" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC2" pad="4"/>
</signal>
<signal name="UCA0">
<contactref element="IC2" pad="23"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
