(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 16)
    (no_connects 8)
    (area 34.490457 51.8726 141.885715 126.8459)
    (thickness 1.6)
    (drawings 32)
    (tracks 426)
    (zones 0)
    (modules 56)
    (nets 2)
  )
  (page A4)
  (layers
    (0 F.Cu power)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.762)
    (user_trace_width 0.381)
    (user_trace_width 0.762)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.001)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (user_via 0.458 0.26)
    (user_via 0.7 0.35)
    (user_via 0.85 0.51)
    (user_via 1 0.6)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.85 0.85)
    (pad_drill 0.51)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFBF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GND)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A8DB679)
    (at 124 57)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AC2CD10)
    (at 96.15 105.04 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference "" (at 0.95 -1.86 180) (layer F.SilkS) hide)
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (at 0.95 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 1.9 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5AC2C926)
    (at 95.515 101.595)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference "" (at 1.27 -3.56) (layer F.SilkS) hide)
    (fp_text value TO-92_Inline_Narrow_Oval (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module help:2200_2301 (layer F.Cu) (tedit 5ABAC9BC)
    (at 114 101 180)
    (fp_text reference REF** (at 3.07 0.59 180) (layer F.SilkS) hide)
    (fp_text value "2200 2301" (at 3.4 -0.46 180) (layer F.Fab))
    (pad 8 thru_hole circle (at -6.22 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.22 0.88 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 11.55 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 11.55 0.89 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -3.68 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AA96D12)
    (at 112.4 95.92 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference REF** (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value D_SOD-123 (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at 0 -2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Mask))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AA96D12)
    (at 112.4 83.92 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference REF** (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value D_SOD-123 (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at 0 -2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Mask))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module help:2200_2301 (layer F.Cu) (tedit 5ABAC9BC)
    (at 114 89 180)
    (fp_text reference REF** (at 3.07 0.59 180) (layer F.SilkS) hide)
    (fp_text value "2200 2301" (at 3.4 -0.46 180) (layer F.Fab))
    (pad 8 thru_hole circle (at -6.22 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.22 0.88 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 11.55 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 11.55 0.89 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -3.68 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5AC2C926)
    (at 95.515 89.595)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference "" (at 1.27 -3.56) (layer F.SilkS) hide)
    (fp_text value TO-92_Inline_Narrow_Oval (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AC2CD10)
    (at 96.15 93.04 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference "" (at 0.95 -1.86 180) (layer F.SilkS) hide)
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (at 0.95 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 1.9 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AC2CD10)
    (at 96.15 69.04 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference "" (at 0.95 -1.86 180) (layer F.SilkS) hide)
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (at 0.95 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 1.9 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5AC2C926)
    (at 95.515 65.595)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference "" (at 1.27 -3.56) (layer F.SilkS) hide)
    (fp_text value TO-92_Inline_Narrow_Oval (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module help:2200_2301 (layer F.Cu) (tedit 5ABAC9BC)
    (at 114 65 180)
    (fp_text reference REF** (at 3.07 0.59 180) (layer F.SilkS) hide)
    (fp_text value "2200 2301" (at 3.4 -0.46 180) (layer F.Fab))
    (pad 8 thru_hole circle (at -6.22 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.22 0.88 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 11.55 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 11.55 0.89 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -3.68 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AA96D12)
    (at 112.4 59.92 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference REF** (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value D_SOD-123 (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at 0 -2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Mask))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AA96D12)
    (at 112.4 71.92 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference REF** (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value D_SOD-123 (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at 0 -2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Mask))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module help:2200_2301 (layer F.Cu) (tedit 5ABAC9BC)
    (at 114 77 180)
    (fp_text reference REF** (at 3.07 0.59 180) (layer F.SilkS) hide)
    (fp_text value "2200 2301" (at 3.4 -0.46 180) (layer F.Fab))
    (pad 8 thru_hole circle (at -6.22 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.22 0.88 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 11.55 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 11.55 0.89 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -3.68 -1.65 180) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5AC2C926)
    (at 95.515 77.595)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference "" (at 1.27 -3.56) (layer F.SilkS) hide)
    (fp_text value TO-92_Inline_Narrow_Oval (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AC2CD10)
    (at 96.15 81.04 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference "" (at 0.95 -1.86 180) (layer F.SilkS) hide)
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (at 0.95 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 1.9 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AC2CD10)
    (at 69.85 85.96)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference "" (at 0.95 -1.86) (layer F.SilkS) hide)
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5AC2C926)
    (at 70.485 89.405 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference "" (at 1.27 -3.56 180) (layer F.SilkS) hide)
    (fp_text value TO-92_Inline_Narrow_Oval (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 2.54 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module help:2200_2301 (layer F.Cu) (tedit 5ABAC9BC)
    (at 52 90)
    (fp_text reference REF** (at 3.07 0.59) (layer F.SilkS) hide)
    (fp_text value "2200 2301" (at 3.4 -0.46) (layer F.Fab))
    (pad 8 thru_hole circle (at -6.22 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.22 0.88) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 11.55 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 11.55 0.89) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -3.68 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AA96D12)
    (at 53.6 95.08)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference REF** (at 0 -2) (layer F.SilkS) hide)
    (fp_text value D_SOD-123 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Mask))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AA96D12)
    (at 53.6 107.08)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference REF** (at 0 -2) (layer F.SilkS) hide)
    (fp_text value D_SOD-123 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Mask))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module help:2200_2301 (layer F.Cu) (tedit 5ABAC9BC)
    (at 52 102)
    (fp_text reference REF** (at 3.07 0.59) (layer F.SilkS) hide)
    (fp_text value "2200 2301" (at 3.4 -0.46) (layer F.Fab))
    (pad 8 thru_hole circle (at -6.22 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.22 0.88) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 11.55 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 11.55 0.89) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -3.68 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5AC2C926)
    (at 70.485 101.405 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference "" (at 1.27 -3.56 180) (layer F.SilkS) hide)
    (fp_text value TO-92_Inline_Narrow_Oval (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 2.54 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AC2CD10)
    (at 69.85 97.96)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference "" (at 0.95 -1.86) (layer F.SilkS) hide)
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AC2CD10)
    (at 69.85 73.96)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference "" (at 0.95 -1.86) (layer F.SilkS) hide)
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5AC2C926)
    (at 70.485 77.405 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference "" (at 1.27 -3.56 180) (layer F.SilkS) hide)
    (fp_text value TO-92_Inline_Narrow_Oval (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 2.54 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module help:2200_2301 (layer F.Cu) (tedit 5ABAC9BC)
    (at 52 78)
    (fp_text reference REF** (at 3.07 0.59) (layer F.SilkS) hide)
    (fp_text value "2200 2301" (at 3.4 -0.46) (layer F.Fab))
    (pad 8 thru_hole circle (at -6.22 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.22 0.88) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 11.55 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 11.55 0.89) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -3.68 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AA96D12)
    (at 53.6 83.08)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference REF** (at 0 -2) (layer F.SilkS) hide)
    (fp_text value D_SOD-123 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Mask))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AA96D12)
    (at 53.6 71.08)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference REF** (at 0 -2) (layer F.SilkS) hide)
    (fp_text value D_SOD-123 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Mask))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5A95A6CE)
    (at 88.05 119.4685)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.75 1) (layers B.Cu B.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5A95A6D3)
    (at 86.78 119.4685)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.75 1) (layers B.Cu B.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5A95A6C3)
    (at 85.51 119.4685)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.75 1) (layers B.Cu B.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5A95A6C8)
    (at 84.24 119.4685)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.75 1) (layers B.Cu B.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5A95A6BE)
    (at 82.97 119.4685)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.75 1) (layers B.Cu B.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5A95A6AD)
    (at 81.7 119.4685)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.75 1) (layers B.Cu B.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5A95A6B1)
    (at 80.43 119.4685)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.75 1) (layers B.Cu B.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5A95A6B5)
    (at 79.16 119.4685)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.75 1) (layers B.Cu B.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5A95A6A1)
    (at 77.89 119.4685)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.75 1) (layers B.Cu B.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5A95A6A6)
    (at 76.62 119.4685)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.75 1) (layers B.Cu B.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5A95A1EE)
    (at 82.97 118.77)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_0-8mmDrill (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.51) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5A95A1EE)
    (at 84.24 118.77)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_0-8mmDrill (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.51) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5A95A1EE)
    (at 88.05 118.77)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_0-8mmDrill (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.51) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5A95A1EE)
    (at 85.51 118.77)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_0-8mmDrill (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.51) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5A95A1EE)
    (at 86.78 118.77)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_0-8mmDrill (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.51) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5A95A1EE)
    (at 80.43 118.77)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_0-8mmDrill (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.51) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5A95A1EE)
    (at 79.16 118.77)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_0-8mmDrill (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.51) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5A95A1EE)
    (at 81.7 118.77)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_0-8mmDrill (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.51) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5A95A1EE)
    (at 77.89 118.77)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_0-8mmDrill (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.51) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A8DB679)
    (at 44 57)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module help:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 5A8DB693)
    (at 82.5 61.5)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_2x05_Pitch2.54mm (at 1.27 12.49) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 5A8DB630)
    (at 45.88 116)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference REF** (at 0 -5) (layer F.SilkS) hide)
    (fp_text value SMA_THT_Jack_Straight (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5A95A1EE)
    (at 76.62 118.77)
    (fp_text reference REF** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_0-8mmDrill (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.85 0.85) (drill 0.51) (layers *.Cu *.Mask))
  )
  (module help:2200_2301 (layer F.Cu) (tedit 5ABAC9BC)
    (at 52 66)
    (fp_text reference REF** (at 3.07 0.59) (layer F.SilkS) hide)
    (fp_text value "2200 2301" (at 3.4 -0.46) (layer F.Fab))
    (pad 8 thru_hole circle (at -6.22 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.22 0.88) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 11.55 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 11.55 0.89) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -3.68 -1.65) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5AC2C926)
    (at 70.485 65.405 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference "" (at 1.27 -3.56 180) (layer F.SilkS) hide)
    (fp_text value TO-92_Inline_Narrow_Oval (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 2.54 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AC2CD10)
    (at 69.85 61.96)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference "" (at 0.95 -1.86) (layer F.SilkS) hide)
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 87 74) (layer F.SilkS))
  (gr_text VCC (at 81 74) (layer F.SilkS))
  (gr_text "FIU switching circuit April 2018" (at 84 56) (layer F.SilkS))
  (gr_text 8 (at 124 65) (layer F.SilkS))
  (gr_text 7 (at 124 77) (layer F.SilkS))
  (gr_text 6 (at 124 90) (layer F.SilkS))
  (gr_text "5\n" (at 124 101) (layer F.SilkS))
  (gr_text 4 (at 42 101) (layer F.SilkS))
  (gr_text "3\n" (at 42 90) (layer F.SilkS))
  (gr_text 2 (at 42 78) (layer F.SilkS))
  (gr_text "1\n" (at 42 66) (layer F.SilkS))
  (dimension 88 (width 0.3) (layer Cmts.User)
    (gr_text "3.4646 in" (at 84 124.35) (layer Cmts.User))
    (feature1 (pts (xy 128 121) (xy 128 125.7)))
    (feature2 (pts (xy 40 121) (xy 40 125.7)))
    (crossbar (pts (xy 40 123) (xy 128 123)))
    (arrow1a (pts (xy 128 123) (xy 126.873496 123.586421)))
    (arrow1b (pts (xy 128 123) (xy 126.873496 122.413579)))
    (arrow2a (pts (xy 40 123) (xy 41.126504 123.586421)))
    (arrow2b (pts (xy 40 123) (xy 41.126504 122.413579)))
  )
  (dimension 68 (width 0.3) (layer Cmts.User)
    (gr_text "2.6772 in" (at 136.35 87 270) (layer Cmts.User))
    (feature1 (pts (xy 128 121) (xy 137.7 121)))
    (feature2 (pts (xy 128 53) (xy 137.7 53)))
    (crossbar (pts (xy 135 53) (xy 135 121)))
    (arrow1a (pts (xy 135 121) (xy 134.413579 119.873496)))
    (arrow1b (pts (xy 135 121) (xy 135.586421 119.873496)))
    (arrow2a (pts (xy 135 53) (xy 134.413579 54.126504)))
    (arrow2b (pts (xy 135 53) (xy 135.586421 54.126504)))
  )
  (gr_line (start 40 121) (end 40 120) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 44 121) (end 40 121) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 40 57) (end 40 120) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 75 121) (end 44 121) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 128 121) (end 125 121) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 128 60) (end 128 121) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 75 121) (end 125 121) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 128 60) (end 128 53) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 56 53) (end 128 53) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 57 53) (end 56 53) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 40 53) (end 57 53) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 40 57) (end 40 53) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_text "\n" (at 46.88 119) (layer F.SilkS))
  (gr_text "8\n" (at 84.5 58.5) (layer F.SilkS))
  (gr_text "4\n" (at 80.5 69.5) (layer F.SilkS))
  (gr_text "1\n" (at 80.5 58.5) (layer F.SilkS))
)
