(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 19)
    (no_connects 0)
    (area 96.444999 82.474999 142.315001 153.745001)
    (thickness 1.6)
    (drawings 22)
    (tracks 114)
    (zones 0)
    (modules 10)
    (nets 20)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(N1-Pad0)")
  (net 2 "Net-(N1-Pad1)")
  (net 3 "Net-(N1-Pad2)")
  (net 4 "Net-(N1-Pad3)")
  (net 5 "Net-(N1-Pad4)")
  (net 6 "Net-(N1-Pad5)")
  (net 7 "Net-(N1-Pad6)")
  (net 8 "Net-(N1-Pad7)")
  (net 9 "Net-(N1-Pad8)")
  (net 10 "Net-(N1-Pad9)")
  (net 11 "Net-(N1-PadA)")
  (net 12 "Net-(N1-PadLHDP)")
  (net 13 VCC)
  (net 14 GND)
  (net 15 +5V)
  (net 16 A)
  (net 17 B)
  (net 18 C)
  (net 19 D)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A)
    (add_net B)
    (add_net C)
    (add_net D)
    (add_net "Net-(N1-Pad0)")
    (add_net "Net-(N1-Pad1)")
    (add_net "Net-(N1-Pad2)")
    (add_net "Net-(N1-Pad3)")
    (add_net "Net-(N1-Pad4)")
    (add_net "Net-(N1-Pad5)")
    (add_net "Net-(N1-Pad6)")
    (add_net "Net-(N1-Pad7)")
    (add_net "Net-(N1-Pad8)")
    (add_net "Net-(N1-Pad9)")
    (add_net "Net-(N1-PadLHDP)")
  )
  (net_class Power ""
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.7)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(N1-PadA)")
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 114.3 143.51 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 A))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 B))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 C))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 D))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Display:nixie_in-12 (layer F.Cu) (tedit 5763CF61)
    (at 119.38 102.87)
    (descr >NAME)
    (fp_text reference N1 (at 9.58088 0.6985 90) (layer F.SilkS))
    (fp_text value IN-12B (at 9.58088 2.0193 90) (layer F.SilkS))
    (fp_text user IN-12 (at 0 -12.7) (layer F.SilkS))
    (fp_text user A (at 5.08 11.43) (layer F.SilkS))
    (pad 0 thru_hole circle (at 5.04698 4.49834) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(N1-Pad0)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad 1 thru_hole circle (at -4.31546 7.81558) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(N1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad 2 thru_hole circle (at -5.99948 4.49834) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(N1-Pad2)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad 3 thru_hole circle (at -6.12648 0) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(N1-Pad3)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad 4 thru_hole circle (at -5.99948 -4.49834) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(N1-Pad4)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad 5 thru_hole circle (at -4.31546 -7.81558) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(N1-Pad5)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad 6 thru_hole circle (at -0.3175 -8.81634) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(N1-Pad6)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad 7 thru_hole circle (at 3.68046 -7.81558) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(N1-Pad7)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad 8 thru_hole circle (at 5.04698 -4.49834) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(N1-Pad8)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad 9 thru_hole circle (at 5.17398 0) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(N1-Pad9)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad A thru_hole circle (at 3.68046 7.81558) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(N1-PadA)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad LHDP thru_hole circle (at -0.3175 8.81634) (size 2.54 2.54) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(N1-PadLHDP)") (solder_mask_margin 0.1016) (clearance 0.254))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 5762DFD4)
    (at 132.08 83.82)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 5762DFD4)
    (at 132.08 154.94)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin (layer F.Cu) (tedit 5762DFD4)
    (at 105.41 154.94)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 129.54 143.51 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 109.22 143.51 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM15mm (layer F.Cu) (tedit 569FCEE8)
    (at 133.35 134.62 90)
    (descr "Resistor, Axial, RM 15mm,")
    (tags "Resistor Axial RM 15mm")
    (fp_text reference R1 (at 7.5 -3.74904 90) (layer F.SilkS))
    (fp_text value 22K (at 7.5 4.0005 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 VCC))
    (pad 2 thru_hole circle (at 15 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(N1-PadA)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM15mm.wrl
      (at (xyz 0.295 0 0))
      (scale (xyz 0.395 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 54130A77)
    (at 109.22 133.35 90)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 0 -5.22 90) (layer F.SilkS))
    (fp_text value K155ID1 (at 0 -3.72 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(N1-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(N1-Pad9)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 A))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 D))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5V))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 B))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 C))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(N1-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(N1-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(N1-Pad7)"))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(N1-Pad6)"))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(N1-Pad4)"))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(N1-Pad5)"))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(N1-Pad1)"))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(N1-Pad0)"))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 5762DFD4)
    (at 105.41 83.82)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_line (start 100.33 81.28) (end 100.33 157.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 157.48) (end 137.16 81.28) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.87 160.02) (end 134.62 160.02) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.87 78.74) (end 134.62 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text MGE (at 118.11 154.94) (layer B.Paste))
  (gr_line (start 102.87 160.02) (end 100.33 157.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 160.02) (end 137.16 157.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 78.74) (end 137.16 81.28) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.33 81.28) (end 102.87 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "IN-12 Nixie Driver" (at 105.41 125.73 90) (layer B.SilkS))
  (gr_text "MGE 2016\nV1.0" (at 106.68 104.14 90) (layer B.SilkS))
  (gr_text 22K (at 134.62 127 90) (layer F.SilkS))
  (gr_text D (at 121.92 148.59 90) (layer F.SilkS))
  (gr_text C (at 119.38 148.59 90) (layer F.SilkS))
  (gr_text B (at 116.84 148.59 90) (layer F.SilkS))
  (gr_text A (at 114.3 148.59 90) (layer F.SilkS))
  (gr_text 5V (at 109.22 148.59 90) (layer F.SilkS))
  (gr_text HV+ (at 129.54 148.59 90) (layer F.SilkS))
  (gr_text GND (at 106.68 148.59 90) (layer F.SilkS))
  (gr_text GND (at 127 148.59 90) (layer F.SilkS))
  (gr_text K155ID1 (at 118.11 129.54) (layer F.SilkS))
)
