(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 45)
    (zones 0)
    (modules 15)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /OptoAnode)
  (net 2 /ShuntUP)
  (net 3 GND)
  (net 4 /ShuntGND)
  (net 5 /Intlk12)
  (net 6 /Las12V)
  (net 7 /KIGND)
  (net 8 /KILCK)
  (net 9 /Sig)
  (net 10 /5VPow)
  (net 11 /LasGND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /5VPow)
    (add_net /Intlk12)
    (add_net /KIGND)
    (add_net /KILCK)
    (add_net /Las12V)
    (add_net /LasGND)
    (add_net /OptoAnode)
    (add_net /ShuntGND)
    (add_net /ShuntUP)
    (add_net /Sig)
    (add_net GND)
  )
  (module JRogersFootprintLIbrary:QLMLogoMedium (layer B.Cu) (tedit 0)
    (at 159 86 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module JRogersFootprintLIbrary:QLMLogoSmall (layer F.Cu) (tedit 0)
    (at 138.5 84.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module JRogersFootprintLIbrary:B2100-13-F (layer F.Cu) (tedit 60462621)
    (at 123.36 90)
    (fp_text reference D1 (at 5.64 0) (layer F.SilkS))
    (fp_text value "B2100-13-F diode" (at 2.64 -3) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 smd rect (at 2.4 0 90) (size 2.21 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /OptoAnode))
    (pad 1 smd rect (at -2.4 0 90) (size 2.21 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /ShuntUP))
    (model R:/Cuprite/Electronics/JoshsKiCADLibraries/SamacSys_Parts.3dshapes/SMB_DIO.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JRogersFootprintLIbrary:B2100-13-F (layer F.Cu) (tedit 60462621)
    (at 152.5 83 180)
    (fp_text reference D2 (at 0 3) (layer F.SilkS))
    (fp_text value "B2100-13-F diode" (at 0.5 -3) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 smd rect (at 2.4 0 270) (size 2.21 2.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -2.4 0 270) (size 2.21 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /OptoAnode))
    (model R:/Cuprite/Electronics/JoshsKiCADLibraries/SamacSys_Parts.3dshapes/SMB_DIO.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PCL712AS (layer B.Cu) (tedit 6040D845)
    (at 139 96)
    (descr PCL712AS-1)
    (tags Connector)
    (fp_text reference PCL712AS (at 0 -12) (layer B.SilkS))
    (fp_text value Intlk12V (at -0.075 -2.49) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 2.355 2.355) (drill 1.57) (layers *.Cu *.Mask B.SilkS)
      (net 3 GND))
    (pad 2 thru_hole circle (at -3.96 -3.96 270) (size 2.355 2.355) (drill 1.57) (layers *.Cu *.Mask B.SilkS)
      (net 4 /ShuntGND))
    (pad 3 thru_hole circle (at 3.81 -4.98 270) (size 2.355 2.355) (drill 1.57) (layers *.Cu *.Mask B.SilkS)
      (net 5 /Intlk12))
    (model R:/Cuprite/Electronics/JoshsKiCADLibraries/SamacSys_Parts.3dshapes/PCL712AS.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5EA53D3B)
    (at 165 91.5 270)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (fp_text reference "NC room intlk" (at 1 -4 90) (layer F.SilkS))
    (fp_text value IntlkNC (at 1.27 4.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 2 /ShuntUP))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 4 /ShuntGND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5EA53D3B)
    (at 153.5 103 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (fp_text reference "12V laser PSU" (at 1.27 -4.12) (layer F.SilkS))
    (fp_text value Las12V (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 6 /Las12V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 11 /LasGND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5EA53D3B)
    (at 163.5 103)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (fp_text reference "KI interlock" (at 1.27 4) (layer F.SilkS))
    (fp_text value KIIntlk (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 7 /KIGND))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 8 /KILCK))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C)
    (at 123 97 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference "TO-236AB transistor" (at -3.5 2.5) (layer F.SilkS))
    (fp_text value TO-236ABBJT (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 /Sig))
    (pad 2 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /OptoAnode))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JRogersFootprintLIbrary:FODM124R2 (layer F.Cu) (tedit 604421B4)
    (at 164 83)
    (fp_text reference Q2 (at 4 0) (layer F.SilkS))
    (fp_text value "FODM121 Opto" (at 0 -3) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -3 -2) (layer F.SilkS))
    (fp_text user * (at -1.9177 -1.9939) (layer F.Fab))
    (fp_text user 0.11in/2.794mm (at -6.0325 0) (layer Dwgs.User))
    (fp_text user 0.022in/0.559mm (at 6.0325 -1.397) (layer Dwgs.User))
    (fp_text user 0.235in/5.969mm (at 0 -4.4831) (layer Dwgs.User))
    (fp_text user 0.076in/1.93mm (at -2.9845 4.4831) (layer Dwgs.User))
    (fp_text user * (at -1.5 -1.5) (layer F.SilkS))
    (fp_text user * (at -1.9177 -1.9939) (layer F.Fab))
    (pad 1 smd rect (at -2.9845 -1.397) (size 1.9304 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 /OptoAnode))
    (pad 2 smd rect (at -2.9845 1.397) (size 1.9304 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 2.9845 1.397) (size 1.9304 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 7 /KIGND))
    (pad 4 smd rect (at 2.9845 -1.397) (size 1.9304 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 8 /KILCK))
    (model R:/Cuprite/Electronics/JoshsKiCADLibraries/SamacSys_Parts.3dshapes/FODM121.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 126 104.45 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference 5k62 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 5k62 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 9 /Sig))
    (pad 2 smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 5 /Intlk12))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 119.5 104.45 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference 100k (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 9 /Sig))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 119.5 82.5 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference 100k (at 0 -2 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 2 /ShuntUP))
    (pad 1 smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 10 /5VPow))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 126 82.5 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference 400 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 400 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 10 /5VPow))
    (pad 2 smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 1 /OptoAnode))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-89-3_Handsoldering (layer F.Cu) (tedit 5C33D6DD)
    (at 155 92.5 90)
    (descr "SOT-89-3 Handsoldering")
    (tags "SOT-89-3 Handsoldering")
    (attr smd)
    (fp_text reference "5V LinReg" (at 0.3 -3.5 90) (layer F.SilkS))
    (fp_text value LinVReg5V (at 0.3 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0.5 0) (layer F.Fab))
    (pad 1 smd rect (at -2.15 -1.5 90) (size 2.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /5VPow))
    (pad 3 smd rect (at -2.15 1.5 90) (size 2.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /Las12V))
    (pad 2 smd custom (at -2.0625 0 90) (size 2.475 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /LasGND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 1.2375 -0.8665) (xy 5.3625 -0.8665) (xy 5.3625 0.8665) (xy 1.2375 0.8665)) (width 0))
      ))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Room interlock 12V" (at 139 103) (layer B.SilkS))
  (gr_text 12V (at 148.5 90.5) (layer B.SilkS))
  (gr_text shunt (at 128 92) (layer B.SilkS))
  (gr_text GND (at 146.5 99.5) (layer B.SilkS))
  (gr_text shunt (at 165 89) (layer F.SilkS))
  (gr_text GND (at 165 96.5) (layer F.SilkS))
  (gr_text GND (at 167.5 99) (layer F.SilkS))
  (gr_text LCK (at 162 99) (layer F.SilkS))
  (gr_text 12V (at 156.5 103) (layer F.SilkS))
  (gr_text GND (at 147.5 103) (layer F.SilkS))
  (gr_line (start 116.5 108.5) (end 116.5 78.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170 108.5) (end 116.5 108.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170 78.5) (end 170 108.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.5 78.5) (end 170 78.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170 108.5) (xy 116.5 108.5) (xy 116.5 78.5) (xy 170 78.5)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170 108.5) (xy 116.5 108.5) (xy 116.5 78.5) (xy 170 78.5)
      )
    )
  )
)
