(kicad_pcb (version 20171130) (host pcbnew 5.1.10)
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 59)
    (zones 0)
    (modules 5)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.5)
    (user_via 1.5 0.75)
    (user_via 2 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /3v3)
  (net 3 /Pump7)
  (net 4 /Pump8)
  (net 5 /Pump10)
  (net 6 "Net-(J1-Pad12)")
  (net 7 "Net-(J1-Pad10)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 /Pump9)
  (net 10 "Net-(J1-Pad5)")
  (net 11 "Net-(J1-Pad3)")
  (net 12 /12v)
  (net 13 /Pump6)
  (net 14 /Pump4)
  (net 15 /Pump3)
  (net 16 /Pump2)
  (net 17 /Pump1)
  (net 18 /DT)
  (net 19 "Net-(J1-Pad28)")
  (net 20 "Net-(J1-Pad27)")
  (net 21 /Pump5)
  (net 22 /Scale_SCK)
  (net 23 "Net-(J1-Pad34)")
  (net 24 "Net-(J1-Pad30)")
  (net 25 "Net-(J1-Pad25)")
  (net 26 "Net-(J1-Pad20)")
  (net 27 "Net-(J1-Pad17)")
  (net 28 "Net-(J1-Pad14)")
  (net 29 "Net-(J1-Pad9)")
  (net 30 "Net-(J1-Pad6)")
  (net 31 "Net-(J1-Pad33)")
  (net 32 "Net-(J1-Pad26)")
  (net 33 "Net-(J1-Pad24)")
  (net 34 "Net-(J1-Pad23)")
  (net 35 "Net-(J1-Pad22)")
  (net 36 "Net-(J1-Pad21)")
  (net 37 "Net-(J1-Pad19)")
  (net 38 "Net-(J1-Pad18)")
  (net 39 "Net-(J1-Pad11)")
  (net 40 "Net-(J1-Pad2)")
  (net 41 "Net-(J1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /12v)
    (add_net /3v3)
    (add_net /DT)
    (add_net /Pump1)
    (add_net /Pump10)
    (add_net /Pump2)
    (add_net /Pump3)
    (add_net /Pump4)
    (add_net /Pump5)
    (add_net /Pump6)
    (add_net /Pump7)
    (add_net /Pump8)
    (add_net /Pump9)
    (add_net /Scale_SCK)
    (add_net GND)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad27)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(J1-Pad33)")
    (add_net "Net-(J1-Pad34)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A433)
    (at 90 73 180)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference J1 (at -1.27 2.77) (layer B.SilkS))
    (fp_text value Raspberry_Pi (at 2 -51.03) (layer B.SilkS))
    (fp_text user %R (at -1.27 -24.13 270) (layer B.Fab))
    (pad 40 thru_hole oval (at -2.54 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /Pump1))
    (pad 39 thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 38 thru_hole oval (at -2.54 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /Pump3))
    (pad 37 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Pump2))
    (pad 36 thru_hole oval (at -2.54 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /Pump5))
    (pad 35 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /Pump4))
    (pad 34 thru_hole oval (at -2.54 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad34)"))
    (pad 33 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad33)"))
    (pad 32 thru_hole oval (at -2.54 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /Pump6))
    (pad 31 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /Scale_SCK))
    (pad 30 thru_hole oval (at -2.54 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad30)"))
    (pad 29 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /DT))
    (pad 28 thru_hole oval (at -2.54 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad28)"))
    (pad 27 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad27)"))
    (pad 26 thru_hole oval (at -2.54 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad26)"))
    (pad 25 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad25)"))
    (pad 24 thru_hole oval (at -2.54 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad24)"))
    (pad 23 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad23)"))
    (pad 22 thru_hole oval (at -2.54 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad22)"))
    (pad 21 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad21)"))
    (pad 20 thru_hole oval (at -2.54 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad20)"))
    (pad 19 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad19)"))
    (pad 18 thru_hole oval (at -2.54 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at -2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Pump8))
    (pad 15 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Pump7))
    (pad 14 thru_hole oval (at -2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Pump9))
    (pad 12 thru_hole oval (at -2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at -2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at -2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Pump10))
    (pad 6 thru_hole oval (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3v3))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 76.5 83.5 90)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0 90) (layer F.Fab) hide)
  )
  (module Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 76.5 76.5 90)
    (descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J5 (at 1 4.5 90) (layer F.SilkS))
    (fp_text value "12V Output" (at 1 -3.5 90) (layer F.SilkS))
    (fp_text user %R (at 1.25 2.7 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 12 /12v))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 83.5 112.5 270)
    (descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J4 (at 10 -4 90) (layer F.SilkS))
    (fp_text value "Scale Connector" (at 2 -4 90) (layer F.SilkS))
    (fp_text user %R (at 3.75 2.7 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 22 /Scale_SCK))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 18 /DT))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 /3v3))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B12B-XH-A_1x12_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 85.5 74 270)
    (descr "JST XH series connector, B12B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J3 (at 22.5 4 90) (layer F.SilkS))
    (fp_text value "Pump Connector" (at 13.75 4.5 90) (layer F.SilkS))
    (fp_text user %R (at 13.75 2.7 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 27.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 17 /Pump1))
    (pad 11 thru_hole oval (at 25 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 /Pump2))
    (pad 10 thru_hole oval (at 22.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 15 /Pump3))
    (pad 9 thru_hole oval (at 20 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 /Pump4))
    (pad 8 thru_hole oval (at 17.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 21 /Pump5))
    (pad 7 thru_hole oval (at 15 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 13 /Pump6))
    (pad 6 thru_hole oval (at 12.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 /Pump7))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 /Pump8))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 /Pump9))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 /Pump10))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 /12v))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B12B-XH-A_1x12_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Bartender v1.2 - Raspberry Pi Hat\ngithub.com/dburnsii/bartender" (at 76.5 105.5 90) (layer F.SilkS))
  (gr_line (start 95 70) (end 95 125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72 70) (end 95 70) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72 125) (end 72 70) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95 125) (end 72 125) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.5 124.5) (xy 73 124.5) (xy 73 70.5) (xy 94.5 70.5)
      )
    )
  )
)
