(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 17)
    (zones 0)
    (modules 8)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (user_trace_width 2)
    (user_trace_width 2.54)
    (user_trace_width 3)
    (user_trace_width 5)
    (user_trace_width 7)
    (user_trace_width 10)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.6 0.3)
    (user_via 0.7 0.3)
    (user_via 0.75 0.3)
    (user_via 0.8 0.35)
    (user_via 0.9 0.425)
    (user_via 1 0.5)
    (user_via 1.25 0.6)
    (user_via 1.5 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 3)
    (pad_drill 1.25)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J3-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net 3 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
  )
  (net_class 120VAC ""
    (clearance 3.250001)
    (trace_width 0.325)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.25)
    (diff_pair_gap 3.250001)
  )
  (net_class 12V ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.175)
    (diff_pair_gap 0.175)
  )
  (net_class 240VAC ""
    (clearance 12.75)
    (trace_width 0.35)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.275)
    (diff_pair_gap 12.75)
  )
  (net_class 24V ""
    (clearance 0.25)
    (trace_width 0.275)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class 48V ""
    (clearance 0.6)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.225)
    (diff_pair_gap 0.4)
  )
  (net_class Diff_100_Ohm_Outer ""
    (clearance 0.1524)
    (trace_width 0.175006)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.175006)
    (diff_pair_gap 0.1524)
  )
  (net_class SE_50_Ohm_Outer ""
    (clearance 0.29337)
    (trace_width 0.29337)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.29337)
    (diff_pair_gap 0.29337)
  )
  (module TPW-Decorative:webster-face (layer F.Cu) (tedit 0)
    (at 40.9 39.7)
    (fp_text reference G?1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value WebsterFace (at 0.75 0) (layer F.SilkS) hide)
  )
  (module TPW-Decorative:sig-wlx (layer F.Cu) (tedit 637727B1)
    (at 51.5 46.5)
    (attr virtual)
    (fp_text reference G1 (at 0 0.1) (layer F.SilkS) hide)
    (fp_text value WLX (at 0.75 0.1) (layer F.SilkS) hide)
  )
  (module TPW-Connectors:01x06-P7.5mm-d1.5mm-SA929 (layer F.Cu) (tedit 65D31D17)
    (at 67 35)
    (fp_text reference J4 (at 3.75 0 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 -3) (layer F.Fab))
    (fp_text user 240V (at -7.5 3) (layer F.SilkS))
    (fp_text user LINE (at 7.5 3) (layer F.SilkS))
    (fp_text user BLUE (at 7.5 4.5) (layer F.SilkS))
    (fp_text user GRAY (at 2.5 4.5) (layer F.SilkS))
    (fp_text user 120V (at 2.5 3) (layer F.SilkS))
    (pad 6 thru_hole oval (at -30 0) (size 3 4) (drill 1.5) (layers F.Cu F.Mask))
    (pad 5 thru_hole oval (at -22.5 0) (size 3 4) (drill 1.5) (layers F.Cu F.Mask))
    (pad 4 thru_hole oval (at -15 0) (size 3 4) (drill 1.5) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 3 thru_hole oval (at 7.5 0) (size 3 4) (drill 1.5) (layers F.Cu F.Mask)
      (net 1 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 0) (size 3 4) (drill 1.5) (layers F.Cu F.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole oval (at -7.5 0) (size 3 4) (drill 1.5) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad1)"))
  )
  (module Connectors_Phoenix:PhoenixContact_MCV-G_03x3.81mm_Vertical (layer F.Cu) (tedit 59566E61)
    (at 59.5 45.5)
    (descr "Generic Phoenix Contact connector footprint for series: MCV-G; number of pins: 03; pin pitch: 3.81mm; Vertical || order number: 1803439 8A 160V")
    (tags "phoenix_contact connector MCV_01x03_G_3.81mm")
    (fp_text reference J5 (at -3.5 0 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 3.81 4) (layer F.Fab))
    (fp_text user %R (at 3.81 -3) (layer F.Fab))
    (pad 3 thru_hole oval (at 7.62 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MCV-G_03x3.81mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TPW-Connectors:01x01-d1.25mm (layer F.Cu) (tedit 65D31D1C)
    (at 72.5 43.5)
    (fp_text reference J3 (at 0 2.5) (layer F.SilkS))
    (fp_text value Line (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.5 3) (drill 1.25) (layers F.Cu F.Mask)
      (net 1 "Net-(J3-Pad1)"))
  )
  (module TPW-Connectors:01x01-d1.25mm (layer F.Cu) (tedit 65D31D24)
    (at 65.5 39.5 180)
    (fp_text reference J2 (at 2.5 0) (layer F.SilkS))
    (fp_text value 120N (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 2.5 3) (drill 1.25) (layers F.Cu F.Mask)
      (net 2 "Net-(J2-Pad1)"))
  )
  (module TPW-Connectors:01x01-d1.25mm (layer F.Cu) (tedit 65D31D29)
    (at 54 41.5)
    (fp_text reference J1 (at 0 2.5) (layer F.SilkS))
    (fp_text value 240N (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.5 3) (drill 1.25) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad1)"))
  )
  (module TPW-Decorative:High_Voltage-5mm-Silk_Screen (layer F.Cu) (tedit 65D2FD45)
    (at 48.5 39.5)
    (fp_text reference REF** (at 0 3.5) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 -2) (layer F.Fab) hide)
  )
  (gr_text 2024 (at 46 46.5) (layer F.SilkS))
  (gr_arc (start 31 32) (end 31 29.999999) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "TPW-APAREPL-XFM01 v1" (at 55 31.5) (layer F.SilkS))
  (gr_arc (start 78.5 41.5) (end 78.5 40) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 78.5 38.5) (end 78.5 40) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 75 47) (end 75 49.000001) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 33 44) (end 29 40) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 39 46) (end 41 46) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 43 47) (end 41 47) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 41 46) (end 41 47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 33 44) (end 39 44) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 28.999999 32) (end 29 40) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 78 32) (end 80 32) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 75 49.000001) (end 43 49) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 77 41.5) (end 77.000001 47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 80 32) (end 80 38.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 78 30) (end 31 29.999999) (layer Edge.Cuts) (width 0.05))
)
