(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 60)
    (zones 0)
    (modules 6)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.0381)
    (solder_mask_min_width 0.254)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 CC2)
  (net 4 CC1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CC1)
    (add_net CC2)
    (add_net GND)
    (add_net VCC)
  )
  (module misc_footprints:3DS_POWER (layer F.Cu) (tedit 5D50F14A)
    (at 113.25 70.25)
    (fp_text reference J2 (at 0 5) (layer F.SilkS))
    (fp_text value 3DS_POWER (at 0 -4.75) (layer F.Fab))
    (fp_text user + (at 5.75 0.25) (layer B.SilkS))
    (fp_text user + (at 2.25 2.25) (layer B.SilkS))
    (fp_text user + (at 5.75 0.25) (layer F.SilkS))
    (fp_text user + (at 2.25 2.25) (layer F.SilkS))
    (pad 1 thru_hole roundrect (at 6.75 1.5) (size 1.5 2) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 thru_hole roundrect (at 4.25 3) (size 1.5 2) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 thru_hole roundrect (at -4.25 3) (size 1.5 2) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 1 3) (size 1.35 2) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 2 thru_hole roundrect (at -1 3) (size 1.35 2) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 thru_hole roundrect (at -6.75 1.5) (size 1.5 2) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
  )
  (module TestPoint:TestPoint_THTPad_1.5x1.5mm_Drill0.7mm (layer F.Cu) (tedit 5D50E49E)
    (at 106.5 67.5)
    (descr "THT rectangular pad as test Point, square 1.5mm side length, hole diameter 0.7mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference VCC (at 0 -1.648) (layer F.SilkS) hide)
    (fp_text value VCC (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module misc_footprints:TYPEC31M17 (layer F.Cu) (tedit 5D562C7D)
    (at 113.25 68.75 180)
    (descr TYPE-C-31-M-17-1)
    (tags Connector)
    (fp_text reference J1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value TYPE-C-31-M-17 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad MH4 thru_hole circle (at -4.32 -2.35 180) (size 2 2) (drill 1.346) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad MH3 thru_hole circle (at 4.32 -2.35 180) (size 2 2) (drill 1.346) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad MH2 thru_hole circle (at 4.32 1.45 180) (size 2 2) (drill 1.346) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad MH1 thru_hole circle (at -4.32 1.45 180) (size 2 2) (drill 1.346) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B12 smd rect (at -2.75 -2.5 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B9 smd rect (at -1.52 -2.5 180) (size 0.76 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad B5 smd rect (at 0.5 -2.5 180) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 CC2))
    (pad A12 smd rect (at 2.75 -2.5 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 1.52 -2.5 180) (size 0.76 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad A5 smd rect (at -0.5 -2.5 180) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 CC1))
    (model TYPE-C-31-M-17.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5D562C72)
    (at 119.25 69.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 CC1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5D562C78)
    (at 107.125 69.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 CC2))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_THTPad_1.5x1.5mm_Drill0.7mm (layer F.Cu) (tedit 5D50E4A6)
    (at 120 67.5)
    (descr "THT rectangular pad as test Point, square 1.5mm side length, hole diameter 0.7mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference VCC (at 0 -1.648) (layer F.SilkS) hide)
    (fp_text value VCC (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 VCC))
  )
  (gr_text makho (at 113.25 71) (layer B.SilkS))
  (gr_line (start 105.75 70.75) (end 105.75 66.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106.5 71.75) (end 105.75 70.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 109 73.25) (end 106.5 71.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 117.5 73.25) (end 109 73.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 120 71.75) (end 117.5 73.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 120.75 70.75) (end 120 71.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 120.75 66.75) (end 120.75 70.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 105.75 66.75) (end 120.75 66.75) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.5 66.25) (xy 121 66.25) (xy 121 74.25) (xy 105.5 74.25)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.5 66.25) (xy 121 66.25) (xy 121 74.25) (xy 105.5 74.25)
      )
    )
  )
)
