<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0.3175" x2="36.5" y2="0.3175" width="0" layer="20"/>
<wire x1="36.5" y1="0.3175" x2="36.5" y2="46.0275" width="0" layer="20"/>
<wire x1="36.5" y1="46.0275" x2="0" y2="46.0275" width="0" layer="20"/>
<wire x1="0" y1="46.0275" x2="0" y2="0.3175" width="0" layer="20"/>
<text>WS Rev 0.1
by SHAFQAT</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="USB-MINIB">
<description>Surface Mount USB Mini-B Connector</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="smd-special">
<description>&lt;b&gt;Special SMD Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMS-001">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE07">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
<package name="FE08">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML1206">
<description>&lt;b&gt;SML10XXKH-TR (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;SML10R3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10E3KH-TR&lt;/td&gt;&lt;td&gt;SUPER REDSUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10O3KH-TR&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PY3KH-TR&lt;/td&gt;&lt;td&gt;PURE YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10OY3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10AG3KH-TR&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10BG3KH-TR&lt;/td&gt;&lt;td&gt;BLUE GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PB1KH-TR&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10CW1KH-TR&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;

Source: http://www.ledtronics.com/ds/smd-1206/dstr0094.PDF</description>
</package>
</packages>
</library>
<library name="RHT03_DHT-22_AM2302">
<description>&lt;h1&gt;RHT03 / DHT-22 / AM2302 library&lt;/h1&gt;
&lt;p&gt;
Library with devices (schematic symbol and packages) for the RHT03 / DHT-22 / AM2302 digital relative humidity and tempearture sensor.&lt;br /&gt;
Warning: Package does not include tKeepout areas so that the part may optionally be placed on a riser with components underneath.  Please keep the package outline and bent-pin space in mind.
&lt;/p&gt;</description>
<packages>
<package name="AM2302">
<description>&lt;h1&gt;AM2302&lt;/h1&gt;
&lt;p&gt;
Package for the AM2302 wired variant of the RHT03/DHT-22 relative humidity and temperature sensor.
&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="adafruit" package="TQFP32-08" value="AT90USB162A"/>
<element name="R8" library="adafruit" package="R1206" value="22">
<attribute name="NAME"/>
</element>
<element name="R7" library="adafruit" package="R1206" value="22">
<attribute name="NAME"/>
</element>
<element name="CN1" library="adafruit" package="USB-MINIB" value=""/>
<element name="C1" library="eagle-ltspice" package="C1206" value="1uF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C4" library="eagle-ltspice" package="C1206" value="22pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="eagle-ltspice" package="C1206" value="22pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="Q1" library="crystal" package="HC49/S" value="8MHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="adafruit" package="R1206" value="14k">
<attribute name="NAME"/>
</element>
<element name="R6" library="adafruit" package="R1206" value="330">
<attribute name="NAME"/>
</element>
<element name="C3" library="eagle-ltspice" package="C1206" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="S1" library="smd-special" package="SMS-001" value="SWS001">
<attribute name="NAME"/>
</element>
<element name="R11" library="adafruit" package="R1206" value="14K">
<attribute name="NAME"/>
</element>
<element name="R12" library="adafruit" package="R1206" value="330">
<attribute name="NAME"/>
</element>
<element name="C2" library="eagle-ltspice" package="C1206" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="S2" library="smd-special" package="SMS-001" value="SWS001">
<attribute name="NAME"/>
</element>
<element name="SV2" library="con-lsta" package="FE07" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-lsta" package="FE08" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="SML1206" value="Green">
<attribute name="NAME"/>
</element>
<element name="LED2" library="led" package="SML1206" value="Green">
<attribute name="NAME"/>
</element>
<element name="LED3" library="led" package="SML1206" value="Green">
<attribute name="NAME"/>
</element>
<element name="LED4" library="led" package="SML1206" value="Green">
<attribute name="NAME"/>
</element>
<element name="LED5" library="led" package="SML1206" value="Red">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit" package="R1206" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R9" library="adafruit" package="R1206" value="330">
<attribute name="NAME"/>
</element>
<element name="R10" library="adafruit" package="R1206" value="330">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="R1206" value="330">
<attribute name="NAME"/>
</element>
<element name="R2" library="adafruit" package="R1206" value="330">
<attribute name="NAME"/>
</element>
<element name="R4" library="adafruit" package="R1206" value="330">
<attribute name="NAME"/>
</element>
<element name="C6" library="eagle-ltspice" package="C1206" value="10uF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="RHT03_DHT-22_AM2302" package="AM2302" value="">
<attribute name="PROD_ID" value="SEN-10167"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="32"/>
<contactref element="IC1" pad="31"/>
<contactref element="R5" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="VDD"/>
</signal>
<signal name="N$1">
<contactref element="R8" pad="2"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="N$2">
<contactref element="R7" pad="2"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="N$3">
<contactref element="R8" pad="1"/>
<contactref element="CN1" pad="D+"/>
</signal>
<signal name="N$4">
<contactref element="CN1" pad="D-"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="GND">
<contactref element="CN1" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="28"/>
<contactref element="IC1" pad="3"/>
<contactref element="S1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED5" pad="C"/>
<contactref element="U1" pad="GND"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="27"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C4" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C5" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R6" pad="1"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="N$9">
<contactref element="R11" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R12" pad="1"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="6"/>
<contactref element="SV2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="7"/>
<contactref element="SV2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="8"/>
<contactref element="SV2" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="9"/>
<contactref element="SV2" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="10"/>
<contactref element="SV2" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="11"/>
<contactref element="SV2" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="12"/>
<contactref element="SV2" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="14"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="15"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="IC1" pad="16"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="IC1" pad="17"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="IC1" pad="18"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="N$24">
<contactref element="IC1" pad="19"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="N$25">
<contactref element="IC1" pad="20"/>
<contactref element="SV1" pad="7"/>
</signal>
<signal name="N$26">
<contactref element="IC1" pad="21"/>
<contactref element="SV1" pad="8"/>
</signal>
<signal name="N$27">
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="U1" pad="DATA"/>
</signal>
<signal name="N$28">
<contactref element="IC1" pad="26"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="IC1" pad="25"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="IC1" pad="23"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="IC1" pad="22"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="R9" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$33">
<contactref element="R10" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$34">
<contactref element="R1" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$35">
<contactref element="R2" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$37">
<contactref element="LED5" pad="A"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="CN1" pad="VBUS"/>
<contactref element="C6" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
