(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.2)
  )
  (paper "USLetter")
  (title_block
    (title "WP-2_IC-Card")
    (date "2023-01-03")
    (rev "Breakout_005")
    (company "Brian K. White - b.kenyon.w@gmail.com")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (33 "F.Adhes" user "F.Adhesive")
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.11) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (aux_axis_origin 139.7 101.045)
    (grid_origin 139.7 101.045)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_${TITLE}_${REVISION}")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/~{CE1}")
  (net 3 "/~{OE}")
  (net 4 "/D0")
  (net 5 "/D1")
  (net 6 "/D2")
  (net 7 "/D3")
  (net 8 "/D4")
  (net 9 "/D5")
  (net 10 "/D6")
  (net 11 "/D7")
  (net 12 "/A16")
  (net 13 "/A15")
  (net 14 "/A14")
  (net 15 "/A13")
  (net 16 "/A12")
  (net 17 "/A11")
  (net 18 "/A10")
  (net 19 "/A9")
  (net 20 "/A8")
  (net 21 "/A7")
  (net 22 "/A6")
  (net 23 "/A5")
  (net 24 "/A4")
  (net 25 "/A3")
  (net 26 "/A2")
  (net 27 "/A1")
  (net 28 "/A0")
  (net 29 "/A17")
  (net 30 "/R~{W}")
  (net 31 "/~{DET}")
  (net 32 "/S1")
  (net 33 "/S2")
  (net 34 "/S3")
  (net 35 "/BCHK")
  (net 36 "/CE2")
  (net 37 "VBUS")
  (footprint "0_LOCAL:SMS-138-01-x-x_edge" (layer "F.Cu")
    (tedit 5F7AC44E)
    (at 139.7 119.52 -90)
    (descr "Through hole straight socket strip, 1x38, 1.27mm pitch, single row")
    (tags "Through hole socket strip THT 1x38 1.27mm single row")
    (property "Sheetfile" "WP-2_IC_Card_Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -2.286 -24.892 -90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x38_Female" (at -4.491 -0.381 -180) (layer "F.Fab"))
    (fp_text user "max insertion 6.3mm" (at 4.3 -22.6 -90 unlocked) (layer "Dwgs.User"))
    (fp_text user "8.51mm" (at 4.14 -24.79 -90 unlocked) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at -2.286 -24.892 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 -23.495 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -1.4 -22.225 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/~{DET}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -1.4 -20.955 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/CE2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at -1.4 -19.685 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/~{CE1}") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at -1.4 -18.415 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/~{OE}") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at -1.4 -17.145 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/D0") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd roundrect (at -1.4 -15.875 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/D1") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd roundrect (at -1.4 -14.605 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/D2") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd roundrect (at -1.4 -13.335 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/D3") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd roundrect (at -1.4 -12.065 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/D4") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd roundrect (at -1.4 -10.795 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/D5") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd roundrect (at -1.4 -9.525 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/D6") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd roundrect (at -1.4 -8.255 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/D7") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd roundrect (at -1.4 -6.985 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd roundrect (at -1.4 -5.715 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/S1") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd roundrect (at -1.4 -4.445 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/S2") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd roundrect (at -1.4 -3.175 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/A17") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd roundrect (at -1.4 -1.905 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/A16") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd roundrect (at -1.4 -0.635 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/A15") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd roundrect (at -1.4 0.635 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/A14") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd roundrect (at -1.4 1.905 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/A13") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd roundrect (at -1.4 3.175 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/A12") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd roundrect (at -1.4 4.445 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/A11") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd roundrect (at -1.4 5.715 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/A10") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd roundrect (at -1.4 6.985 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/A9") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd roundrect (at -1.4 8.255 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/A8") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd roundrect (at -1.4 9.525 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/A7") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd roundrect (at -1.4 10.795 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/A6") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd roundrect (at -1.4 12.065 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/A5") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd roundrect (at -1.4 13.335 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/A4") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd roundrect (at -1.4 14.605 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/A3") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd roundrect (at -1.4 15.875 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/A2") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd roundrect (at -1.4 17.145 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/A1") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd roundrect (at -1.4 18.415 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/A0") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd roundrect (at -1.4 19.685 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/R~{W}") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd roundrect (at -1.4 20.955 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/S3") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd roundrect (at -1.4 22.225 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/BCHK") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd roundrect (at -1.4 23.495 270) (size 2.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "VBUS") (pinfunction "Pin_38") (pintype "passive"))
    (model "${KIPRJMOD}/3d/SMS-138-01-x-x.step"
      (offset (xyz 0 0 0.204))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "0_LOCAL:PinHeader_2x19_P2.54mm" (layer "F.Cu")
    (tedit 60661EE4)
    (at 162.56 81.42 -90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "WP-2_IC_Card_Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -2.33 -90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x19_Odd_Even" (at 1.27 48.514 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 24.13) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 31 "/~{DET}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 36 "/CE2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 2.54 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 2 "/~{CE1}") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 5.08 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 3 "/~{OE}") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 5.08 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 4 "/D0") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 5 "/D1") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 7.62 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 6 "/D2") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 10.16 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 7 "/D3") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 10.16 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 8 "/D4") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 12.7 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 9 "/D5") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 2.54 12.7 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 10 "/D6") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 15.24 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 11 "/D7") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 2.54 15.24 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at 0 17.78 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 32 "/S1") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at 2.54 17.78 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 33 "/S2") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at 0 20.32 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 29 "/A17") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at 2.54 20.32 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 12 "/A16") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at 0 22.86 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 13 "/A15") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 2.54 22.86 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 14 "/A14") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole circle (at 0 25.4 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 15 "/A13") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole circle (at 2.54 25.4 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 16 "/A12") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole circle (at 0 27.94 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 17 "/A11") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole circle (at 2.54 27.94 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 18 "/A10") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole circle (at 0 30.48 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 19 "/A9") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole circle (at 2.54 30.48 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 20 "/A8") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole circle (at 0 33.02 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 21 "/A7") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole circle (at 2.54 33.02 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 22 "/A6") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole circle (at 0 35.56 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 23 "/A5") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole circle (at 2.54 35.56 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 24 "/A4") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole circle (at 0 38.1 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 25 "/A3") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole circle (at 2.54 38.1 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 26 "/A2") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole circle (at 0 40.64 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 27 "/A1") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole circle (at 2.54 40.64 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 28 "/A0") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole circle (at 0 43.18 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 30 "/R~{W}") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole circle (at 2.54 43.18 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 34 "/S3") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole circle (at 0 45.72 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 35 "/BCHK") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole circle (at 2.54 45.72 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 37 "VBUS") (pinfunction "Pin_38") (pintype "passive"))
    (model "${KIPRJMOD}/3d/IDC-Header_2x19_P2.54mm_Vertical.step" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3d/PinHeader_2x19_P2.54mm_Vertical.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:npth_0.6mm" (layer "F.Cu")
    (tedit 5F75C0E6)
    (at 163.7 119.82)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 4.445) (layer "F.SilkS") hide)
    (fp_text value "npth_0.6mm" (at 0 -1) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.6) (layers F&B.Cu)
      (zone_connect 0))
  )
  (footprint "0_LOCAL:npth_0.6mm" (layer "F.Cu")
    (tedit 5F75C0E6)
    (at 115.7 119.82)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 4.445) (layer "F.SilkS") hide)
    (fp_text value "npth_0.6mm" (at 0 -1) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.6) (layers F&B.Cu)
      (zone_connect 0))
  )
  (footprint "0_LOCAL:WP-2_IC_Card_Cover_Breakout" (layer "F.Cu")
    (tedit 0)
    (at 139.7 101.045)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.Fab") hide)
    (fp_text value "WP-2_IC_Card_Cover_Breakout" (at 0 0 unlocked) (layer "F.Fab"))
    (model "${KIPRJMOD}/3d/WP-2_IC-Card_Cover_Breakout.step"
      (offset (xyz 0 0 1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 180))
    )
  )
  (gr_line (start 164 128.045) (end 164 119.52) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 112.7 76.045) (mid 113.285786 74.630786) (end 114.7 74.045) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 166.7 126.045) (mid 166.114214 127.459214) (end 164.7 128.045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 164.7 128.045) (end 164 128.045) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 113.285786 77.459214) (mid 112.85224 76.810367) (end 112.7 76.045) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 112.699999 94.045) (mid 112.85224 93.279633) (end 113.285786 92.630786) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 113.285786 77.459214) (mid 113.719307 78.108067) (end 113.871572 78.873428) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 113.871573 91.216572) (mid 113.719334 91.981938) (end 113.285786 92.630786) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 113.871573 91.216572) (end 113.871572 78.873428) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 166.114214 92.630786) (mid 166.54776 93.279633) (end 166.7 94.045) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 165.528427 78.873428) (mid 165.680666 78.108062) (end 166.114214 77.459214) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 166.114214 92.630786) (mid 165.680693 91.981933) (end 165.528428 91.216572) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 166.700001 76.045) (mid 166.54776 76.810367) (end 166.114214 77.459214) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 165.528427 78.873428) (end 165.528428 91.216572) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 164.7 74.045) (mid 166.114214 74.630786) (end 166.7 76.045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 115.4 119.52) (end 115.4 128.045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 166.7 94.045) (end 166.7 126.045) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 113.2 118.545) (mid 113.553553 118.691447) (end 113.7 119.045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 115.4 128.045) (end 114.2 128.045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 164 119.52) (end 115.4 119.52) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 114.2 128.045) (mid 113.846447 127.898553) (end 113.7 127.545) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 113.7 127.545) (end 113.7 119.045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 112.7 118.045) (end 112.699999 94.045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 114.7 74.045) (end 164.7 74.045) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 113.2 118.545) (mid 112.846447 118.398553) (end 112.7 118.045) (layer "Edge.Cuts") (width 0.05))
  (gr_text "github.com/bkw777/WP-2_IC_Card" (at 139.7 112.06) (layer "B.SilkS"))
  (gr_text "1" (at 162.2 116.795 -90) (layer "B.SilkS"))
  (gr_text "Connector: Samtec SMS-138-01-G-S" (at 139.7 118.41) (layer "B.SilkS"))
  (gr_text "S3" (at 119.38 86.5 270) (layer "B.SilkS"))
  (gr_text "D1" (at 154.94 78.88 270) (layer "B.SilkS"))
  (gr_text "A3" (at 124.46 78.88 270) (layer "B.SilkS"))
  (gr_text "D0" (at 157.48 86.5 270) (layer "B.SilkS"))
  (gr_text "A6" (at 129.54 86.5 270) (layer "B.SilkS"))
  (gr_text "D2" (at 154.94 86.5 270) (layer "B.SilkS"))
  (gr_text "A4" (at 127 86.5 270) (layer "B.SilkS"))
  (gr_text "A2" (at 124.46 86.5 270) (layer "B.SilkS"))
  (gr_text "CE2" (at 160.02 78.88 270) (layer "B.SilkS"))
  (gr_text "2" (at 164.465 83.96 270) (layer "B.SilkS"))
  (gr_text "WP-2_IC_Card_Breakout v004" (at 139.7 110.155) (layer "B.SilkS"))
  (gr_text "A10" (at 134.62 86.5 270) (layer "B.SilkS"))
  (gr_text "A8" (at 132.08 86.5 270) (layer "B.SilkS"))
  (gr_text "S1" (at 144.78 78.88 270) (layer "B.SilkS"))
  (gr_text "38" (at 116.95 116.795 -90) (layer "B.SilkS"))
  (gr_text "S2" (at 144.78 86.5 270) (layer "B.SilkS"))
  (gr_text "~{DET}" (at 162.56 86.5 270) (layer "B.SilkS"))
  (gr_text "A5" (at 127 78.88 270) (layer "B.SilkS"))
  (gr_text "GND" (at 147.32 86.5 270) (layer "B.SilkS"))
  (gr_text "D5" (at 149.86 78.88 270) (layer "B.SilkS"))
  (gr_text "D4" (at 152.4 86.5 270) (layer "B.SilkS"))
  (gr_text "A1" (at 121.92 78.88 270) (layer "B.SilkS"))
  (gr_text "1" (at 164.465 81.42 270) (layer "B.SilkS"))
  (gr_text "37" (at 114.935 81.42 270) (layer "B.SilkS"))
  (gr_text "THIS SIDE DOWN" (at 139.7 103.045) (layer "B.SilkS"))
  (gr_text "D7" (at 147.32 78.88 270) (layer "B.SilkS"))
  (gr_text "A16" (at 142.24 86.5 270) (layer "B.SilkS"))
  (gr_text "A9" (at 132.08 78.88 270) (layer "B.SilkS"))
  (gr_text "A7" (at 129.54 78.88 270) (layer "B.SilkS"))
  (gr_text "D6" (at 149.86 86.5 270) (layer "B.SilkS"))
  (gr_text "~{CE1}" (at 160.02 86.5 270) (layer "B.SilkS"))
  (gr_text "GND" (at 162.56 78.88 270) (layer "B.SilkS"))
  (gr_text "A0" (at 121.92 86.5 270) (layer "B.SilkS"))
  (gr_text "VBUS" (at 116.84 86.5 270) (layer "B.SilkS"))
  (gr_text "A13" (at 137.16 78.88 270) (layer "B.SilkS"))
  (gr_text "D3" (at 152.4 78.88 270) (layer "B.SilkS"))
  (gr_text "38" (at 114.935 83.96 270) (layer "B.SilkS"))
  (gr_text "A15" (at 139.7 78.88 270) (layer "B.SilkS"))
  (gr_text "A11" (at 134.62 78.88 270) (layer "B.SilkS"))
  (gr_text "R~{W}" (at 119.38 78.88 270) (layer "B.SilkS"))
  (gr_text "A17" (at 142.24 78.88 270) (layer "B.SilkS"))
  (gr_text "A14" (at 139.7 86.5 270) (layer "B.SilkS"))
  (gr_text "~{OE}" (at 157.48 78.88 270) (layer "B.SilkS"))
  (gr_text "A12" (at 137.16 86.5 270) (layer "B.SilkS"))
  (gr_text "BCHK" (at 116.84 78.88 270) (layer "B.SilkS"))
  (gr_text "1" (at 162.2 114.795 -90) (layer "F.SilkS"))
  (gr_text "38" (at 116.95 113.795 -90) (layer "F.SilkS"))
  (gr_text "D0" (at 157.48 86.5 -90) (layer "F.SilkS"))
  (gr_text "D2" (at 154.94 86.5 -90) (layer "F.SilkS"))
  (gr_text "D4" (at 152.4 86.5 -90) (layer "F.SilkS"))
  (gr_text "D6" (at 149.86 86.5 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 147.32 86.5 -90) (layer "F.SilkS"))
  (gr_text "S2" (at 144.78 86.5 -90) (layer "F.SilkS"))
  (gr_text "A16" (at 142.24 86.5 -90) (layer "F.SilkS"))
  (gr_text "A14" (at 139.7 86.5 -90) (layer "F.SilkS"))
  (gr_text "A12" (at 137.16 86.5 -90) (layer "F.SilkS"))
  (gr_text "A10" (at 134.62 86.5 -90) (layer "F.SilkS"))
  (gr_text "A8" (at 132.08 86.5 -90) (layer "F.SilkS"))
  (gr_text "A6" (at 129.54 86.5 -90) (layer "F.SilkS"))
  (gr_text "A4" (at 127 86.5 -90) (layer "F.SilkS"))
  (gr_text "A2" (at 124.46 86.5 -90) (layer "F.SilkS"))
  (gr_text "A0" (at 121.92 86.5 -90) (layer "F.SilkS"))
  (gr_text "S3" (at 119.38 86.5 -90) (layer "F.SilkS"))
  (gr_text "VBUS" (at 116.84 86.5 -90) (layer "F.SilkS"))
  (gr_text "R~{W}" (at 119.38 78.88 -90) (layer "F.SilkS"))
  (gr_text "A1" (at 121.92 78.88 -90) (layer "F.SilkS"))
  (gr_text "A3" (at 124.46 78.88 -90) (layer "F.SilkS"))
  (gr_text "A5" (at 127 78.88 -90) (layer "F.SilkS"))
  (gr_text "A7" (at 129.54 78.88 -90) (layer "F.SilkS"))
  (gr_text "A9" (at 132.08 78.88 -90) (layer "F.SilkS"))
  (gr_text "A11" (at 134.62 78.88 -90) (layer "F.SilkS"))
  (gr_text "A13" (at 137.16 78.88 -90) (layer "F.SilkS"))
  (gr_text "A15" (at 139.7 78.88 -90) (layer "F.SilkS"))
  (gr_text "A17" (at 142.24 78.88 -90) (layer "F.SilkS"))
  (gr_text "S1" (at 144.78 78.88 -90) (layer "F.SilkS"))
  (gr_text "D7" (at 147.32 78.88 -90) (layer "F.SilkS"))
  (gr_text "D5" (at 149.86 78.88 -90) (layer "F.SilkS"))
  (gr_text "D3" (at 152.4 78.88 -90) (layer "F.SilkS"))
  (gr_text "D1" (at 154.94 78.88 -90) (layer "F.SilkS"))
  (gr_text "~{OE}" (at 157.48 78.88 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 162.56 78.88 -90) (layer "F.SilkS"))
  (gr_text "BCHK" (at 116.84 78.88 -90) (layer "F.SilkS"))
  (gr_text "CE2" (at 160.02 78.88 -90) (layer "F.SilkS"))
  (gr_text "TANDY WP-2 IC-Card Breakout" (at 139.7 99.835) (layer "F.SilkS"))
  (gr_text "~{CE1}" (at 160.02 86.5 -90) (layer "F.SilkS"))
  (gr_text "38" (at 114.681 83.96 -90) (layer "F.SilkS"))
  (gr_text "37" (at 114.681 81.42 -90) (layer "F.SilkS"))
  (gr_text "2" (at 164.592 83.96 -90) (layer "F.SilkS"))
  (gr_text "~{DET}" (at 162.56 86.5 -90) (layer "F.SilkS"))
  (gr_text "1" (at 164.592 81.42 -90) (layer "F.SilkS"))
  (gr_text "PCB thickness 1.2mm" (at 139.7 131.745) (layer "Dwgs.User"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 112.7 128.045)
        (xy 112.7 74.045)
        (xy 166.7 74.045)
        (xy 166.7 128.045)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 112.7 128.045)
        (xy 112.7 74.045)
        (xy 166.7 74.045)
        (xy 166.7 128.045)
      )
    )
  )
)
