(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 142)
    (tracks 237)
    (zones 0)
    (modules 5)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2032)
    (trace_clearance 0.2)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.8128 0.4064)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad4)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad6)")
  (net 6 "Net-(J1-Pad5)")
  (net 7 "Net-(J1-Pad8)")
  (net 8 "Net-(J1-Pad7)")
  (net 9 "Net-(J1-Pad10)")
  (net 10 "Net-(J1-Pad9)")
  (net 11 "Net-(J1-Pad12)")
  (net 12 "Net-(J1-Pad11)")
  (net 13 "Net-(J1-Pad14)")
  (net 14 "Net-(J1-Pad13)")
  (net 15 "Net-(J1-Pad16)")
  (net 16 "Net-(J1-Pad15)")
  (net 17 "Net-(J1-Pad18)")
  (net 18 "Net-(J1-Pad17)")
  (net 19 "Net-(J1-Pad20)")
  (net 20 "Net-(J1-Pad19)")
  (net 21 "Net-(J2-Pad4)")
  (net 22 "Net-(J2-Pad3)")
  (net 23 "Net-(J2-Pad2)")
  (net 24 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 6000766F)
    (at 148.971 88.519)
    (fp_text reference REF** (at -2.032 0.127) (layer F.SilkS) hide)
    (fp_text value TP (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad20)"))
  )
  (module t_logos:Thales_15x2_Cu (layer F.Cu) (tedit 0)
    (at 139.192 72.5805)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "t_connectors:FH12A-24S-0.5SH(55)_flex_connector" (layer F.Cu) (tedit 600073E6)
    (at 128.3462 74.8284 90)
    (attr smd)
    (fp_text reference J2 (at -4.3688 1.8542 90) (layer F.SilkS))
    (fp_text value "Conn_FH12A-24S-0.5SH(55)" (at -4.6482 3.3782 90) (layer F.Fab))
    (pad 25 smd rect (at 2.4384 -3.3528 90) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad20)"))
    (pad 26 smd rect (at -13.4112 -3.302 90) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad20)"))
    (pad 24 smd oval (at -11.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 23 smd oval (at -10.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 22 smd oval (at -10.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 21 smd oval (at -9.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 20 smd oval (at -9.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 19 smd oval (at -8.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad6)"))
    (pad 18 smd oval (at -8.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad7)"))
    (pad 17 smd oval (at -7.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 16 smd oval (at -7.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad9)"))
    (pad 15 smd oval (at -6.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad10)"))
    (pad 14 smd oval (at -6.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad11)"))
    (pad 13 smd oval (at -5.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad12)"))
    (pad 12 smd oval (at -5.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad13)"))
    (pad 11 smd oval (at -4.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad14)"))
    (pad 10 smd oval (at -4.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad15)"))
    (pad 9 smd oval (at -3.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad16)"))
    (pad 8 smd oval (at -3.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad17)"))
    (pad 7 smd oval (at -2.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad18)"))
    (pad 6 smd oval (at -2.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad19)"))
    (pad 5 smd oval (at -1.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad20)"))
    (pad 4 smd oval (at -1.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad4)"))
    (pad 3 smd oval (at -0.7364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J2-Pad3)"))
    (pad 2 smd oval (at -0.2364 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at 0.2636 0 90) (size 0.3 1.32) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J2-Pad1)"))
    (model ${T_LIBS}/3d/t_connectors/FH12A-24S-0.5SH.stp
      (offset (xyz -26 22 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 143.0274 88.3666)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad_TopBottom (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers B.Cu B.Mask))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers F.Cu F.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module t_connectors:AXK6S20447Y_header (layer B.Cu) (tedit 600043C6)
    (at 148.0312 79.9592 180)
    (attr smd)
    (fp_text reference J1 (at -0.381 -4.7752) (layer B.SilkS))
    (fp_text value AXK6S20447Y_header (at 0 0) (layer B.Fab))
    (pad 2 smd oval (at 2.54 -2 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at 2.5146 1.9812 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 4 smd oval (at 1.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 3 smd oval (at 1.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 6 smd oval (at 1.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad6)"))
    (pad 5 smd oval (at 1.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 8 smd oval (at 0.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 7 smd oval (at 0.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad7)"))
    (pad 10 smd oval (at 0.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad10)"))
    (pad 9 smd oval (at 0.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J1-Pad9)"))
    (pad 12 smd oval (at -0.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J1-Pad12)"))
    (pad 11 smd oval (at -0.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J1-Pad11)"))
    (pad 14 smd oval (at -0.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J1-Pad14)"))
    (pad 13 smd oval (at -0.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J1-Pad13)"))
    (pad 16 smd oval (at -1.25 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J1-Pad16)"))
    (pad 15 smd oval (at -1.25 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J1-Pad15)"))
    (pad 18 smd oval (at -1.75 -2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J1-Pad18)"))
    (pad 17 smd oval (at -1.75 2 180) (size 0.25 2) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J1-Pad17)"))
    (pad 20 smd oval (at -2.5146 -2.032 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J1-Pad20)"))
    (pad 19 smd oval (at -2.5146 1.9812 180) (size 0.75 2) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J1-Pad19)"))
  )
  (gr_text GND (at 148.717 86.6775) (layer F.SilkS))
  (gr_text "Javelin \nKeyboard Adapter" (at 138.557 75.692) (layer F.SilkS))
  (gr_text "Jan 2021" (at 133.5405 88.8365) (layer F.SilkS))
  (gr_text SK1599 (at 133.5405 87.1855) (layer F.SilkS))
  (gr_line (start 120.65 91.44) (end 153.67 91.44) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.65 70.485) (end 120.65 91.44) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.67 70.485) (end 120.65 70.485) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.67 91.44) (end 153.67 70.485) (layer Edge.Cuts) (width 0.05))
  (zone (net 19) (net_name "Net-(J1-Pad20)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.035 90.805) (xy 121.285 90.805) (xy 121.285 71.12) (xy 153.035 71.12)
      )
    )
  )
  (zone (net 19) (net_name "Net-(J1-Pad20)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.035 90.782279) (xy 121.285 90.782279) (xy 121.285 71.097279) (xy 153.035 71.097279)
      )
    )
  )
)
