(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(BT1-+)")
	(net 3 "Net-(D1-A)")
	(net 4 "Net-(SC1-+)")
	(footprint "Connector_Wire:SolderWire-1sqmm_1x02_P5.4mm_D1.4mm_OD2.7mm"
		(layer "F.Cu")
		(at 156.15 91.6 180)
		(descr "Soldered wire connection, for 2 times 1 mm² wires, basic insulation, conductor diameter 1.4mm, outer diameter 2.7mm, size source Multi-Contact FLEXI-E 1.0 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 1sqmm")
		(property "Reference" "D1"
			(at 2.7 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 2.7 2.58 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-1sqmm_1x02_P5.4mm_D1.4mm_OD2.7mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Untitled Field" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Solar-Garden-light-YX805.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 2.7 0 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2.75 2.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.090909)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.4 0 180)
			(size 2.75 2.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1sqmm_1x02_P5.4mm_D1.4mm_OD2.7mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-1sqmm_1x02_P5.4mm_D1.4mm_OD2.7mm"
		(layer "F.Cu")
		(at 150.75 87.55)
		(descr "Soldered wire connection, for 2 times 1 mm² wires, basic insulation, conductor diameter 1.4mm, outer diameter 2.7mm, size source Multi-Contact FLEXI-E 1.0 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 1sqmm")
		(property "Reference" "SC1"
			(at 2.7 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Solar_Cell"
			(at 2.7 2.58 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-1sqmm_1x02_P5.4mm_D1.4mm_OD2.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single solar cell"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Untitled Field" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Solar-Garden-light-YX805.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 2.7 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.75 2.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.090909)
			(net 4 "Net-(SC1-+)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.4 0)
			(size 2.75 2.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1sqmm_1x02_P5.4mm_D1.4mm_OD2.7mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-1sqmm_1x02_P5.4mm_D1.4mm_OD2.7mm"
		(layer "F.Cu")
		(at 150.75 83.5)
		(descr "Soldered wire connection, for 2 times 1 mm² wires, basic insulation, conductor diameter 1.4mm, outer diameter 2.7mm, size source Multi-Contact FLEXI-E 1.0 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 1sqmm")
		(property "Reference" "BT1"
			(at 2.7 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Battery_Cell"
			(at 2.7 2.58 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-1sqmm_1x02_P5.4mm_D1.4mm_OD2.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single-cell battery"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Untitled Field" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Solar-Garden-light-YX805.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 2.7 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.75 2.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.090909)
			(net 2 "Net-(BT1-+)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.4 0)
			(size 2.75 2.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-1sqmm_1x02_P5.4mm_D1.4mm_OD2.7mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "+++Sherms-kicad5-libs:YX805-A"
		(layer "F.Cu")
		(at 150.825 79.885)
		(property "Reference" "YX805"
			(at 2.475 -1.335 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 1 4.75 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "+++Sherms-kicad5-libs:YX805-A"
			(at 1 3.75 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Untitled Field" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Solar-Garden-light-YX805.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0.25)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(SC1-+)")
			(pinfunction "Sol")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 1.75 0.25)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(BT1-+)")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 3.5 0.25)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 5.25 0.25)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-A)")
			(pinfunction "Light")
			(pintype "output")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical"
		(layer "F.Cu")
		(at 155.765 76.45 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=5.08mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 5.08mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "L1"
			(at 2.815 0.8 180)
			(layer "F.SilkS")
		)
		(property "Value" "L"
			(at 2.54 2.37 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Untitled Field" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "Solar-Garden-light-YX805.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -2.37 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(BT1-+)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 148.3 74.7)
		(end 158.55 93.75)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "Sherm Stebbins\nSolar Garden\nV1"
		(at 155.5 80.8 90)
		(layer "B.SilkS")
	)
	(gr_text "-"
		(at 156.9 85.15 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 148.95 80.5 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 156.9 89.3 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 151.65 89.75 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 151.55 93.35 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 156.95 93.65 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 151.7 85.7 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 148.05 74.5) (xy 147.9 94.35) (xy 159.45 94.35) (xy 159.3 74.2)
			)
		)
	)
)
