(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./")
    )
  )
  (net 0 "")
  (net 1 "Net-(BT1-+)")
  (net 2 "Net-(BT1--)")
  (net 3 "Net-(BT2-+)")
  (net 4 "Net-(BT3-+)")
  (net 5 "Net-(PA1616S1-VCC)")
  (net 6 "Net-(SW1A-B)")
  (net 7 "unconnected-(PA1616S1-Reset-Pad2)")
  (net 8 "Net-(PA1616S1-TX0)")
  (net 9 "Net-(PA1616S1-RX0)")
  (net 10 "Net-(XBee900HP1-Data_In)")
  (net 11 "Net-(XBee900HP1-Data_Out)")
  (net 12 "Net-(D2-A)")
  (net 13 "Net-(D1-K)")
  (net 14 "Net-(D1-A)")
  (net 15 "Net-(D2-K)")
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 171.45 120.65)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "4-40 SCREW" (at 0 5.08) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at -12.7 1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 150.925 104.775)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "0.1 microfarad" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "Net-(BT1--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 3 "Net-(BT2-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Battery:BatteryHolder_Keystone_500" (layer "F.Cu")
    (at 156.577818 117.475 180)
    (descr "Keystone #500, 12mm CR1220 battery holder, http://www.keyelco.com/product-pdf.cfm?p=710")
    (tags "CR1220 battery holder")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr through_hole)
    (fp_text reference "BT2" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "CR1220 3V" (at 9.525 8.89) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9.525 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.54 2.54) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(BT2-+)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at 9.9822 0 180) (size 2.54 2.54) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(BT1--)") (pinfunction "-") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_500.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0805_2012Metric" (layer "F.Cu")
    (at 140.335 87.63)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D2" (at -0.635 1.905) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 153.67 96.315 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "1.0 microfarad" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 5 "Net-(PA1616S1-VCC)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "Net-(BT1--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 168.6325 112.395)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "330" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 13 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 2 "Net-(BT1--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 134.62 87.63)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0.635 1.905) (layer "F.SilkS"))
    (fp_text value "330" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 2 "Net-(BT1--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 15 "Net-(D2-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0805_2012Metric" (layer "F.Cu")
    (at 161.29 112.395 180)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at 0 1.905) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 133.35 120.65)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "4-40 SCREW" (at 0 5.08) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 11.43 3.175) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 171.45 57.15)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "4-40 SCREW" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 142.24 103.075 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "0.1 microfarad" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "Net-(BT1--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 6 "Net-(SW1A-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 173.785 78.105)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "47 picofarad" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 12 "Net-(D2-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "Net-(BT1--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 133.35 57.15)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "4-40 SCREW" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 167.005 78.3825 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "470" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 11 "Net-(XBee900HP1-Data_Out)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 9 "Net-(PA1616S1-RX0)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 145.415 95.045 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "2.2 microfarad" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "Net-(BT1--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 12 "Net-(D2-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 163.195 78.4625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "470" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 10 "Net-(XBee900HP1-Data_In)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 8 "Net-(PA1616S1-TX0)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Adafruit:Adafruit PA1616S" (layer "F.Cu")
    (at 165.355 105.02)
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "PA1616S1" (at 0 -5.5 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 -4 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -8 -10) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(PA1616S1-VCC)") (pinfunction "VCC") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "2" smd rect (at -8 -8.5) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(PA1616S1-Reset-Pad2)") (pinfunction "Reset") (pintype "input") (thermal_bridge_angle 45))
    (pad "3" smd rect (at -8 -7) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(BT1--)") (pinfunction "GND") (pintype "power_out") (thermal_bridge_angle 45))
    (pad "4" smd rect (at -8 -5.5) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(BT2-+)") (pinfunction "VBACKUP") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "5" smd rect (at -8 -4) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(D1-A)") (pinfunction "3D_Fix") (pintype "output") (thermal_bridge_angle 45))
    (pad "6" smd rect (at -8 -2.5) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "7" smd rect (at -8 -1) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "8" smd rect (at -8 0.5) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "9" smd rect (at -8 2) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(PA1616S1-TX0)") (pinfunction "TX0") (pintype "output") (thermal_bridge_angle 45))
    (pad "10" smd rect (at -8 3.5) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(PA1616S1-RX0)") (pinfunction "RX0") (pintype "output") (thermal_bridge_angle 45))
    (pad "11" smd rect (at 8 3.5) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "12" smd rect (at 8 2) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "13" smd rect (at 8 0.5) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "14" smd rect (at 8 -1) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "15" smd rect (at 8 -2.5) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "16" smd rect (at 8 -4) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "17" smd rect (at 8 -5.5) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "18" smd rect (at 8 -7) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "19" smd rect (at 8 -8.5) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
    (pad "20" smd rect (at 8 -10) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (thermal_bridge_angle 45))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 149.86 96.315 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "0.1 microfarad" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 5 "Net-(PA1616S1-VCC)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "Net-(BT1--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 148.745 92.71)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead, small symbol")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr smd)
    (fp_text reference "FB1" (at 2.385 0) (layer "F.SilkS"))
    (fp_text value "GMLB-100505-0600A-N8-RU" (at 0.635 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D2-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(PA1616S1-VCC)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "XBee:SMD Switch - JS102011SCQN" (layer "F.Cu")
    (at 135.93 107.95 -90)
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch, separate symbol")
    (property "ki_keywords" "switch lever")
    (attr smd)
    (fp_text reference "SW1" (at 0 -0.5 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "SW_DPST_x2" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.5 3 180) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(BT3-+)") (pinfunction "A") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.5 180) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(SW1A-B)") (pinfunction "B") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 2.5 3 180) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
  )
  (footprint "XBee:XBee 900HP SMD Pins" (layer "F.Cu")
    (at 161.45 77.63 -90)
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "XBee900HP1" (at -0.16 0.795 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -12 -10 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D2-A)") (pinfunction "3.3_V") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at -10 -8 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(XBee900HP1-Data_Out)") (pinfunction "Data_Out") (pintype "output") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at -12 -6 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(XBee900HP1-Data_In)") (pinfunction "Data_In") (pintype "input") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at -10 -4 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at -12 -2 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at -10 0 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at -12 2 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at -10 4 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "9" smd roundrect (at -12 6 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "10" smd roundrect (at -10 8 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(BT1--)") (pinfunction "GND") (pintype "output") (thermal_bridge_angle 45))
    (pad "11" smd roundrect (at 12 8 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "12" smd roundrect (at 10 6 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "13" smd roundrect (at 12 4 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "14" smd roundrect (at 10 2 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "15" smd roundrect (at 12 0 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "16" smd roundrect (at 10 -2 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "17" smd roundrect (at 12 -4 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "18" smd roundrect (at 10 -6 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "19" smd roundrect (at 12 -8 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "20" smd roundrect (at 10 -10 270) (size 2.29 0.82) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "F.Cu")
    (at 136.92 95.63 180)
    (descr "TO-252/DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Positive 500mA 20V Linear Regulator, Fixed Output 3.3V, TO-252 (D-PAK)")
    (property "ki_keywords" "Voltage Regulator 500mA Positive")
    (attr smd)
    (fp_text reference "U1" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "KF33BDT" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -5.04 -2.28 180) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 6 "Net-(SW1A-B)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.415 -1.525 180) (size 3.05 2.75) (layers "F.Cu" "F.Paste") (roundrect_rratio 0.09090909091)
      (net 2 "Net-(BT1--)") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.415 1.525 180) (size 3.05 2.75) (layers "F.Cu" "F.Paste") (roundrect_rratio 0.09090909091)
      (net 2 "Net-(BT1--)") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at 1.26 0 180) (size 6.4 5.8) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.04310293103)
      (net 2 "Net-(BT1--)") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at 2.935 -1.525 180) (size 3.05 2.75) (layers "F.Cu" "F.Paste") (roundrect_rratio 0.09090909091)
      (net 2 "Net-(BT1--)") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at 2.935 1.525 180) (size 3.05 2.75) (layers "F.Cu" "F.Paste") (roundrect_rratio 0.09090909091)
      (net 2 "Net-(BT1--)") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -5.04 2.28 180) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 12 "Net-(D2-A)") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 173.785 73.66)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "1.0 microfarad" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 12 "Net-(D2-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "Net-(BT1--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Misc Custom:Keystone 1050 CR123 Battery Holder SMD" (layer "B.Cu")
    (at 162.56 92.71 180)
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr smd)
    (fp_text reference "BT1" (at 0 0.5 unlocked) (layer "B.SilkS"))
    (fp_text value "CR123A Battery " (at 0 -1 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab"))
    (pad "" thru_hole circle (at 8.1 22 180) (size 2 2) (drill 1.98) (layers "*.Mask"))
    (pad "1" smd rect (at 0 25.4 180) (size 7.5 8.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "Net-(BT1-+)") (pinfunction "+") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd rect (at 0 -18.635898 180) (size 7.5 8.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(BT1--)") (pinfunction "-") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Misc Custom:Keystone 1050 CR123 Battery Holder SMD" (layer "B.Cu")
    (at 142.24 85.945898)
    (property "Sheetfile" "LV_GPS_V2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr smd)
    (fp_text reference "BT3" (at 0 0.5 180 unlocked) (layer "B.SilkS"))
    (fp_text value "CR123A Battery " (at 0 -1 180 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 180 unlocked) (layer "B.Fab"))
    (pad "" thru_hole circle (at 8.1 22) (size 2 2) (drill 1.98) (layers "*.Mask"))
    (pad "1" smd rect (at 0 25.4) (size 7.5 8.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "Net-(BT3-+)") (pinfunction "+") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd rect (at 0 -18.635898) (size 7.5 8.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "Net-(BT1-+)") (pinfunction "-") (pintype "passive") (thermal_bridge_angle 45))
  )
  (gr_rect (start 127 50.8) (end 177.8 127)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "FIX" (at 160.02 114.935) (layer "F.SilkS"))
  (gr_text "THIS SIDE UP" (at 152.4 54.61) (layer "F.SilkS"))
  (gr_text "10" (at 156.21 110.49) (layer "F.SilkS"))
  (gr_text "1" (at 172.72 65.405) (layer "F.SilkS"))
  (gr_text "POWER" (at 137.795 86.36) (layer "F.SilkS"))
  (gr_text "10" (at 150.495 67.945) (layer "F.SilkS"))
  (gr_text "UAH CRW GPS LOCATOR\nREV. 2.0.0" (at 140.97 79.375) (layer "F.SilkS"))
  (gr_text "ON" (at 132.715 103.505) (layer "F.SilkS"))
  (gr_text "11" (at 172.085 110.49) (layer "F.SilkS"))
  (gr_text "20" (at 172.085 93.98) (layer "F.SilkS"))
  (gr_text "1" (at 156.845 93.98) (layer "F.SilkS"))
  (gr_text "20" (at 172.72 88.265) (layer "F.SilkS"))
  (gr_text "11" (at 151.13 90.17) (layer "F.SilkS"))
  (gr_text "OFF" (at 132.715 114.3) (layer "F.SilkS"))
)
