(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 155 105)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "magandpin/")
		)
	)
	(net 0 "")
	(net 1 "+3.3V")
	(net 2 "GND")
	(net 3 "Net-(U1-SCL)")
	(net 4 "unconnected-(H1-Pad1)")
	(net 5 "Net-(U1-SDA)")
	(net 6 "Net-(L1-Pad1)")
	(net 7 "Net-(H11-Pad1)")
	(footprint "Capacitor_SMD:C_01005_0402Metric_Pad0.57x0.30mm_HandSolder"
		(layer "F.Cu")
		(at 162.5 115.6 -90)
		(descr "Capacitor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 1.45 0.15 180)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_01005_0402Metric_Pad0.57x0.30mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.62 -90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.3625 0 270)
			(size 0.41 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.3625 0 270)
			(size 0.41 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3375 0 270)
			(size 0.575 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3375 0 270)
			(size 0.575 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_01005_0402Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "coilfromtiff:coilfromtiff"
		(layer "F.Cu")
		(at 163.05 96.825)
		(property "Reference" "L1"
			(at -5.5 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "L"
			(at -4.75 -4.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "coilfromtiff:coilfromtiff"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr board_only exclude_from_pos_files)
		(pad "1" connect rect
			(at 6.5 1)
			(size 0.889 2.54)
			(layers "F.Cu" "F.Mask")
			(net 6 "Net-(L1-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 163.895 106.275)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H10"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "10" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 161.355 118.975)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H4"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "4" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 163.895 118.975)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H3"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "3" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Capacitor_SMD:C_01005_0402Metric_Pad0.57x0.30mm_HandSolder"
		(layer "F.Cu")
		(at 164 115.5175 -90)
		(descr "Capacitor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 1.5325 -0.2 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 1 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_01005_0402Metric_Pad0.57x0.30mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.62 -90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.3625 0 270)
			(size 0.41 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.3625 0 270)
			(size 0.41 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3375 0 270)
			(size 0.575 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3375 0 270)
			(size 0.575 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_01005_0402Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SAMTEC_TSM-104-01-L-SH"
		(layer "F.Cu")
		(at 172.805 112.5875 -90)
		(property "Reference" "J1"
			(at 6 5 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TSM-104-01-L-SH"
			(at -1 8.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:SAMTEC_TSM-104-01-L-SH"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "R"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Samtec"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr smd)
		(pad "01" smd rect
			(at -3.81 5.28 270)
			(size 1.27 3.18)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(U1-SCL)")
			(pinfunction "01")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "02" smd rect
			(at -1.27 5.28 270)
			(size 1.27 3.18)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-SDA)")
			(pinfunction "02")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "03" smd rect
			(at 1.27 5.28 270)
			(size 1.27 3.18)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "+3.3V")
			(pinfunction "03")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "04" smd rect
			(at 3.81 5.28 270)
			(size 1.27 3.18)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "04")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "C:/Users/NGS/Documents/KiCad/8.0/3dmodels/TSM-104-01-L-SH.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 180 180)
			)
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 158.815 118.975)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H5"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "5" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Resistor_SMD:R_01005_0402Metric_Pad0.57x0.30mm_HandSolder"
		(layer "F.Cu")
		(at 161.6375 110 180)
		(descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -1.9125 -0.15 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.7K"
			(at 0 1 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_01005_0402Metric_Pad0.57x0.30mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.62 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.3625 0 180)
			(size 0.41 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.3625 0 180)
			(size 0.41 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3375 0 180)
			(size 0.575 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3375 0 180)
			(size 0.575 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U1-SDA)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 158.815 106.275)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H8"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "8" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Resistor_SMD:R_01005_0402Metric_Pad0.57x0.30mm_HandSolder"
		(layer "F.Cu")
		(at 161.6375 108.8 180)
		(descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -1.8625 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.7K"
			(at 0 1 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_01005_0402Metric_Pad0.57x0.30mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.62 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.3625 0 180)
			(size 0.41 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.3625 0 180)
			(size 0.41 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3375 0 180)
			(size 0.575 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3375 0 180)
			(size 0.575 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-SCL)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 166.435 106.275)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H11"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 9.5 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "11" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(H11-Pad1)")
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 156.275 116.435)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H7"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "7" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "footprints:XDCR_MMC5603NJ"
		(layer "F.Cu")
		(at 162.5 112.55 180)
		(property "Reference" "U1"
			(at 1.9 -1.575 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MMC5603NJ"
			(at 6.35 0.4 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:XDCR_MMC5603NJ"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "B"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Memsic Inc."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SNAPEDA_PN" "MMC5603NJ"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.6 mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr smd)
		(pad "A1" smd circle
			(at -0.2 -0.2 180)
			(size 0.23 0.23)
			(layers "F.Cu" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSA")
			(pintype "power_in")
		)
		(pad "A2" smd circle
			(at 0.2 -0.2 180)
			(size 0.23 0.23)
			(layers "F.Cu" "F.Paste")
			(net 3 "Net-(U1-SCL)")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "B1" smd circle
			(at -0.2 0.2 180)
			(size 0.23 0.23)
			(layers "F.Cu" "F.Paste")
			(net 1 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "B2" smd circle
			(at 0.2 0.2 180)
			(size 0.23 0.23)
			(layers "F.Cu" "F.Paste")
			(net 5 "Net-(U1-SDA)")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(model "C:/Users/NGS/Documents/KiCad/8.0/3dmodels/MMC5603NJ.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 180 180)
			)
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 161.355 106.275)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H9"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "9" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 168.975 118.975)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H1"
			(at 4.525 0.525 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(H1-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 166.435 118.975)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H2"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "2" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 156.275 118.975)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H6"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "6" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "mountinghole_1mm:MountingHole_1mm"
		(layer "F.Cu")
		(at 168.975 106.275)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H12"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "mountinghole_1mm:MountingHole_1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "12" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(L1-Pad1)")
		)
	)
	(footprint "coilfromtiff:coilfromtiff"
		(layer "B.Cu")
		(at 162.275 96.85 180)
		(property "Reference" "L2"
			(at -4.272035 4.029012 180)
			(layer "B.SilkS")
		)
		(property "Value" "L"
			(at -4.75 4.5 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "coilfromtiff:coilfromtiff"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "Magnetometer.kicad_sch")
		(attr board_only exclude_from_pos_files)
		(pad "1" connect rect
			(at 6.5 -1 180)
			(size 0.889 2.54)
			(layers "B.Cu" "B.Mask")
			(net 7 "Net-(H11-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(gr_line
		(start 155 89.75)
		(end 170.25 89.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155 105)
		(end 155 120.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155 89.75)
		(end 155 105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.25 120.25)
		(end 155 120.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.25 89.75)
		(end 170.25 105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.25 105)
		(end 170.25 120.25)
		(layer "Edge.Cuts")
	)
	(gr_text "SDA"
		(at 168.675 111.925 0)
		(layer "B.SilkS")
	)
	(gr_text "SDA"
		(at 160.95 117.8 -90)
		(layer "B.SilkS")
	)
	(gr_text "3.3V"
		(at 168.9 114.55 0)
		(layer "B.SilkS")
	)
	(gr_text "SCL"
		(at 163.35 117.875 -90)
		(layer "B.SilkS")
	)
	(gr_text "SCL"
		(at 168.775 109.425 0)
		(layer "B.SilkS")
	)
	(gr_text "Lin 3-28-24"
		(at 165.55 108.8 0)
		(layer "B.SilkS")
	)
	(gr_text "3.3V"
		(at 158.35 117.75 270)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 157.075 117.625 -90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 169 117.1 0)
		(layer "B.SilkS")
	)
	(gr_text "y"
		(at 157.85 110.95 0)
		(layer "F.SilkS")
	)
	(gr_text "z"
		(at 157.15 114.1 0)
		(layer "F.SilkS")
	)
	(gr_text "x"
		(at 159.9 113.5 0)
		(layer "F.SilkS")
	)
)