<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="61.75" y2="0" width="0" layer="20"/>
<wire x1="61.75" y1="0" x2="61.75" y2="46" width="0" layer="20"/>
<wire x1="61.75" y1="46" x2="0" y2="46" width="0" layer="20"/>
<wire x1="0" y1="46" x2="0" y2="0" width="0" layer="20"/>
<text>Sinful Media Tech.
Http://Media.Sinful-Flesh.com</text>
</plain>
<libraries>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TRACE_ANTENNA_2.4GHZ_15.2MM">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X17">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="cc3200mod">
<packages>
<package name="CC3200MOD">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="SOD-123FL">
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOT230P700X180-4N">
</package>
</packages>
</library>
<library name="Seeed-OPL-Inductor">
<packages>
<package name="L0805">
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="Seeed-OPL-Connector">
<packages>
<package name="MICRO-USB5+6P-SMD-0.65-AB">
</package>
</packages>
</library>
<library name="A_SFT_Logo">
<packages>
<package name="SFM_LOGO_SMALLER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E1" library="SparkFun-RF" package="TRACE_ANTENNA_2.4GHZ_15.2MM" value="ANTENNATRACE-15.2MM"/>
<element name="JP1" library="pinhead" package="1X17" value=" ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X17" value=" ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CC3200MOD" library="cc3200mod" package="CC3200MOD" value="CC3200">
<attribute name="NAME"/>
</element>
<element name="C1" library="adafruit" package="C0805K" value="1pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Texas Instruments_By_element14_Batch_1" package="SOT230P700X180-4N" value="REG1117-3.3">
<attribute name="OC_FARNELL" value="1212355"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="PACKAGE" value="SOT-223-4"/>
<attribute name="MPN" value="REG1117-3.3"/>
<attribute name="OC_NEWARK" value="35C1963"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="Seeed-OPL-Inductor" package="L0805" value=" "/>
<element name="FB2" library="Seeed-OPL-Inductor" package="L0805" value=" ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="adafruit" package="SOD-123FL" value=" "/>
<element name="C3" library="eagle-ltspice" package="C0805" value="100uF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C4" library="eagle-ltspice" package="C0805" value="22uF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="led" package="CHIP-LED0805" value=" ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="Seeed-OPL-Connector" package="MICRO-USB5+6P-SMD-0.65-AB" value="ZX62-B-5PA">
<attribute name="MPN" value="ZX62-B-5PA"/>
<attribute name="NAME"/>
</element>
<element name="U$2" library="A_SFT_Logo" package="SFM_LOGO_SMALLER" value="SMF_LOGO_SMALLER"/>
</elements>
<signals>
<signal name="GPIO12">
<contactref element="CC3200MOD" pad="P9"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="GPIO13">
<contactref element="CC3200MOD" pad="P10"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="GPIO14">
<contactref element="CC3200MOD" pad="P5"/>
<contactref element="JP2" pad="17"/>
</signal>
<signal name="GPIO15">
<contactref element="CC3200MOD" pad="P6"/>
<contactref element="JP2" pad="16"/>
</signal>
<signal name="GPIO16">
<contactref element="CC3200MOD" pad="P7"/>
<contactref element="JP2" pad="15"/>
</signal>
<signal name="GPIO17">
<contactref element="CC3200MOD" pad="P8"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="GPIO22">
<contactref element="CC3200MOD" pad="P11"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="GPIO28">
<contactref element="CC3200MOD" pad="P19"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="GPIO30">
<contactref element="CC3200MOD" pad="P42"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="SOP0">
<contactref element="CC3200MOD" pad="P34"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="JTAG_TDI">
<contactref element="CC3200MOD" pad="P12"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="N_RESET">
<contactref element="CC3200MOD" pad="P35"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="3V3">
<contactref element="CC3200MOD" pad="P37"/>
<contactref element="CC3200MOD" pad="P36"/>
<contactref element="CC3200MOD" pad="P40"/>
<contactref element="JP1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="GPIO11">
<contactref element="CC3200MOD" pad="P4"/>
<contactref element="JP1" pad="17"/>
</signal>
<signal name="GPIO10">
<contactref element="CC3200MOD" pad="P3"/>
<contactref element="JP1" pad="16"/>
</signal>
<signal name="GPIO9">
<contactref element="CC3200MOD" pad="P54"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="GPIO8">
<contactref element="CC3200MOD" pad="P53"/>
<contactref element="JP1" pad="14"/>
</signal>
<signal name="GPIO7">
<contactref element="CC3200MOD" pad="P52"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="GPIO6">
<contactref element="CC3200MOD" pad="P51"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="GPIO5">
<contactref element="CC3200MOD" pad="P50"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="GPIO4">
<contactref element="CC3200MOD" pad="P49"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="GPIO3">
<contactref element="CC3200MOD" pad="P48"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="GPIO2">
<contactref element="CC3200MOD" pad="P47"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="GPIO1">
<contactref element="CC3200MOD" pad="P46"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="GPIO0">
<contactref element="CC3200MOD" pad="P44"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="ANT_SEL_2">
<contactref element="JP2" pad="2"/>
<contactref element="CC3200MOD" pad="P26"/>
</signal>
<signal name="ANT_SEL_1">
<contactref element="JP2" pad="3"/>
<contactref element="CC3200MOD" pad="P25"/>
</signal>
<signal name="SOP1">
<contactref element="JP2" pad="4"/>
<contactref element="CC3200MOD" pad="P24"/>
</signal>
<signal name="SOP2">
<contactref element="JP2" pad="5"/>
<contactref element="CC3200MOD" pad="P23"/>
</signal>
<signal name="JTAG_TMS">
<contactref element="JP2" pad="6"/>
<contactref element="CC3200MOD" pad="P22"/>
</signal>
<signal name="JTAG_TCK">
<contactref element="JP2" pad="7"/>
<contactref element="CC3200MOD" pad="P21"/>
</signal>
<signal name="JTAG_TDO">
<contactref element="JP2" pad="9"/>
<contactref element="CC3200MOD" pad="P18"/>
</signal>
<signal name="GND">
<contactref element="CC3200MOD" pad="P1"/>
<contactref element="CC3200MOD" pad="P63"/>
<contactref element="CC3200MOD" pad="P62"/>
<contactref element="CC3200MOD" pad="P61"/>
<contactref element="CC3200MOD" pad="P60"/>
<contactref element="CC3200MOD" pad="P59"/>
<contactref element="CC3200MOD" pad="P58"/>
<contactref element="CC3200MOD" pad="P57"/>
<contactref element="CC3200MOD" pad="P56"/>
<contactref element="CC3200MOD" pad="P55"/>
<contactref element="CC3200MOD" pad="P43"/>
<contactref element="CC3200MOD" pad="P38"/>
<contactref element="CC3200MOD" pad="P32"/>
<contactref element="CC3200MOD" pad="P30"/>
<contactref element="CC3200MOD" pad="P28"/>
<contactref element="CC3200MOD" pad="P27"/>
<contactref element="CC3200MOD" pad="P16"/>
<contactref element="CC3200MOD" pad="P2"/>
<contactref element="JP2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="PWR" pad="C"/>
<contactref element="U1" pad="1"/>
<contactref element="FB2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="CC3200MOD" pad="P31"/>
<contactref element="E1" pad="ANT"/>
</signal>
<signal name="N$2">
<contactref element="E1" pad="GND"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="D2" pad="C"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="1"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="VIN">
<contactref element="D2" pad="A"/>
<contactref element="FB1" pad="2"/>
</signal>
<signal name="VBUS">
<contactref element="FB1" pad="1"/>
<contactref element="USB1" pad="1"/>
</signal>
<signal name="SHIELD">
<contactref element="USB1" pad="5"/>
<contactref element="USB1" pad="P6"/>
<contactref element="USB1" pad="P2"/>
<contactref element="USB1" pad="P3"/>
<contactref element="USB1" pad="P1"/>
<contactref element="USB1" pad="P4"/>
<contactref element="USB1" pad="P5"/>
<contactref element="FB2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
