<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="19.05" y2="0" width="0" layer="20"/>
<wire x1="19.05" y1="0" x2="19.084290625" y2="38.029515625" width="0" layer="20"/>
<wire x1="19.084290625" y1="38.029515625" x2="0.034290625" y2="38.029515625" width="0" layer="20"/>
<wire x1="0.034290625" y1="38.029515625" x2="0" y2="0" width="0" layer="20"/>
<text>NE5U Altus Metrum, Featherlight Switch, Battery Interface</text>
<text>NE5U Power Board</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="JST-PH-2-THM">
<description>4UCon #01528
http://www.4uconnector.com/online/object/4udrawing/01528.pdf</description>
</package>
</packages>
</library>
<library name="con-JST PH">
<description>
&lt;b&gt;JST Connectors&lt;/b&gt; - PH Series, 2.00mm pitch disconnectable crimp style connectors&lt;p&gt;

&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;

&lt;author&gt;Author: kylie &lt;/author&gt;, 02/2017&lt;p&gt;

&lt;a href="http://www.jst-mfg.com/product/detail_e.php?series=199"&gt;
&lt;img src="http://www.jst-mfg.com/product/images/pict/ph.jpg"  &gt;&lt;/a&gt;&lt;p&gt;
&lt;a href="http://www.jst-mfg.com/product/pdf/eng/ePH.pdf"&gt; Data sheet (PDF)&lt;/a&gt;&lt;p&gt;
&lt;p&gt; similar to:&lt;p&gt;
&lt;a href="https://www.hirose.com/product/en/products/DF3/"&gt; HIROSE DF3 series&lt;/a&gt;&lt;p&gt;
Würth 6200xxxxx22 series
&lt;a href="http://katalog.we-online.de/en/em/WTB_2_00_MALE_VERTICAL_SHROUDED_HEADER_6200XX11622?sid=331765e5c"&gt; vertical through-hole&lt;/a&gt;,  
&lt;a href="http://katalog.we-online.de/en/em/WTB_2_00_MALE_HORIZONTAL_SHROUDED_HEADER_6200XX11722?sid=331765e5c"&gt; horizontal through-hole&lt;/a&gt;,
&lt;a href="http://katalog.we-online.de/en/em/WTB_2_00_FEMALE_TERMINAL_HOUSING_6200XX113322?sid=331765e5cc"&gt; female terminal housing&lt;/a&gt;</description>
<packages>
<package name="B3B-PH-K-S">
<description>

&lt;b&gt;JST PH series header&lt;/b&gt; 2.00mm pitch disconnectable crimp style connectors, through-hole vertical (top entry type), 3 pins&lt;p&gt;

</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BATT1" library="adafruit" package="JST-PH-2-THM" value="3.7V LiPo">
<attribute name="NAME"/>
</element>
<element name="BATT2" library="adafruit" package="JST-PH-2-THM" value="3.7V LiPo">
<attribute name="NAME"/>
</element>
<element name="FLT1" library="adafruit" package="JST-PH-2-THM" value="FC1">
<attribute name="NAME"/>
</element>
<element name="SW" library="con-JST PH" package="B3B-PH-K-S" value="Mag SW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,2" value="MOUNT-HOLE3.2">
<attribute name="POPULARITY" value="7"/>
</element>
<element name="H2" library="holes" package="3,2" value="MOUNT-HOLE3.2">
<attribute name="POPULARITY" value="7"/>
</element>
<element name="FLT2" library="adafruit" package="JST-PH-2-THM" value="FC2">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="BATT1" pad="1"/>
<contactref element="SW" pad="1"/>
<contactref element="BATT2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="FLT1" pad="1"/>
<contactref element="SW" pad="3"/>
<contactref element="FLT2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="BATT1" pad="2"/>
<contactref element="SW" pad="2"/>
<contactref element="FLT1" pad="2"/>
<contactref element="BATT2" pad="2"/>
<contactref element="FLT2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
