(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "Spectrum Analyzer Resolution Filter")
    (date "2022-07-30")
    (rev "0")
    (company "Andy McCann KA3KAF Doug McCann KA3KAG")
    (comment 2 "Wes Hayward W7ZOI")
    (comment 3 "Original Design By")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 101.6 111.76)
    (pcbplotparams
      (layerselection 0x0000030_7ffffffe)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits false)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C501-Pad1)")
  (net 2 "Net-(C501-Pad2)")
  (net 3 "GND")
  (net 4 "/501-in")
  (net 5 "Net-(C509-Pad2)")
  (net 6 "Net-(C514-Pad2)")
  (net 7 "Net-(C519-Pad2)")
  (net 8 "/502-in")
  (net 9 "Net-(C523-Pad2)")
  (net 10 "Net-(K502-Pad1)")
  (net 11 "/VIn")
  (net 12 "Net-(C503-Pad3)")
  (net 13 "Net-(J503-Pad1)")
  (net 14 "Net-(K501-Pad5)")
  (net 15 "Net-(K501-Pad10)")
  (net 16 "Net-(K502-Pad10)")
  (net 17 "Net-(C511-Pad1)")
  (net 18 "Net-(C513-Pad1)")
  (net 19 "Net-(C505-Pad1)")
  (net 20 "Net-(C508-Pad1)")
  (net 21 "Net-(C516-Pad1)")
  (net 22 "Net-(C518-Pad1)")
  (footprint "resolution-filters:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 162.0359 88.1125)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C513" (at 2.54 -1.61026) (layer "F.SilkS"))
    (fp_text value "1.8p-10p" (at 2.54 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.1363 -1.4223) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 18 "Net-(C513-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 120.5169 75.6412)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C510" (at 2.44455 -1.905) (layer "F.SilkS"))
    (fp_text value "12p-60p" (at 2.54 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.0447 -1.6002) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 5 "Net-(C509-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 117.5572 72.2884 -90)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L501" (at -0.381 2.8 90) (layer "F.SilkS"))
    (fp_text value "1.15u" (at 0 8.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(C501-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/T37-6 IND004.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/T37-6 IND004.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 176.8348 96.774)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R509" (at 3.556 -0.381) (layer "F.SilkS"))
    (fp_text value "10M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(K502-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 187.5 68.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "R")
    (attr exclude_from_pos_files)
    (fp_text reference "H503" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 115.0366 94.6658 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R501" (at 3.81 -0.127) (layer "F.SilkS"))
    (fp_text value "150" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "/VIn") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 140.9446 94.488)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP506" (at 0 -1.998) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(C523-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 106.5 106.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "R")
    (attr exclude_from_pos_files)
    (fp_text reference "H502" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "resolution-filters:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 169.6875 88.1125)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C516" (at 2.54 -1.61026) (layer "F.SilkS"))
    (fp_text value "1.8p-10p" (at 2.54 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at 0.0099 -1.2953) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 21 "Net-(C516-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 135.0203 88.3412)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C508" (at 2.44455 -1.905) (layer "F.SilkS"))
    (fp_text value "1.8p-10p" (at 2.54 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.2479 -1.6002) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 20 "Net-(C508-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 175.133 66.802)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R504" (at 3.6068 0.0254) (layer "F.SilkS"))
    (fp_text value "270" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/501-in") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C503-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 108.4326 99.0854)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP503" (at 0 -1.998) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 4 "/501-in") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 145.5106 72.4154 90)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L503" (at 0.0254 2.799994 90) (layer "F.SilkS"))
    (fp_text value "1.15u" (at 0 8.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(C514-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/T37-6 IND004.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Dougl/OneDrive/Ham Radio/KiCad Files/W7ZOI Spectrum Analyzer/if-and-log-amp/if-and-log-amp/if-log-amp-models/if-log-amp-3D/T37-6 IND004.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 102.783 75.438)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C506" (at 2.423795 0) (layer "F.SilkS"))
    (fp_text value ".1u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/501-in") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 154.1719 75.7682)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C520" (at 2.59695 -2.1336) (layer "F.SilkS"))
    (fp_text value "12p-60p" (at 2.54 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.1209 -1.8034) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 7 "Net-(C519-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 120.269 99.0092 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R503" (at 3.81 -0.127 90) (layer "F.SilkS"))
    (fp_text value "150" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(K501-Pad5)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 137.3571 75.7174)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C515" (at 2.44455 -1.905) (layer "F.SilkS"))
    (fp_text value "12p-60p" (at 2.54 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.1209 -1.8034) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 6 "Net-(C514-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 119.4816 94.107)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP502" (at 0 -1.998) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 15 "Net-(K501-Pad10)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 128.645 72.3646 90)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L502" (at 0.0762 2.749194 90) (layer "F.SilkS"))
    (fp_text value "1.15u" (at 0 8.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(C509-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/T37-6 IND004.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Dougl/OneDrive/Ham Radio/KiCad Files/W7ZOI Spectrum Analyzer/if-and-log-amp/if-and-log-amp/if-log-amp-models/if-log-amp-3D/T37-6 IND004.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 164.0478 81.6102)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C524" (at 2.3622 -0.0762) (layer "F.SilkS"))
    (fp_text value "120p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C523-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 177.1142 81.5594 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C521" (at 2.7286 0.0254) (layer "F.SilkS"))
    (fp_text value ".1u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/502-in") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:XTAL_ECS-10.7-7.5B" (layer "F.Cu")
    (tedit 62B58515)
    (at 151.5872 104.9959 90)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y503" (at -3.3605 -1.397 90) (layer "F.SilkS"))
    (fp_text value "10.7MHz" (at 5.93 3.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.44 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 18 "Net-(C513-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 21 "Net-(C516-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.44 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/UM-007.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/UM-007.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 150.7744 95.5802)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R511" (at 3.9116 -0.0368) (layer "F.SilkS"))
    (fp_text value "10M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C523-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 104.521 98.961 90)
    (descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Conn_Coaxial")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr exclude_from_pos_files)
    (fp_text reference "J501" (at 2.3 -2.25 90) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 2.3 2.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.3 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 11 "/VIn") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.6 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Ext") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 150.241 84.963 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R506" (at 3.63234 -0.035346 90) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C511-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C513-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 117.1194 89.662)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R502" (at 3.429 0) (layer "F.SilkS"))
    (fp_text value "36" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "/VIn") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(K501-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 148.2998 81.661)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C522" (at 2.4892 -0.0254) (layer "F.SilkS"))
    (fp_text value "120p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C519-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Transformer_THT:Transformer_Toroid_Horizontal_D14.0mm_Amidon-T50" (layer "F.Cu")
    (tedit 5A030845)
    (at 125.0188 94.0054 -90)
    (descr "Transformer, Toroid, horizontal, laying, Diameter 14mm, Amidon T50,")
    (tags "Transformer Toroid horizontal laying Diameter 14mm Amidon T50 ")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "T501" (at 7.3904 -10.4864 -90) (layer "F.SilkS"))
    (fp_text value "Transformer_1P_1S" (at 8 3.8 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8 -5 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(K501-Pad10)") (pinfunction "AA") (pintype "passive"))
    (pad "2" thru_hole circle (at 16 0 270) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "AB") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -10 270) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "SA") (pintype "passive"))
    (pad "4" thru_hole circle (at 16 -10 270) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(C505-Pad1)") (pinfunction "SB") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/L_Tor_13x8x5_3a_cp.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/L_Tor_13x8x5_3a_cp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 127.5527 88.3158)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C505" (at 2.372146 -1.80326) (layer "F.SilkS"))
    (fp_text value "1.8p-10p" (at 2.54 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.1717 -1.6256) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 19 "Net-(C505-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 117.3518 81.6609)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C509" (at 2.5 -0.0253) (layer "F.SilkS"))
    (fp_text value "5.6p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C501-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C509-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 124.7587 81.6609)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C514" (at 2.4083 -0.0253) (layer "F.SilkS"))
    (fp_text value "3.3p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C509-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C514-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 114.0206 80.2024 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C507" (at 2.4492 0.0254 90) (layer "F.SilkS"))
    (fp_text value "120p" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C501-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 117.6166 85.8266)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C512" (at 2.3984 -0.1524) (layer "F.SilkS"))
    (fp_text value "180p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C509-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:XTAL_ECS-10.7-7.5B" (layer "F.Cu")
    (tedit 62B58515)
    (at 157.0736 104.9959 90)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y504" (at -3.048 -1.397 90) (layer "F.SilkS"))
    (fp_text value "10.7MHz" (at 5.93 3.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.44 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 21 "Net-(C516-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 22 "Net-(C518-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.44 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/UM-007.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/UM-007.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 106.5 68.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "R")
    (attr exclude_from_pos_files)
    (fp_text reference "H501" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 132.6934 81.6356)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C517" (at 2.4492 -0.0508) (layer "F.SilkS"))
    (fp_text value "180p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C514-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 157.8864 92.6084 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R507" (at 3.96226 0.035346 90) (layer "F.SilkS"))
    (fp_text value "9.1k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C513-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 109.474 86.186 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C501" (at 2.4092 -0.1016 90) (layer "F.SilkS"))
    (fp_text value "56p" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C501-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C501-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Transformer_THT:Transformer_Toroid_Horizontal_D14.0mm_Amidon-T50" (layer "F.Cu")
    (tedit 5A030845)
    (at 172.5384 109.8032 90)
    (descr "Transformer, Toroid, horizontal, laying, Diameter 14mm, Amidon T50,")
    (tags "Transformer Toroid horizontal laying Diameter 14mm Amidon T50 ")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "T502" (at 8.4826 0.2324 90) (layer "F.SilkS"))
    (fp_text value "Transformer_1P_1S" (at 8 3.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8 -5 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(K502-Pad10)") (pinfunction "AA") (pintype "passive"))
    (pad "2" thru_hole circle (at 16 0 90) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "AB") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -10 90) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "SA") (pintype "passive"))
    (pad "4" thru_hole circle (at 16 -10 90) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(C518-Pad1)") (pinfunction "SB") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/L_Tor_13x8x5_3a_cp.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/L_Tor_13x8x5_3a_cp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 190.0682 98.6168 90)
    (descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Conn_Coaxial")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr exclude_from_pos_files)
    (fp_text reference "J503" (at 2.3 -2.25 90) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 2.3 2.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.3 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 13 "Net-(J503-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.6 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Ext") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 186.2582 100.6856)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP504" (at 0 -1.998) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 8 "/502-in") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 113.5126 89.1794)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP501" (at 0 -1.998) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 2 "Net-(C501-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "resolution-filters:XTAL_ECS-10.7-7.5B" (layer "F.Cu")
    (tedit 62B58515)
    (at 140.6144 104.9705 90)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y501" (at -3.2335 -1.397 90) (layer "F.SilkS"))
    (fp_text value "10.7MHz" (at 5.93 3.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.44 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 19 "Net-(C505-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 20 "Net-(C508-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.44 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/UM-007.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/UM-007.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 176.8348 93.5736)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R510" (at 3.6322 -0.0762) (layer "F.SilkS"))
    (fp_text value "0" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(K502-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C523-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 156.1122 81.6102)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C523" (at 2.4238 -0.0254) (layer "F.SilkS"))
    (fp_text value "56p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C519-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C523-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 140.6337 81.6609)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C519" (at 2.4337 -0.0253) (layer "F.SilkS"))
    (fp_text value "5.6p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C514-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C519-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 174.0916 69.8754 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D501" (at 4.191 -0.0508 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/501-in") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_SPDT_Omron_G5V-1" (layer "F.Cu")
    (tedit 5A57D9C3)
    (at 111.887 99.314)
    (descr "Relay Omron G5V-1, see http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v_1.pdf")
    (tags "Relay Omron G5V-1")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K501" (at 2.4075 6.7355) (layer "F.SilkS"))
    (fp_text value "G5V-1" (at 2.5 12.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C501-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/501-in") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(K501-Pad5)") (pintype "passive"))
    (pad "6" thru_hole circle (at 5.08 10.16) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(K501-Pad5)") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(K501-Pad10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_Omron_G5V-1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 142.4686 88.3666)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C511" (at 2.499146 -2.05726) (layer "F.SilkS"))
    (fp_text value "1.8p-10p" (at 2.54 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.2032 -1.524) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 17 "Net-(C511-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 154.051 92.5576 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R505" (at 4.14006 -0.015454 90) (layer "F.SilkS"))
    (fp_text value "9.1k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C511-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 162.1984 72.3646 90)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L504" (at -0.127 2.749194 90) (layer "F.SilkS"))
    (fp_text value "1.15u" (at 0 8.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(C519-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/T37-6 IND004.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Dougl/OneDrive/Ham Radio/KiCad Files/W7ZOI Spectrum Analyzer/if-and-log-amp/if-and-log-amp/if-log-amp-models/if-log-amp-3D/T37-6 IND004.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 177.1489 88.1125)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C518" (at 2.54 -1.61026) (layer "F.SilkS"))
    (fp_text value "1.8p-10p" (at 2.54 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.0601 -1.4731) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 22 "Net-(C518-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 182.1942 69.9516 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R508" (at 3.8862 -0.1016 90) (layer "F.SilkS"))
    (fp_text value "270" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C503-Pad3)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/502-in") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 146.1262 94.5388)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP505" (at 0 -1.998) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 16 "Net-(K502-Pad10)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 187.5 106.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "R")
    (attr exclude_from_pos_files)
    (fp_text reference "H504" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "resolution-filters:691137710002" (layer "F.Cu")
    (tedit 62B4FAFD)
    (at 187.833 85.1408 90)
    (descr "<b>WR-TBL Serie 1377 - 5.00 mm Horiz Entry w. Pressure Clamp Glow Wire<br></b>Max Height = 11.5mm , Pitch 5mm , 2 Pins")
    (property "DATASHEET-URL" "https://www.we-online.com/catalog/datasheet/691137710002.pdf")
    (property "IR-UL" "16A")
    (property "IR-VDE" "24A")
    (property "MOUNT" "THT")
    (property "PART-NUMBER" "691137710002")
    (property "PINS" "2")
    (property "PITCH" "5mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Terminal Block")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (property "TYPE" "Horizontal")
    (property "VALUE" "691137710002")
    (property "WIRE" "12 to 30 (AWG) 3.31 to 0.05 (mm²)")
    (property "WORKING-VOLTAGE-UL" "300V(AC)")
    (property "WORKING-VOLTAGE-VDE" "250V(AC)")
    (attr through_hole)
    (fp_text reference "J502" (at 2.5146 -4.6736 90) (layer "F.SilkS"))
    (fp_text value "Terminal Block" (at 4.12 5.365 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.5 0 90) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(C503-Pad3)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 90) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/691103110002.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/691103110002_1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 178.5112 77.6224 90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D502" (at 4.1402 0.0762 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/502-in") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 104.521 91.226 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C502" (at 2.6308 0.0254 90) (layer "F.SilkS"))
    (fp_text value "120p" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C501-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 102.7115 80.645)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C504" (at 2.69855 -1.778) (layer "F.SilkS"))
    (fp_text value "12p-60p" (at 2.54 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.0701 -1.6764) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 1 "Net-(C501-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/Trimmer Cap - Brown.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Dougl/OneDrive/Ham Radio/KiCad Files/W7ZOI Spectrum Analyzer/if-and-log-amp/if-and-log-amp/if-log-amp-models/if-log-amp-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_SPDT_Omron_G5V-1" (layer "F.Cu")
    (tedit 5A57D9C3)
    (at 177.3737 100.2239)
    (descr "Relay Omron G5V-1, see http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v_1.pdf")
    (tags "Relay Omron G5V-1")
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K502" (at 2.9155 7.1165) (layer "F.SilkS"))
    (fp_text value "G5V-1" (at 2.5 12.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(K502-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/502-in") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J503-Pad1)") (pintype "passive"))
    (pad "6" thru_hole circle (at 5.08 10.16) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J503-Pad1)") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(K502-Pad10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_Omron_G5V-1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "resolution-filters:XTAL_ECS-10.7-7.5B" (layer "F.Cu")
    (tedit 62B58515)
    (at 146.1262 104.9958 90)
    (property "Sheetfile" "resolution-filters.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y502" (at -3.302 -1.27 90) (layer "F.SilkS"))
    (fp_text value "10.7MHz" (at 5.93 3.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.44 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 20 "Net-(C508-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 17 "Net-(C511-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.44 0 90) (size 1.03 1.03) (drill 0.63) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/UM-007.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/resolution-filters-models/resolution-filters-3D/UM-007.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 101.117263 67.604851) (mid 102.349348 64.630345) (end 105.323854 63.39826) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 188.301482 63.39826) (end 105.323854 63.39826) (layer "Edge.Cuts") (width 0.16))
  (gr_arc (start 105.669624 112.16626) (mid 102.45063 110.832893) (end 101.117263 107.613899) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 192.811263 108.177585) (end 192.811263 67.908041) (layer "Edge.Cuts") (width 0.16))
  (gr_arc (start 192.811263 108.177585) (mid 191.643 110.998) (end 188.822588 112.16626) (layer "Edge.Cuts") (width 0.16))
  (gr_arc (start 188.301482 63.39826) (mid 191.490367 64.719153) (end 192.811263 67.908041) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 101.117263 67.604851) (end 101.117263 107.613899) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 105.669624 112.16626) (end 188.822588 112.16626) (layer "Edge.Cuts") (width 0.16))
  (gr_text "Andy McCann KA3KAF\nDoug McCann KA3KAG" (at 125.1712 66.5226) (layer "B.SilkS"))
  (gr_text "Spectrum Analyzer\nResolution Filter Rev O" (at 158.5468 66.421) (layer "B.SilkS"))
  (gr_text "+15" (at 185.4454 102.489) (layer "F.SilkS"))
  (gr_text "LC Filter\nOut" (at 140.5636 97.1296) (layer "F.SilkS"))
  (gr_text "+15" (at 108.1278 101.1936) (layer "F.SilkS"))
  (gr_text "+15" (at 189.0014 78.0542) (layer "F.SilkS"))
  (gr_text "Out" (at 190.119 101.9048) (layer "F.SilkS"))
  (gr_text "Xtal Filter\nOut" (at 146.5072 97.1804) (layer "F.SilkS"))
  (gr_text "In" (at 102.743 101.981) (layer "F.SilkS"))
  (gr_text "Xtal Filter\nIn" (at 119.2276 96.8248) (layer "F.SilkS"))
  (gr_text "LC Filter\nIn" (at 113.7666 91.8718) (layer "F.SilkS"))
  (zone (net 3) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.1604 64.2366)
        (xy 192.8622 67.31)
        (xy 192.7098 108.585)
        (xy 192.0748 110.4646)
        (xy 189.1284 112.1664)
        (xy 105.3084 112.0902)
        (xy 102.4636 111.0996)
        (xy 101.0412 108.3818)
        (xy 101.1682 66.7004)
        (xy 102.9208 64.1096)
        (xy 104.9274 63.4238)
        (xy 105.3592 63.4238)
        (xy 188.468 63.3984)
      )
    )
  )
)
