(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 1064)
    (zones 0)
    (modules 35)
    (nets 96)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad14)")
  (net 2 "Net-(U1-Pad17)")
  (net 3 "Net-(U1-Pad18)")
  (net 4 "Net-(U1-Pad19)")
  (net 5 "Net-(U1-Pad23)")
  (net 6 "Net-(U3-Pad16)")
  (net 7 "Net-(U3-Pad17)")
  (net 8 "Net-(U3-Pad18)")
  (net 9 "Net-(U4-Pad8)")
  (net 10 "Net-(U4-Pad9)")
  (net 11 "Net-(U5-Pad16)")
  (net 12 "Net-(U5-Pad15)")
  (net 13 "Net-(U5-Pad13)")
  (net 14 "Net-(U5-Pad12)")
  (net 15 "Net-(U5-Pad10)")
  (net 16 "Net-(U5-Pad2)")
  (net 17 "Net-(C3-Pad1)")
  (net 18 GND)
  (net 19 "Net-(C4-Pad1)")
  (net 20 /A10)
  (net 21 /D4)
  (net 22 /D5)
  (net 23 /D6)
  (net 24 /D7)
  (net 25 /D3)
  (net 26 /D2)
  (net 27 /D1)
  (net 28 /D0)
  (net 29 -5V)
  (net 30 /A0)
  (net 31 /A1)
  (net 32 /A2)
  (net 33 +12V)
  (net 34 /A3)
  (net 35 /A4)
  (net 36 /A5)
  (net 37 /A6)
  (net 38 /A7)
  (net 39 /A8)
  (net 40 /A9)
  (net 41 /A15)
  (net 42 /A12)
  (net 43 /A13)
  (net 44 /A14)
  (net 45 /A11)
  (net 46 RESb)
  (net 47 MCU39)
  (net 48 RESCDIV)
  (net 49 8080HOLD)
  (net 50 DISINT)
  (net 51 CLKMON)
  (net 52 SP1)
  (net 53 +5V)
  (net 54 "Net-(J1-Pad2)")
  (net 55 "Net-(J1-Pad3)")
  (net 56 "Net-(J1-Pad4)")
  (net 57 "Net-(J1-Pad5)")
  (net 58 "Net-(C2-Pad1)")
  (net 59 "Net-(C5-Pad1)")
  (net 60 "Net-(C5-Pad2)")
  (net 61 "Net-(C6-Pad2)")
  (net 62 "Net-(C6-Pad1)")
  (net 63 "Net-(C7-Pad1)")
  (net 64 /CTS)
  (net 65 "Net-(J2-Pad3)")
  (net 66 /RX)
  (net 67 /TX)
  (net 68 "Net-(J2-Pad6)")
  (net 69 MCU20)
  (net 70 MCU19)
  (net 71 MCU18)
  (net 72 MCU17)
  (net 73 DISHOLD)
  (net 74 RES)
  (net 75 "Net-(J3-Pad1)")
  (net 76 "Net-(J3-Pad2)")
  (net 77 "Net-(J3-Pad4)")
  (net 78 "Net-(J3-Pad7)")
  (net 79 "Net-(J3-Pad8)")
  (net 80 "Net-(J3-Pad10)")
  (net 81 "Net-(J5-Pad23)")
  (net 82 "Net-(J5-Pad25)")
  (net 83 "Net-(J5-Pad27)")
  (net 84 "Net-(J5-Pad29)")
  (net 85 "Net-(J5-Pad31)")
  (net 86 "Net-(J5-Pad33)")
  (net 87 "Net-(J5-Pad34)")
  (net 88 "Net-(J5-Pad35)")
  (net 89 "Net-(J5-Pad36)")
  (net 90 "Net-(J5-Pad37)")
  (net 91 "Net-(J5-Pad38)")
  (net 92 "Net-(J5-Pad40)")
  (net 93 "Net-(J1-Pad6)")
  (net 94 "Net-(U2-Pad6)")
  (net 95 "Net-(U2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net -5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CTS)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /RX)
    (add_net /TX)
    (add_net 8080HOLD)
    (add_net CLKMON)
    (add_net DISHOLD)
    (add_net DISINT)
    (add_net GND)
    (add_net MCU17)
    (add_net MCU18)
    (add_net MCU19)
    (add_net MCU20)
    (add_net MCU39)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J5-Pad23)")
    (add_net "Net-(J5-Pad25)")
    (add_net "Net-(J5-Pad27)")
    (add_net "Net-(J5-Pad29)")
    (add_net "Net-(J5-Pad31)")
    (add_net "Net-(J5-Pad33)")
    (add_net "Net-(J5-Pad34)")
    (add_net "Net-(J5-Pad35)")
    (add_net "Net-(J5-Pad36)")
    (add_net "Net-(J5-Pad37)")
    (add_net "Net-(J5-Pad38)")
    (add_net "Net-(J5-Pad40)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U4-Pad9)")
    (add_net "Net-(U5-Pad10)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad13)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad16)")
    (add_net "Net-(U5-Pad2)")
    (add_net RES)
    (add_net RESCDIV)
    (add_net RESb)
    (add_net SP1)
  )
  (net_class HiPower ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.4)
    (uvia_drill 0.2)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.4)
    (uvia_drill 0.2)
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BD12)
    (at 25.3594 102.806 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C12 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BD18)
    (at 25.3441 96.1898 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C14 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 -5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BC63)
    (at 55.7378 93.3704)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C15 (at 1.25 -2.5) (layer F.SilkS))
    (fp_text value .1uF (at -1.83894 0.02036 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 +12V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 5BA8BC71)
    (at 67.3405 93.2612)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at 3.87604 -2.41808) (layer F.SilkS))
    (fp_text value 47k (at 3.92684 -0.04318) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 71 MCU18))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 53 +5V))
  )
  (module Resistors_THT:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 5BA8BCD4)
    (at 64.7065 105.931 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R5 (at 3.96242 -2.41804 90) (layer F.SilkS))
    (fp_text value 47k (at 3.9624 0.04318 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 GND))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 72 MCU17))
  )
  (module Housings_DIP:DIP-40_W15.24mm (layer F.Cu) (tedit 5BA8BC7F)
    (at 29.8983 67.8917)
    (descr "40-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U1 (at -2.26568 -1.66116 180) (layer F.SilkS))
    (fp_text value 8080A (at 7.52348 3.29946) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /A10))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /D4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /D5))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /D6))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /D7))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /D3))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /D2))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /D1))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /D0))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 -5V))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 RES))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 8080HOLD))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(J5-Pad29)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(J5-Pad31)"))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad17)"))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad19)"))
    (pad 20 thru_hole oval (at 0 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 21 thru_hole oval (at 15.24 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "Net-(J5-Pad40)"))
    (pad 22 thru_hole oval (at 15.24 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "Net-(J5-Pad38)"))
    (pad 23 thru_hole oval (at 15.24 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad23)"))
    (pad 24 thru_hole oval (at 15.24 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(J5-Pad34)"))
    (pad 25 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /A0))
    (pad 26 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /A1))
    (pad 27 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /A2))
    (pad 28 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 +12V))
    (pad 29 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /A3))
    (pad 30 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /A4))
    (pad 31 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /A5))
    (pad 32 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /A6))
    (pad 33 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /A7))
    (pad 34 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /A8))
    (pad 35 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A9))
    (pad 36 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /A15))
    (pad 37 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /A12))
    (pad 38 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /A13))
    (pad 39 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /A14))
    (pad 40 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /A11))
    (model Housings_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm (layer F.Cu) (tedit 5BA8BC85)
    (at 78.2599 63.1596)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U3 (at 1.0643 36.35754) (layer F.SilkS))
    (fp_text value PIC18LF2420-E_SP (at 3.76682 15.81912 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 RESb))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 MCU39))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 RESCDIV))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 8080HOLD))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 DISINT))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 CLKMON))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 SP1))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C4-Pad1)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 MCU20))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 MCU19))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 MCU18))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 MCU17))
    (pad 15 thru_hole oval (at 7.62 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 DISHOLD))
    (pad 16 thru_hole oval (at 7.62 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U3-Pad16)"))
    (pad 17 thru_hole oval (at 7.62 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U3-Pad17)"))
    (pad 18 thru_hole oval (at 7.62 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(U3-Pad18)"))
    (pad 19 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 20 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 21 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /D0))
    (pad 22 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /D1))
    (pad 23 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /D2))
    (pad 24 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /D3))
    (pad 25 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /D4))
    (pad 26 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /D5))
    (pad 27 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /D6))
    (pad 28 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /D7))
    (model Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5BA8BCB6)
    (at 52.1386 98.2701)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U5 (at -2.10314 -1.37164 90) (layer F.SilkS))
    (fp_text value 74HC4049N,652 (at 3.95986 8.80364 90) (layer F.SilkS))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U5-Pad16)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(U5-Pad15)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U5-Pad13)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(U5-Pad12)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U5-Pad10)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(J5-Pad29)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "Net-(U2-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "Net-(J5-Pad38)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(U2-Pad7)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U5-Pad2)"))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BCC8)
    (at 71.0768 114.539 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.23698 -2.26822 90) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8C45D)
    (at 94.6455 73.8937)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at -0.42674 -2.26824) (layer F.SilkS))
    (fp_text value .1uF (at 2.2352 -2.29108) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(C2-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BCC3)
    (at 77.1093 101.829 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 1.4478 2.2733 270) (layer F.SilkS))
    (fp_text value 22pF (at 1.26492 -2.44348 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BCBC)
    (at 77.1144 109.931 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C4 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 22pF (at 1.25 2.5 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C4-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8C463)
    (at 91.6584 77.8408 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 2.63144 2.20726 180) (layer F.SilkS))
    (fp_text value .1uF (at -0.05592 2.2631 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 60 "Net-(C5-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BCF1)
    (at 87.3735 106.086 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value .1uF (at 4.35094 0.2159) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 61 "Net-(C6-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BCF8)
    (at 87.3735 112.365 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value .1uF (at 4.43464 0.13462) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(C7-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8C469)
    (at 94.4905 77.8231)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at -0.59436 2.38252) (layer F.SilkS))
    (fp_text value .1uF (at 1.99648 2.37486) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BC68)
    (at 64.0791 93.3069 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C9 (at 1.28778 2.38252 180) (layer F.SilkS))
    (fp_text value .1uF (at 4.25196 -0.25654 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BD59)
    (at 74.0232 68.1584 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C10 (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BCA0)
    (at 74.0232 75.9511 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C11 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value .1uF (at 1.25 2.5 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BD0B)
    (at 25.08 112.057 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C13 (at 5.33146 -0.02794 270) (layer F.SilkS))
    (fp_text value "4.7uF Tant" (at 2.9972 -2.48158 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BC77)
    (at 49.5148 93.3831)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C16 (at 1.25 -2.5) (layer F.SilkS))
    (fp_text value .1uF (at 4.34912 -0.01778 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5BA8BD47)
    (at 46.322 62.3316 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C17 (at 4.57708 -0.01524 270) (layer F.SilkS))
    (fp_text value "1uF Tant" (at 1.16332 -2.27076 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 74 RES))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 5BA8BD27)
    (at 24.9835 73.5127 90)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D1 (at 5.1435 1.59766 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 4.89458 -1.77546 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 270) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 270) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 74 RES))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (offset (xyz 5.079999923706055 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5BA8BD53)
    (at 70.2589 62.3291 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J4 (at -0.04314 -2.46376 270) (layer F.SilkS))
    (fp_text value "+5v PWR" (at -2.6797 1.08458 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 93 "Net-(J1-Pad6)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5BA8BD40)
    (at 34.5364 62.3037 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at -0.11176 -3.02768 90) (layer F.SilkS))
    (fp_text value RES_ENA (at -2.42316 1.26492 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 "Net-(J5-Pad23)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 RES))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_THT:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 5BA8BD1E)
    (at 24.9581 85.1459 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 4.08432 2.27838 90) (layer F.SilkS))
    (fp_text value 100k (at 3.8354 -0.02794 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 GND))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 74 RES))
  )
  (module Resistors_THT:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 5BA8BCCE)
    (at 64.7167 117.135 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 3.85064 -2.32156 90) (layer F.SilkS))
    (fp_text value 47k (at 3.94716 -0.00762 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 53 +5V))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 69 MCU20))
  )
  (module Resistors_THT:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 5BA8BCA8)
    (at 74.0791 80.5485 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 3.9624 -2.47142 270) (layer F.SilkS))
    (fp_text value 47k (at 3.72364 -0.02032 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 70 MCU19))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 53 +5V))
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5BA8BC8E)
    (at 89.2658 83.6397)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U4 (at -0.37084 -3.34518) (layer F.SilkS))
    (fp_text value HIN232ECBNZ (at 4.03606 8.91794 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(C2-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(C5-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(C6-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(C6-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(C7-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /CTS))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U4-Pad8)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(U4-Pad9)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U3-Pad16)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U3-Pad17)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(U3-Pad18)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /RX))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 /TX))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 +5V))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 5BA8BCDC)
    (at 71.1454 103.845 90)
    (descr "Crystal Quarz HC49/U vertical stehend")
    (tags "Crystal Quarz HC49/U vertical stehend")
    (fp_text reference X1 (at 6.4135 -0.01016 180) (layer F.SilkS))
    (fp_text value 10Mhz (at 0.00254 -3.2639 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.44094 0 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 19 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.44094 0 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 17 "Net-(C3-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5BA8BCE1)
    (at 82.5906 115.288 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at -2.77622 13.72362 180) (layer F.SilkS))
    (fp_text value RS232 (at 0 -3.1 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 /CTS))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 /RX))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 /TX))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 68 "Net-(J2-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (offset (xyz 0 -6.349999904632568 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5BA8BD4C)
    (at 51.6763 62.3367 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at 0.01016 -2.36474 270) (layer F.SilkS))
    (fp_text value JTAG (at -2.76606 12.52474 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 93 "Net-(J1-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (offset (xyz 0 -6.349999904632568 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 (layer F.Cu) (tedit 5BA8BCE8)
    (at 95.1128 117.279 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J3 (at 5.56768 -1.29794 180) (layer F.SilkS))
    (fp_text value RS232_DB9 (at -2.62382 5.25018 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 /TX))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 /RX))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 /CTS))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 "Net-(J3-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "Net-(J3-Pad10)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (offset (xyz 1.269999980926514 -5.079999923706055 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20 (layer F.Cu) (tedit 5BA8BD02)
    (at 17.5793 65.7123)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J5 (at -1.05664 -2.7686) (layer F.SilkS))
    (fp_text value "8080 Bus" (at 1.8415 51.23942 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /A10))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 /A11))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 /A14))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /D4))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 /A13))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /D5))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 /A12))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /D6))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 /A15))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /D7))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 /A9))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /D3))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 /A8))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /D2))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 /A7))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /D1))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 /A6))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /D0))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /A5))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 -5V))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /A4))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 "Net-(J5-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /A3))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 "Net-(J5-Pad25)"))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 +12V))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 "Net-(J5-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /A2))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 84 "Net-(J5-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /A1))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 85 "Net-(J5-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /A0))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 86 "Net-(J5-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 87 "Net-(J5-Pad34)"))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 88 "Net-(J5-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 89 "Net-(J5-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 90 "Net-(J5-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 91 "Net-(J5-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 92 "Net-(J5-Pad40)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (offset (xyz 1.269999980926514 -24.12999963760376 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Sockets:PLCC44 (layer F.Cu) (tedit 0)
    (at 59.3242 77.7519 270)
    (descr "Support Plcc 44 pins, pads ronds")
    (tags PLCC)
    (fp_text reference U2 (at 13.97 -1.27) (layer F.SilkS))
    (fp_text value XC9536PC44 (at -2.54 0) (layer F.Fab))
    (pad 1 thru_hole rect (at -6.35 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 71 MCU18))
    (pad 2 thru_hole circle (at -8.89 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 72 MCU17))
    (pad 3 thru_hole circle (at -6.35 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 73 DISHOLD))
    (pad 4 thru_hole circle (at -8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 /D6))
    (pad 5 thru_hole circle (at -6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 /D7))
    (pad 6 thru_hole circle (at -8.89 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 94 "Net-(U2-Pad6)"))
    (pad 7 thru_hole circle (at -6.35 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 95 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at -6.35 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 /D5))
    (pad 9 thru_hole circle (at -3.81 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 /D4))
    (pad 10 thru_hole circle (at -3.81 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 11 thru_hole circle (at -1.27 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 /D3))
    (pad 12 thru_hole circle (at -1.27 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 74 RES))
    (pad 13 thru_hole circle (at 1.27 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 49 8080HOLD))
    (pad 14 thru_hole circle (at 1.27 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at 3.81 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 56 "Net-(J1-Pad4)"))
    (pad 16 thru_hole circle (at 3.81 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 57 "Net-(J1-Pad5)"))
    (pad 17 thru_hole circle (at 6.35 8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 54 "Net-(J1-Pad2)"))
    (pad 18 thru_hole circle (at 8.89 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 82 "Net-(J5-Pad25)"))
    (pad 19 thru_hole circle (at 6.35 6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 90 "Net-(J5-Pad37)"))
    (pad 20 thru_hole circle (at 8.89 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad17)"))
    (pad 21 thru_hole circle (at 6.35 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 22 thru_hole circle (at 8.89 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad23)"))
    (pad 23 thru_hole circle (at 6.35 1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 24 thru_hole circle (at 8.89 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad18)"))
    (pad 25 thru_hole circle (at 6.35 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 83 "Net-(J5-Pad27)"))
    (pad 26 thru_hole circle (at 8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 86 "Net-(J5-Pad33)"))
    (pad 27 thru_hole circle (at 6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 89 "Net-(J5-Pad36)"))
    (pad 28 thru_hole circle (at 8.89 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 88 "Net-(J5-Pad35)"))
    (pad 29 thru_hole circle (at 6.35 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad19)"))
    (pad 30 thru_hole circle (at 6.35 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 55 "Net-(J1-Pad3)"))
    (pad 31 thru_hole circle (at 3.81 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 32 thru_hole circle (at 3.81 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 33 thru_hole circle (at 1.27 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 /D0))
    (pad 34 thru_hole circle (at 1.27 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 /D1))
    (pad 35 thru_hole circle (at -1.27 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 51 CLKMON))
    (pad 36 thru_hole circle (at -1.27 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 50 DISINT))
    (pad 37 thru_hole circle (at -3.81 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 48 RESCDIV))
    (pad 38 thru_hole circle (at -3.81 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 /D2))
    (pad 39 thru_hole circle (at -6.35 -8.89 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 47 MCU39))
    (pad 40 thru_hole circle (at -8.89 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 46 RESb))
    (pad 41 thru_hole circle (at -6.35 -6.35 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 42 thru_hole circle (at -8.89 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 52 SP1))
    (pad 43 thru_hole circle (at -6.35 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 69 MCU20))
    (pad 44 thru_hole circle (at -8.89 -1.27 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 70 MCU19))
  )
  (gr_text + (at 67.99072 60.17514) (layer F.SilkS))
  (gr_text + (at 51.69408 64.80302) (layer F.SilkS))
  (gr_text + (at 46.35246 59.92114) (layer F.SilkS))
  (gr_text "Design © R.Grieb / Tauntek" (at 48.12284 107.2769 90) (layer F.SilkS))
  (gr_text "8080\nICE" (at 88.011 72.3265) (layer F.SilkS))
  (gr_text TaunTek (at 92.45092 69.41058) (layer F.SilkS))
  (gr_line (start 14.8971 119.70004) (end 14.8971 59.1947) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 98.70694 119.70004) (end 14.86154 119.70004) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 98.6917 59.1947) (end 98.6917 119.70004) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 14.8971 59.1947) (end 98.6917 59.1947) (layer Edge.Cuts) (width 0.2))
  (gr_text "JonB Retro" (at 92.62564 66.78414) (layer F.SilkS))
)
