(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 116)
    (zones 0)
    (modules 8)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 1.6)
    (via_drill 0.6)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.7 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x310f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.200000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../Gerber/"))
  )
  (net 0 "")
  (net 1 /TRG_PWR)
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 /DSP_RST_BUF)
  (net 6 /SCL_BUF)
  (net 7 /SDA_BUF)
  (net 8 /DSP_RESET)
  (net 9 /PROG_EN)
  (net 10 "Net-(R1-Pad1)")
  (net 11 "Net-(U2-Pad1)")
  (net 12 "Net-(U2-Pad2)")
  (net 13 "Net-(U2-Pad3)")
  (net 14 "Net-(U2-Pad5)")
  (net 15 "Net-(U2-Pad7)")
  (net 16 "Net-(U2-Pad8)")
  (net 17 "Net-(U2-Pad12)")
  (net 18 "Net-(U2-Pad15)")
  (net 19 "Net-(U2-Pad16)")
  (net 20 "Net-(U2-Pad17)")
  (net 21 "Net-(U2-Pad18)")
  (net 22 "Net-(U2-Pad19)")
  (net 23 "Net-(U2-Pad20)")
  (net 24 "Net-(U2-Pad21)")
  (net 25 "Net-(U2-Pad22)")
  (net 26 "Net-(U2-Pad23)")
  (net 27 "Net-(U2-Pad24)")
  (net 28 "Net-(U2-Pad25)")
  (net 29 "Net-(U2-Pad26)")
  (net 30 "Net-(U2-Pad27)")
  (net 31 "Net-(U2-Pad30)")
  (net 32 "Net-(U2-Pad31)")
  (net 33 "Net-(U2-Pad32)")
  (net 34 "Net-(U2-Pad33)")
  (net 35 "Net-(U2-Pad34)")
  (net 36 "Net-(U2-Pad35)")
  (net 37 "Net-(U2-Pad36)")
  (net 38 "Net-(U2-Pad37)")
  (net 39 "Net-(U2-Pad38)")
  (net 40 "Net-(U2-Pad39)")
  (net 41 "Net-(U2-Pad40)")
  (net 42 "Net-(U1-Pad8)")
  (net 43 "Net-(U1-Pad10)")
  (net 44 "Net-(U2-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.3)
    (via_dia 1.6)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DSP_RESET)
    (add_net /DSP_RST_BUF)
    (add_net /PROG_EN)
    (add_net /SCL_BUF)
    (add_net /SDA_BUF)
    (add_net /TRG_PWR)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad33)")
    (add_net "Net-(U2-Pad34)")
    (add_net "Net-(U2-Pad35)")
    (add_net "Net-(U2-Pad36)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad40)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
  )
  (module Pin_Headers:Pin_Header_Angled_1x05 (layer F.Cu) (tedit 55D0DB70)
    (at 183.79 135.5 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.5 -0.09 270) (layer F.SilkS) hide)
    (fp_text value PROG_BUF (at 2.6 14.79) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 2.032 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SDA_BUF))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL_BUF))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 /DSP_RST_BUF))
    (pad 5 thru_hole rect (at 0 10.16 270) (size 2.032 1.7272) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 /TRG_PWR))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x05.wrl
      (offset (xyz 0 -5.079999923706055 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module H_dev_kits:CY7C68013A_dev_kit (layer F.Cu) (tedit 55C8DFE3)
    (at 165 109.25)
    (fp_text reference U2 (at -3.302 -19.304) (layer F.SilkS) hide)
    (fp_text value CY7C68013A_dev_kit (at 3.048 -17.399) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(U2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U2-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U2-Pad3)"))
    (pad 4 thru_hole circle (at 2.54 2.54) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole circle (at 0 5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U2-Pad5)"))
    (pad 6 thru_hole circle (at 2.54 5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole circle (at 0 7.62) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at 2.54 7.62) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U2-Pad8)"))
    (pad 9 thru_hole circle (at 0 10.16) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole circle (at 2.54 10.16) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U2-Pad10)"))
    (pad 11 thru_hole circle (at 0 12.7) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.8 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U2-Pad12)"))
    (pad 13 thru_hole circle (at 0 15.24) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(U1-Pad10)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.8 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U1-Pad8)"))
    (pad 15 thru_hole circle (at 0 17.78) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U2-Pad15)"))
    (pad 16 thru_hole circle (at 2.54 17.78) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U2-Pad16)"))
    (pad 17 thru_hole circle (at 0 20.32) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U2-Pad17)"))
    (pad 18 thru_hole circle (at 2.54 20.32) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U2-Pad18)"))
    (pad 19 thru_hole circle (at 0 22.86) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U2-Pad19)"))
    (pad 20 thru_hole circle (at 2.54 22.86) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U2-Pad20)"))
    (pad 21 thru_hole circle (at 30.48 22.86) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U2-Pad21)"))
    (pad 22 thru_hole circle (at 27.94 22.86) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U2-Pad22)"))
    (pad 23 thru_hole circle (at 30.48 20.32) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U2-Pad23)"))
    (pad 24 thru_hole circle (at 27.94 20.32) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U2-Pad24)"))
    (pad 25 thru_hole circle (at 30.48 17.78) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U2-Pad25)"))
    (pad 26 thru_hole circle (at 27.94 17.78) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U2-Pad26)"))
    (pad 27 thru_hole oval (at 30.48 15.24) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U2-Pad27)"))
    (pad 28 thru_hole oval (at 27.94 15.24) (size 1.8 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 /PROG_EN))
    (pad 29 thru_hole circle (at 30.48 12.7) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 8 /DSP_RESET))
    (pad 30 thru_hole oval (at 27.94 12.7) (size 1.8 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U2-Pad30)"))
    (pad 31 thru_hole circle (at 30.48 10.16) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U2-Pad31)"))
    (pad 32 thru_hole circle (at 27.94 10.16) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U2-Pad32)"))
    (pad 33 thru_hole circle (at 30.48 7.62) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U2-Pad33)"))
    (pad 34 thru_hole circle (at 27.94 7.62) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U2-Pad34)"))
    (pad 35 thru_hole circle (at 30.48 5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U2-Pad35)"))
    (pad 36 thru_hole circle (at 27.94 5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U2-Pad36)"))
    (pad 37 thru_hole circle (at 30.48 2.54) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U2-Pad37)"))
    (pad 38 thru_hole circle (at 27.94 2.54) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U2-Pad38)"))
    (pad 39 thru_hole circle (at 30.48 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U2-Pad39)"))
    (pad 40 thru_hole circle (at 27.94 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U2-Pad40)"))
  )
  (module Sockets_DIP:DIP-14__300_ELL (layer F.Cu) (tedit 55D0DB3C)
    (at 183.711746 118.016521 90)
    (descr "14 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U1 (at -10.983479 2.288254 180) (layer F.SilkS))
    (fp_text value 74LV4066 (at 1.27 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -7.62 3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at -5.08 3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at -2.54 3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(R1-Pad1)"))
    (pad 4 thru_hole oval (at 0 3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /DSP_RESET))
    (pad 5 thru_hole oval (at 2.54 3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /PROG_EN))
    (pad 6 thru_hole oval (at 5.08 3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /PROG_EN))
    (pad 7 thru_hole oval (at 7.62 3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole oval (at 7.62 -3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U1-Pad8)"))
    (pad 9 thru_hole oval (at 5.08 -3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SDA_BUF))
    (pad 10 thru_hole oval (at 2.54 -3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(U1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL_BUF))
    (pad 12 thru_hole oval (at -2.54 -3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /PROG_EN))
    (pad 13 thru_hole oval (at -5.08 -3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /PROG_EN))
    (pad 14 thru_hole oval (at -7.62 -3.81 90) (size 1.5748 2.286) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /TRG_PWR))
    (model Sockets_DIP.3dshapes/DIP-14__300_ELL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module H_LEDs:Diode_LED_3mm_round_vertical (layer F.Cu) (tedit 55CF08B9)
    (at 189.5 135.5 180)
    (descr "Leuchtdiode, LED, 3mm, round, rund,  vertical,")
    (tags "Leuchtdiode, LED,  3mm, round, rund,  vertical,")
    (fp_text reference D1 (at -1 -2.25 180) (layer F.SilkS))
    (fp_text value LED (at 0 2.25 180) (layer F.Fab))
    (fp_text user + (at -2.286 -1.524 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad2)"))
    (model I:/Electronics/Projects/Hardware/kicad_libs/3d_models/leds/led_3mm_clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 55CF08DA)
    (at 177.25 129)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 0.75 -2) (layer F.SilkS))
    (fp_text value 100n (at 1.25 0.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /TRG_PWR))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.7 1.7) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (offset (xyz 1.250000021226883 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 55D0DBED)
    (at 174.5 125.19 270)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at -1.75 -2) (layer F.SilkS))
    (fp_text value 330R (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /DSP_RST_BUF))
    (model Resistors_ThroughHole.3dshapes/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 55C85B6B)
    (at 181.06 132)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 0.69 -1.75) (layer F.SilkS))
    (fp_text value 2k2 (at 0 0.025) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /TRG_PWR))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 55C89B40)
    (at 190.25 114.25 90)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R3 (at 5.65 -0.05 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /PROG_EN))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 165.25 110.5) (end 162.25 110.5) (angle 90) (layer Edge.Cuts) (width 0.8))
  (gr_arc (start 195.25 110.5) (end 195.25 107.5) (angle 90) (layer Edge.Cuts) (width 0.8))
  (gr_arc (start 195.25 136.5) (end 198.25 136.5) (angle 90) (layer Edge.Cuts) (width 0.8))
  (gr_arc (start 165.25 136.5) (end 165.25 139.5) (angle 90) (layer Edge.Cuts) (width 0.8))
  (dimension 11 (width 0.3) (layer Dwgs.User)
    (gr_text "11,000 mm" (at 195 140.9) (layer Dwgs.User))
    (feature1 (pts (xy 189.5 146) (xy 189.5 139.55)))
    (feature2 (pts (xy 200.5 146) (xy 200.5 139.55)))
    (crossbar (pts (xy 200.5 142.25) (xy 189.5 142.25)))
    (arrow1a (pts (xy 189.5 142.25) (xy 190.626504 141.663579)))
    (arrow1b (pts (xy 189.5 142.25) (xy 190.626504 142.836421)))
    (arrow2a (pts (xy 200.5 142.25) (xy 199.373496 141.663579)))
    (arrow2b (pts (xy 200.5 142.25) (xy 199.373496 142.836421)))
  )
  (gr_text "(c) 2015 www.hexeguitar.com" (at 180 137.75) (layer B.SilkS))
  (gr_text "EZ-USB FX2LP" (at 169.85 113.9 90) (layer B.SilkS))
  (gr_text "CY7C68013A MINI BOARD" (at 171.45 117.7 90) (layer B.SilkS))
  (gr_text "I2C EEPROM\nBURNER" (at 173.75 114) (layer F.SilkS))
  (gr_text RST (at 170.5 131) (layer F.SilkS))
  (gr_text SCL (at 178.75 133.65) (layer F.SilkS))
  (gr_text SDA (at 181.25 133.65) (layer F.SilkS))
  (gr_text "TRG PWR" (at 172 132.25) (layer F.SilkS))
  (gr_text GND (at 183.75 133.65) (layer F.SilkS))
  (gr_text USB (at 172.75 109.5) (layer F.SilkS))
  (dimension 32 (width 0.3) (layer Dwgs.User)
    (gr_text "32,000 mm" (at 155.15 123.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 159.25 107.5) (xy 153.8 107.5)))
    (feature2 (pts (xy 159.25 139.5) (xy 153.8 139.5)))
    (crossbar (pts (xy 156.5 139.5) (xy 156.5 107.5)))
    (arrow1a (pts (xy 156.5 107.5) (xy 157.086421 108.626504)))
    (arrow1b (pts (xy 156.5 107.5) (xy 155.913579 108.626504)))
    (arrow2a (pts (xy 156.5 139.5) (xy 157.086421 138.373496)))
    (arrow2b (pts (xy 156.5 139.5) (xy 155.913579 138.373496)))
  )
  (dimension 36 (width 0.3) (layer Dwgs.User)
    (gr_text "36,000 mm" (at 180.25 148.849999) (layer Dwgs.User))
    (feature1 (pts (xy 198.25 140) (xy 198.25 150.199999)))
    (feature2 (pts (xy 162.25 140) (xy 162.25 150.199999)))
    (crossbar (pts (xy 162.25 147.499999) (xy 198.25 147.499999)))
    (arrow1a (pts (xy 198.25 147.499999) (xy 197.123496 148.08642)))
    (arrow1b (pts (xy 198.25 147.499999) (xy 197.123496 146.913578)))
    (arrow2a (pts (xy 162.25 147.499999) (xy 163.376504 148.08642)))
    (arrow2b (pts (xy 162.25 147.499999) (xy 163.376504 146.913578)))
  )
  (gr_line (start 162.25 110.5) (end 162.25 136.5) (layer Edge.Cuts) (width 0.8))
  (gr_line (start 195.25 107.5) (end 165.25 107.5) (layer Edge.Cuts) (width 0.8))
  (gr_line (start 198.25 136.5) (end 198.25 110.5) (layer Edge.Cuts) (width 0.8))
  (gr_line (start 165.25 139.5) (end 195.25 139.5) (layer Edge.Cuts) (width 0.8))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.28))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.28) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 159.25 107.5) (xy 200.5 107.5) (xy 200.5 139.5) (xy 159.25 139.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.28))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.28) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 159.25 107.5) (xy 200.5 107.5) (xy 200.5 139.5) (xy 159.25 139.5)
      )
    )
  )
)
