(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 15)
    (zones 0)
    (modules 5)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.127)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.254)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VBUS)
  (net 2 /ID)
  (net 3 /GND)
  (net 4 /D-)
  (net 5 /D+)
  (net 6 "Net-(J2-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.254)
    (add_net /D+)
    (add_net /D-)
    (add_net /ID)
    (add_net "Net-(D1-Pad2)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.254)
    (add_net /GND)
    (add_net /VBUS)
    (add_net "Net-(J2-Pad1)")
  )
  (module kicad_custom:GCT_USB3150-30-130-A (layer F.Cu) (tedit 605B9919)
    (at 182.88 74.93 180)
    (fp_text reference J1 (at 0.445 -3.889) (layer F.SilkS) hide)
    (fp_text value USB3150-30-130-A (at 1.27 -2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.3 -0.65 180) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 1 /VBUS))
    (pad 2 thru_hole circle (at -0.65 0 180) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 4 /D-))
    (pad 3 thru_hole circle (at 0 -0.65 180) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 5 /D+))
    (pad 4 thru_hole circle (at 0.65 0 180) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 2 /ID))
    (pad 5 thru_hole circle (at 1.3 -0.65 180) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad S3 thru_hole circle (at -1.5 0.93 180) (size 0.79 0.79) (drill 0.55) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad S4 thru_hole circle (at 1.5 0.93 180) (size 0.79 0.79) (drill 0.55) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad S2 thru_hole circle (at 1.5 -1.57 180) (size 0.79 0.79) (drill 0.55) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad S1 thru_hole circle (at -1.5 -1.57 180) (size 0.79 0.79) (drill 0.55) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad S5 thru_hole circle (at -3.325 -0.03 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad S6 thru_hole circle (at 3.325 -0.03 180) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad None np_thru_hole circle (at -2.8 -1.07 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 2.8 -1.07 180) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (model C:/Users/jerem/Documents/kicad_custom/USB3150-30-130-A.step
      (offset (xyz 0 0.4 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 180 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 187.96 80.01 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x05_Female (at 2.54 5.08 180) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /D-))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /D+))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /ID))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_1812_4532Metric_Pad1.30x3.40mm_HandSolder (layer F.Cu) (tedit 5F68FEF1)
    (at 190.5 73.66 90)
    (descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (attr smd)
    (fp_text reference TH1 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 1812L110/33MR (at 3.81 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.225 0 90) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 6 "Net-(J2-Pad1)"))
    (pad 2 smd roundrect (at 2.225 0 90) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 1 /VBUS))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEF1)
    (at 175.26 74.93 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.905) (layer F.SilkS))
    (fp_text value LTST-C190KRKT (at 7.62 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /GND))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEF1)
    (at 175.26 72.39 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.905) (layer F.SilkS))
    (fp_text value 150 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /VBUS))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "5W MAX" (at 182.88 71.12) (layer B.SilkS))
  (gr_text "micro usb" (at 182.88 67.31) (layer F.SilkS))
  (gr_circle (center 182.88 76.2) (end 193.04 81.28) (layer Edge.Cuts) (width 0.05))
  (gr_text "for steeb" (at 182.88 67.31) (layer B.SilkS))
  (gr_text "synack 2021" (at 182.88 68.58) (layer F.SilkS))
  (gr_text ID (at 180.34 82.55 270) (layer F.SilkS))
  (gr_text D- (at 185.42 82.55 270) (layer F.SilkS))
  (gr_text D+ (at 182.88 82.55 270) (layer F.SilkS))
  (gr_text GND (at 177.8 82.55 90) (layer B.SilkS))
  (gr_text +5V (at 187.96 82.55 90) (layer B.SilkS))
  (gr_text +5V (at 187.96 82.55 -90) (layer F.SilkS))
  (gr_text GND (at 177.8 82.55 -90) (layer F.SilkS))
  (zone (net 1) (net_name /VBUS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.58 88.9) (xy 170.18 88.9) (xy 170.18 63.5) (xy 195.58 63.5)
      )
    )
  )
  (zone (net 3) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.58 88.9) (xy 170.18 88.9) (xy 170.18 63.5) (xy 195.58 63.5)
      )
    )
  )
)
