(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(3 "In3.Cu" signal)
		(4 "In4.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 0.535)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In3.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 4"
				(type "core")
				(thickness 0.535)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In4.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 5"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(IC1-NC_9-Pad15)")
	(net 2 "unconnected-(IC1-NC_4-Pad4)")
	(net 3 "unconnected-(IC1-NC_8-Pad14)")
	(net 4 "unconnected-(IC1-NC_7-Pad13)")
	(net 5 "unconnected-(IC1-NC_11-Pad17)")
	(net 6 "unconnected-(IC1-NC_1-Pad1)")
	(net 7 "unconnected-(IC1-NC_2-Pad2)")
	(net 8 "unconnected-(IC1-NC_3-Pad3)")
	(net 9 "unconnected-(IC1-NC_10-Pad16)")
	(net 10 "unconnected-(IC1-NC_12-Pad18)")
	(net 11 "unconnected-(IC1-NC_5-Pad5)")
	(net 12 "unconnected-(IC1-NC_6-Pad6)")
	(net 13 "unconnected-(J1-PadP1)")
	(net 14 "unconnected-(J1-PadP2)")
	(net 15 "Net-(IC1-VSSA)")
	(net 16 "Net-(IC1-MSEL)")
	(net 17 "Net-(IC1-M1)")
	(net 18 "Net-(IC1-M3)")
	(net 19 "Net-(IC1-VDD)")
	(net 20 "Net-(IC1-VDDA)")
	(net 21 "Net-(IC1-VSS_2)")
	(net 22 "Net-(IC1-VSS_1)")
	(net 23 "Net-(IC1-M0)")
	(net 24 "Net-(IC1-I)")
	(net 25 "Net-(IC1-M2)")
	(net 26 "Net-(IC1-B)")
	(net 27 "Net-(IC1-A)")
	(footprint "SamacSys_Parts:QFN50P400X400X100-25N-D"
		(layer "F.Cu")
		(at 140.8365 92.0515)
		(descr "QFN 24 leads, 4 mm × 4 mm")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 0 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "AEAT-9922-Q24"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "SamacSys_Parts:QFN50P400X400X100-25N-D"
			(at 0 -6 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/AEAT-9922-Programmable-Angular-Magnetic-Encoder-IC-DS"
			(at 0 -6 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Rotary Encoder Magnetic Programmable PWM"
			(at 0 -6 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Broadcom Pi"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AEAT-9922-Q24"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "encoder.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.95 -7.25 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "unconnected-(IC1-NC_1-Pad1)")
			(pinfunction "NC_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.95 -6.75 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(IC1-NC_2-Pad2)")
			(pinfunction "NC_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.95 -6.25 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(IC1-NC_3-Pad3)")
			(pinfunction "NC_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.95 -5.75 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "unconnected-(IC1-NC_4-Pad4)")
			(pinfunction "NC_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.95 -5.25 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(IC1-NC_5-Pad5)")
			(pinfunction "NC_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -1.95 -4.75 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "unconnected-(IC1-NC_6-Pad6)")
			(pinfunction "NC_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -1.25 -4.05)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(IC1-VDDA)")
			(pinfunction "VDDA")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -0.75 -4.05)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(IC1-VSSA)")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -0.25 -4.05)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(IC1-M0)")
			(pinfunction "M0")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.25 -4.05)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(IC1-M1)")
			(pinfunction "M1")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 0.75 -4.05)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(IC1-M2)")
			(pinfunction "M2")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 1.25 -4.05)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(IC1-M3)")
			(pinfunction "M3")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 1.95 -4.75 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "unconnected-(IC1-NC_7-Pad13)")
			(pinfunction "NC_7")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 1.95 -5.25 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "unconnected-(IC1-NC_8-Pad14)")
			(pinfunction "NC_8")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 1.95 -5.75 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "unconnected-(IC1-NC_9-Pad15)")
			(pinfunction "NC_9")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 1.95 -6.25 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "unconnected-(IC1-NC_10-Pad16)")
			(pinfunction "NC_10")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 1.95 -6.75 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "unconnected-(IC1-NC_11-Pad17)")
			(pinfunction "NC_11")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 1.95 -7.25 90)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "unconnected-(IC1-NC_12-Pad18)")
			(pinfunction "NC_12")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 1.25 -7.95)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(IC1-MSEL)")
			(pinfunction "MSEL")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 0.75 -7.95)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(IC1-I)")
			(pinfunction "I")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 0.25 -7.95)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(IC1-VDD)")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at -0.25 -7.95)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(IC1-VSS_1)")
			(pinfunction "VSS_1")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at -0.75 -7.95)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(IC1-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at -1.25 -7.95)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(IC1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 0 -6)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(IC1-VSS_2)")
			(pinfunction "VSS_2")
			(pintype "passive")
		)
		(model "C:\\Users\\Rayan\\Documents\\kicadlib\\SamacSys_Parts.3dshapes\\AEAT-9922-Q24.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CON_5020781362_MOL"
		(layer "B.Cu")
		(at 140.9899 86.06 180)
		(tags "5020781362 ")
		(property "Reference" "J1"
			(at 0 4.572 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "5020781362"
			(at 0 4.572 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "footprints:CON_5020781362_MOL"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "5020781362"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CON_5020781362_MOL")
		(sheetname "Root")
		(sheetfile "encoder.kicad_sch")
		(attr smd)
		(fp_text user "5020781362"
			(at 0 8.889999 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 4.572 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "5020781362"
			(at 0 8.889999 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.499995 -1.09 180)
			(size 0.25 0.72)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "Net-(IC1-VSSA)")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -1.250059 1.31 180)
			(size 0.25 0.57)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 22 "Net-(IC1-VSS_1)")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -0.999995 -1.09 180)
			(size 0.25 0.72)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "Net-(IC1-VSS_2)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at -0.750059 1.31 180)
			(size 0.25 0.57)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "Net-(IC1-A)")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -0.499995 -1.09 180)
			(size 0.25 0.72)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 26 "Net-(IC1-B)")
			(pinfunction "5")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -0.250059 1.31 180)
			(size 0.25 0.57)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 24 "Net-(IC1-I)")
			(pinfunction "6")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at 0 -1.09 180)
			(size 0.25 0.72)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 16 "Net-(IC1-MSEL)")
			(pinfunction "7")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at 0.249941 1.31 180)
			(size 0.25 0.57)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "Net-(IC1-M3)")
			(pinfunction "8")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at 0.500005 -1.09 180)
			(size 0.25 0.72)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "Net-(IC1-M2)")
			(pinfunction "9")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at 0.749941 1.31 180)
			(size 0.25 0.57)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 17 "Net-(IC1-M1)")
			(pinfunction "10")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at 1.000005 -1.09 180)
			(size 0.25 0.72)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 23 "Net-(IC1-M0)")
			(pinfunction "11")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at 1.249941 1.31 180)
			(size 0.25 0.57)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 19 "Net-(IC1-VDD)")
			(pinfunction "12")
			(pintype "unspecified")
		)
		(pad "13" smd rect
			(at 1.500005 -1.09 180)
			(size 0.25 0.72)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "Net-(IC1-VDDA)")
			(pinfunction "13")
			(pintype "unspecified")
		)
		(pad "P1" smd rect
			(at -2.169996 -0.824999 180)
			(size 0.4 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 13 "unconnected-(J1-PadP1)")
			(pinfunction "P1")
			(pintype "unspecified")
		)
		(pad "P2" smd rect
			(at 2.169996 -0.824999 180)
			(size 0.4 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 14 "unconnected-(J1-PadP2)")
			(pinfunction "P2")
			(pintype "unspecified")
		)
	)
	(gr_circle
		(center 140.91 85.86)
		(end 145.414598 85.86)
		(fill none)
		(layer "Edge.Cuts")
	)
)