<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="13.081" y2="0" width="0" layer="20"/>
<wire x1="13.081" y1="0" x2="13.081" y2="37.465" width="0" layer="20"/>
<wire x1="13.081" y1="37.465" x2="0" y2="37.465" width="0" layer="20"/>
<wire x1="0" y1="37.465" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="Misc Conn">
<packages>
<package name="USB-AB-MICRO-SMD_V03_SMT">
</package>
</packages>
</library>
<library name="ipc-7351-capacitor">
<description>&lt;b&gt;IPC-7351 compliant SMT capacitors&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Symbols copied from CadSoft rcl.lbr&lt;br&gt;
Packages generated using genpkg_chp.ulp, genpkg_cae.ulp and genpkg_mld.ulp&lt;br&gt;
Devices are Vishay chip types, generic AEC types and Kemet T491 series molded body types.&lt;br&gt;
&lt;br&gt;
Weartronics 2006&lt;br&gt;
http://www.weartronics.com/</description>
<packages>
<package name="CAPC1608X92N">
</package>
</packages>
</library>
<library name="Misc Analog">
<packages>
<package name="UQN12">
</package>
</packages>
</library>
<library name="ipc-7351-diode">
<description>&lt;b&gt;IPC-7351 compliant SMT diodes&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Symbols copied from CadSoft diode.lbr.&lt;br&gt;
Packages generated using genpkg_sod.ulp, genpkg_sot.ulp and genpkg_mld.ulp.&lt;br&gt;
Devices are Fairchild Semiconductor types.&lt;br&gt;
&lt;br&gt;
Weartronics 2006&lt;br&gt;
http://www.weartronics.com/</description>
<packages>
<package name="DIOM5436X265N">
</package>
</packages>
</library>
<library name="Misc Power">
<packages>
<package name="SOT95P280X135-3N">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 2.8 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="USB1" library="Misc Conn" package="USB-AB-MICRO-SMD_V03_SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB2" library="Misc Conn" package="USB-AB-MICRO-SMD_V03_SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB3" library="Misc Conn" package="USB-AB-MICRO-SMD_V03_SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="ipc-7351-capacitor" package="CAPC1608X92N" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Misc Analog" package="UQN12" value="NCN9252"/>
<element name="D1" library="ipc-7351-diode" package="DIOM5436X265N" value="MBRS140">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="ipc-7351-diode" package="DIOM5436X265N" value="MBRS140">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="ipc-7351-diode" package="DIOM5436X265N" value="MBRS140">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="Misc Power" package="SOT95P280X135-3N" value="MCP1700/TT">
<attribute name="NAME"/>
</element>
<element name="C2" library="ipc-7351-capacitor" package="CAPC1608X92N" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="ipc-7351-capacitor" package="CAPC1608X92N" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="H2" library="holes" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
</elements>
<signals>
<signal name="GND">
<contactref element="USB1" pad="S1"/>
<contactref element="USB1" pad="S2"/>
<contactref element="USB1" pad="S3"/>
<contactref element="USB1" pad="S4"/>
<contactref element="USB1" pad="GND"/>
<contactref element="USB2" pad="S1"/>
<contactref element="USB2" pad="S2"/>
<contactref element="USB2" pad="S3"/>
<contactref element="USB2" pad="S4"/>
<contactref element="USB2" pad="GND"/>
<contactref element="USB3" pad="S1"/>
<contactref element="USB3" pad="S2"/>
<contactref element="USB3" pad="S3"/>
<contactref element="USB3" pad="S4"/>
<contactref element="USB3" pad="GND"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="9"/>
<contactref element="U2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="H1" pad="B2,8"/>
<contactref element="H2" pad="B2,8"/>
</signal>
<signal name="1D-">
<contactref element="USB1" pad="D-"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="2D-">
<contactref element="USB2" pad="D-"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="3D-">
<contactref element="USB3" pad="D-"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="1D+">
<contactref element="USB1" pad="D+"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="3D+">
<contactref element="USB3" pad="D+"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="2D+">
<contactref element="U1" pad="5"/>
<contactref element="USB2" pad="D+"/>
</signal>
<signal name="VCC">
<contactref element="D1" pad="K"/>
<contactref element="D2" pad="K"/>
<contactref element="D3" pad="K"/>
<contactref element="U2" pad="3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="USB3" pad="VBUS1"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="USB2" pad="VBUS1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="USB1" pad="VBUS1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="+3.3V">
<contactref element="U2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="D-">
<contactref element="U1" pad="10"/>
</signal>
<signal name="D+">
<contactref element="U1" pad="8"/>
</signal>
<signal name="SEL0">
<contactref element="U1" pad="11"/>
</signal>
<signal name="SEL1">
<contactref element="U1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
