<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0.1524" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="73" width="0.1524" layer="20"/>
<wire x1="100" y1="73" x2="0" y2="73" width="0.1524" layer="20"/>
<wire x1="0" y1="73" x2="0" y2="0" width="0.1524" layer="20"/>
<text>Just</text>
<text>Another</text>
<text>Big</text>
<text>Bandwidth</text>
<text>Event</text>
<text>Recorder</text>
<text>With</text>
<text>Oscilloscope</text>
<text>Capabilities</text>
<text>JABBERWOCKY arm7-labrador3-oscilloscope</text>
<text>creative commons by-nc-sa</text>
<text>2008-04 mza</text>
<text>rev00</text>
</plain>
<libraries>
<library name="mza-atmel-microcontrollers">
<packages>
<package name="LQFP-100">
</package>
</packages>
</library>
<library name="mza-test-points">
<packages>
<package name="TEST-POINT-SURFACE-MOUNT-1X1">
</package>
<package name="TEST-POINT-THROUGH-HOLE">
</package>
</packages>
</library>
<library name="mza-linear-technology-voltage-regulators">
<packages>
<package name="SOT-23-6">
</package>
<package name="DFN-14">
</package>
<package name="MSOP-10">
</package>
</packages>
</library>
<library name="mza-discrete-components-surface-mount">
<packages>
<package name="B3U-1000P">
</package>
<package name="0603">
</package>
<package name="0805">
<description>0805 EIA two-terminal surface mount package</description>
</package>
<package name="1005-DIODE-SCHOTTKY">
</package>
</packages>
</library>
<library name="mza-maxim-amplifiers">
<packages>
<package name="SOT-23-5">
</package>
</packages>
</library>
<library name="mza-molex-connectors">
<packages>
<package name="USB-MINI-B-THROUGH-HOLE">
<description>mini usb b through hole connector</description>
</package>
<package name="SMA-SHORT-BARREL-SD-73251-115">
</package>
</packages>
</library>
<library name="mza-fairchild-fets">
<packages>
<package name="SOT-23">
<description>when viewing from the top with the side with the single pin facing 12 o'clock on a clock face, pin 08 = at 8 o'clock, etc</description>
</package>
</packages>
</library>
<library name="mza-kyocera-oscillators">
<packages>
<package name="OSCILLATOR-2.5X2.0">
</package>
</packages>
</library>
<library name="mza-through-hole-connectors">
<packages>
<package name="HEADER-2MM-2X3">
</package>
</packages>
</library>
<library name="mza-bourns-potentiometers">
<packages>
<package name="3313J-1">
</package>
</packages>
</library>
<library name="mza-taiyo-yuden-inductors">
<packages>
<package name="1007">
</package>
</packages>
</library>
<library name="mza-discrete-components-through-hole">
<packages>
<package name="TSL250-BENT">
<description>TSL250 package with the pins bend 90 degrees</description>
</package>
</packages>
</library>
<library name="mza-analog-devices-multiplexers">
<packages>
<package name="TSSOP-16">
</package>
</packages>
</library>
<library name="mza-jst-through-hole-connectors">
<packages>
<package name="S2B-PH-K">
</package>
</packages>
</library>
<library name="mza-panasonic-inductors">
<packages>
<package name="ELL4-M">
</package>
</packages>
</library>
<library name="mza-osram-leds">
<packages>
<package name="0603">
</package>
</packages>
</library>
<library name="mza-UH-IDL">
<packages>
<package name="LQFP-100">
</package>
</packages>
</library>
<library name="mza-omron-connectors">
<packages>
<package name="XF2M-3015-1A-TOP-CONTACTS-IN-USE">
<description>this connector has double-sided contacts; in this case, only the TOP ones are in use</description>
</package>
</packages>
</library>
<library name="mza-coiltronics-inductors">
<packages>
<package name="SD6030">
</package>
</packages>
</library>
<library name="mza-national-semiconductor-voltage-regulators">
<packages>
<package name="SOT-23-5">
</package>
</packages>
</library>
<library name="mza-univision-oled-displays">
<packages>
<package name="OLED-DISPLAY-OUTLINE-UNFURLED">
</package>
</packages>
</library>
<library name="mza-seiko-rtcs">
<packages>
<package name="TSSOP-8">
</package>
</packages>
</library>
<library name="mza-citizen-crystals">
<packages>
<package name="CFS206">
</package>
</packages>
</library>
<library name="mza-texas-instruments-voltage-level-translators">
<packages>
<package name="TSSOP-48">
</package>
</packages>
</library>
<library name="mza-texas-instruments-logic">
<packages>
<package name="SC-70-6">
</package>
<package name="VSSOP-8">
</package>
<package name="SC-70-5">
</package>
</packages>
</library>
<library name="mza-operational-amplifiers">
<packages>
<package name="SOT-23-6">
</package>
</packages>
</library>
<library name="mza-analog-devices-comparators">
<packages>
<package name="SC-70-6">
</package>
</packages>
</library>
<library name="mza-fairchild-multiplexers">
<packages>
<package name="TSSOP-14">
</package>
</packages>
</library>
<library name="mza-diodes">
<packages>
<package name="SOT-23">
<description>when viewing from the top with the side with the single pin facing 12 o'clock on a clock face, pin 08 = at 8 o'clock, etc</description>
</package>
</packages>
</library>
<library name="mza-tdk-inductors">
<packages>
<package name="1210">
</package>
</packages>
</library>
<library name="mza-analog-devices-dacs">
<packages>
<package name="TSSOP-14">
</package>
</packages>
</library>
<library name="mza-screw-holes">
<packages>
<package name="MOUNTING-HOLE-4-40-SHCS">
</package>
</packages>
</library>
<library name="mza-linear-oscillators">
<packages>
<package name="SOT-23-5">
</package>
</packages>
</library>
<library name="mza-panasonic-rotary-encoders">
<packages>
<package name="EVQWK4">
</package>
</packages>
</library>
<library name="mza-nxp-i2c-gpio-extenders">
<packages>
<package name="TSSOP-16">
</package>
<package name="MSOP-8-OR-TSSOP-8">
<description>for the powerpad, put 5 vias from the top to the ground plane for thermal conductivity, and when soldering, fill them with solder</description>
</package>
</packages>
</library>
<library name="mza-texas-instruments-voltage-regulators">
<packages>
<package name="SOT-23-5">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="UC" library="mza-atmel-microcontrollers" package="LQFP-100" value="AT91SAM7A3">
<attribute name="NAME"/>
</element>
<element name="USB" library="mza-molex-connectors" package="USB-MINI-B-THROUGH-HOLE" value="USB-MINI-B"/>
<element name="D+" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1">
<attribute name="NAME"/>
</element>
<element name="D-" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1">
<attribute name="NAME"/>
</element>
<element name="R29" library="mza-discrete-components-surface-mount" package="0603" value="27">
<attribute name="NAME"/>
</element>
<element name="R30" library="mza-discrete-components-surface-mount" package="0603" value="27">
<attribute name="NAME"/>
</element>
<element name="VBUS" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1"/>
<element name="FET1" library="mza-fairchild-fets" package="SOT-23" value="NDS332P"/>
<element name="R33" library="mza-discrete-components-surface-mount" package="0603" value="1.5k">
<attribute name="NAME"/>
</element>
<element name="OSC1" library="mza-kyocera-oscillators" package="OSCILLATOR-2.5X2.0" value="KC2520B-C2"/>
<element name="R6" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="C29" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="JTAG" library="mza-through-hole-connectors" package="HEADER-2MM-2X3" value="HEADER-2MM-2X3-JTAG">
<attribute name="NAME"/>
</element>
<element name="R47" library="mza-discrete-components-surface-mount" package="0603" value="100">
<attribute name="NAME"/>
</element>
<element name="C48" library="mza-discrete-components-surface-mount" package="0603" value="10nF">
<attribute name="NAME"/>
</element>
<element name="C49" library="mza-discrete-components-surface-mount" package="0603" value="2.2nF">
<attribute name="NAME"/>
</element>
<element name="7-18VDC" library="mza-linear-technology-voltage-regulators" package="SOT-23-6" value="LT3461">
<attribute name="NAME"/>
</element>
<element name="U$71" library="mza-maxim-amplifiers" package="SOT-23-5" value="MAX4372">
<attribute name="NAME"/>
</element>
<element name="R18" library="mza-discrete-components-surface-mount" package="0805" value="1">
<attribute name="NAME"/>
</element>
<element name="C32" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C36" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="R31" library="mza-discrete-components-surface-mount" package="0603" value="53.6k">
<attribute name="NAME"/>
</element>
<element name="R32" library="mza-discrete-components-surface-mount" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="C39" library="mza-discrete-components-surface-mount" package="0603" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C40" library="mza-discrete-components-surface-mount" package="0805" value="2.2uF@~18V">
<attribute name="NAME"/>
</element>
<element name="VDISP" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1">
<attribute name="NAME"/>
</element>
<element name="R9" library="mza-bourns-potentiometers" package="3313J-1" value="50k">
<attribute name="NAME"/>
</element>
<element name="R44" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="C42" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R50" library="mza-discrete-components-surface-mount" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="L3" library="mza-taiyo-yuden-inductors" package="1007" value="22uH">
<attribute name="NAME"/>
</element>
<element name="LTV" library="mza-discrete-components-through-hole" package="TSL250-BENT" value="TLS250-BENT"/>
<element name="R34" library="mza-discrete-components-surface-mount" package="0603" value="1.47M">
<attribute name="NAME"/>
</element>
<element name="R35" library="mza-discrete-components-surface-mount" package="0603" value="200k">
<attribute name="NAME"/>
</element>
<element name="R36" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="R37" library="mza-discrete-components-surface-mount" package="0603" value="330k">
<attribute name="NAME"/>
</element>
<element name="R38" library="mza-discrete-components-surface-mount" package="0603" value="330k">
<attribute name="NAME"/>
</element>
<element name="R39" library="mza-discrete-components-surface-mount" package="0603" value="330k">
<attribute name="NAME"/>
</element>
<element name="MPEX" library="mza-analog-devices-multiplexers" package="TSSOP-16" value="ADG728">
<attribute name="NAME"/>
</element>
<element name="ANALOG" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1">
<attribute name="NAME"/>
</element>
<element name="BAT" library="mza-jst-through-hole-connectors" package="S2B-PH-K" value="BATTERY-ON-EXTERNAL-CONNECTOR"/>
<element name="U$72" library="mza-maxim-amplifiers" package="SOT-23-5" value="MAX4372">
<attribute name="NAME"/>
</element>
<element name="R19" library="mza-discrete-components-surface-mount" package="0805" value="0.1">
<attribute name="NAME"/>
</element>
<element name="CHRG" library="mza-linear-technology-voltage-regulators" package="DFN-14" value="LTC4088">
<attribute name="NAME"/>
</element>
<element name="L1" library="mza-panasonic-inductors" package="ELL4-M" value="3.3uH">
<attribute name="NAME"/>
</element>
<element name="CHARGE" library="mza-osram-leds" package="0603" value="LED">
<attribute name="NAME"/>
</element>
<element name="R20" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="R21" library="mza-discrete-components-surface-mount" package="0603" value="100k-thermistor">
<attribute name="NAME"/>
</element>
<element name="R22" library="mza-discrete-components-surface-mount" package="0603" value="8.2">
<attribute name="NAME"/>
</element>
<element name="C10" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R23" library="mza-discrete-components-surface-mount" package="0603" value="2.94k">
<attribute name="NAME"/>
</element>
<element name="R24" library="mza-discrete-components-surface-mount" package="0603" value="499">
<attribute name="NAME"/>
</element>
<element name="C11" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF"/>
<element name="R25" library="mza-discrete-components-surface-mount" package="0603" value="1"/>
<element name="C12" library="mza-discrete-components-surface-mount" package="0805" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C13" library="mza-discrete-components-surface-mount" package="0805" value="10uF"/>
<element name="R26" library="mza-discrete-components-surface-mount" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R27" library="mza-discrete-components-surface-mount" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R28" library="mza-discrete-components-surface-mount" package="0603" value="10k"/>
<element name="C14" library="mza-discrete-components-surface-mount" package="0603" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C19" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C37" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="VOUT" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1">
<attribute name="NAME"/>
</element>
<element name="3.3V-ALWAYS" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1">
<attribute name="NAME"/>
</element>
<element name="VBAT" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1"/>
<element name="LAB3" library="mza-UH-IDL" package="LQFP-100" value="LABRADOR3">
<attribute name="NAME"/>
</element>
<element name="OLED" library="mza-omron-connectors" package="XF2M-3015-1A-TOP-CONTACTS-IN-USE" value="OLED-DISPLAY-CONNECTOR-2TOP-CONTACTS-IN-USE"/>
<element name="C1" library="mza-discrete-components-surface-mount" package="0603" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="mza-discrete-components-surface-mount" package="0603" value="1uF@~10V">
<attribute name="NAME"/>
</element>
<element name="C3" library="mza-discrete-components-surface-mount" package="0603" value="1uF@~10V">
<attribute name="NAME"/>
</element>
<element name="C4" library="mza-discrete-components-surface-mount" package="0603" value="1uF@~10V">
<attribute name="NAME"/>
</element>
<element name="C5" library="mza-discrete-components-surface-mount" package="0805" value="4.7uF@~12V">
<attribute name="NAME"/>
</element>
<element name="R4" library="mza-discrete-components-surface-mount" package="0603" value="1M">
<attribute name="NAME"/>
</element>
<element name="Z1" library="mza-discrete-components-surface-mount" package="0603" value="3.6V">
<attribute name="NAME"/>
</element>
<element name="R5" library="mza-discrete-components-surface-mount" package="0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="C16" library="mza-discrete-components-surface-mount" package="0603" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C28" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="R2" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="R3" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="WAKEUP" library="mza-discrete-components-surface-mount" package="B3U-1000P" value="B3U-1000P">
<attribute name="NAME"/>
</element>
<element name="RESET" library="mza-discrete-components-surface-mount" package="B3U-1000P" value="B3U-1000P">
<attribute name="NAME"/>
</element>
<element name="R7" library="mza-discrete-components-surface-mount" package="0603" value="100k"/>
<element name="R8" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="R10" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="R11" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="R12" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="R13" library="mza-discrete-components-surface-mount" package="0603" value="340k">
<attribute name="NAME"/>
</element>
<element name="R14" library="mza-discrete-components-surface-mount" package="0603" value="200k">
<attribute name="NAME"/>
</element>
<element name="L2" library="mza-coiltronics-inductors" package="SD6030" value="22uH">
<attribute name="NAME"/>
</element>
<element name="C7" library="mza-discrete-components-surface-mount" package="0805" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R15" library="mza-discrete-components-surface-mount" package="0603" value="340k">
<attribute name="NAME"/>
</element>
<element name="R16" library="mza-discrete-components-surface-mount" package="0603" value="200k">
<attribute name="NAME"/>
</element>
<element name="C8" library="mza-discrete-components-surface-mount" package="0603" value="1.5nF">
<attribute name="NAME"/>
</element>
<element name="R17" library="mza-discrete-components-surface-mount" package="0603" value="15k">
<attribute name="NAME"/>
</element>
<element name="3.3VDC" library="mza-linear-technology-voltage-regulators" package="MSOP-10" value="LTC3440">
<attribute name="NAME"/>
</element>
<element name="C9" library="mza-discrete-components-surface-mount" package="0805" value="22uF">
<attribute name="NAME"/>
</element>
<element name="U$70" library="mza-maxim-amplifiers" package="SOT-23-5" value="MAX4372">
<attribute name="NAME"/>
</element>
<element name="R41" library="mza-discrete-components-surface-mount" package="0805" value="0.1"/>
<element name="C33" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C35" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="3.3V" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1"/>
<element name="R45" library="mza-discrete-components-surface-mount" package="0603" value="20k">
<attribute name="NAME"/>
</element>
<element name="C43" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="2.5VDC" library="mza-national-semiconductor-voltage-regulators" package="SOT-23-5" value="LM3670">
<attribute name="NAME"/>
</element>
<element name="U$69" library="mza-maxim-amplifiers" package="SOT-23-5" value="MAX4372">
<attribute name="NAME"/>
</element>
<element name="R40" library="mza-discrete-components-surface-mount" package="0805" value="0.1"/>
<element name="C15" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C17" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="C34" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C38" library="mza-discrete-components-surface-mount" package="0603" value="10uF">
<attribute name="NAME"/>
</element>
<element name="2.5V" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1">
<attribute name="NAME"/>
</element>
<element name="R43" library="mza-discrete-components-surface-mount" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="C41" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="OLED-DISPLAY" library="mza-univision-oled-displays" package="OLED-DISPLAY-OUTLINE-UNFURLED" value="">
<attribute name="NAME"/>
</element>
<element name="RTC" library="mza-seiko-rtcs" package="TSSOP-8" value="S-35390A">
<attribute name="NAME"/>
</element>
<element name="U$41" library="mza-citizen-crystals" package="CFS206" value="CFS206"/>
<element name="C30" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R48" library="mza-discrete-components-surface-mount" package="0603" value="4.7k"/>
<element name="R49" library="mza-discrete-components-surface-mount" package="0603" value="4.7k">
<attribute name="NAME"/>
</element>
<element name="R46" library="mza-discrete-components-surface-mount" package="0603" value="49.9k">
<attribute name="NAME"/>
</element>
<element name="R51" library="mza-discrete-components-surface-mount" package="0603" value="49.9k"/>
<element name="C6" library="mza-discrete-components-surface-mount" package="0603" value="1nF">
<attribute name="NAME"/>
</element>
<element name="R52" library="mza-bourns-potentiometers" package="3313J-1" value="50k">
<attribute name="NAME"/>
</element>
<element name="VRAMP" library="mza-test-points" package="TEST-POINT-SURFACE-MOUNT-1X1" value="TEST-POINTSURFACE-MOUNT-1X1"/>
<element name="FET2" library="mza-fairchild-fets" package="SOT-23" value="NDS331N">
<attribute name="NAME"/>
</element>
<element name="FFA" library="mza-texas-instruments-logic" package="SC-70-6" value="74LVC1G175">
<attribute name="NAME"/>
</element>
<element name="FFB" library="mza-texas-instruments-logic" package="SC-70-6" value="74LVC1G175">
<attribute name="NAME"/>
</element>
<element name="XOR" library="mza-texas-instruments-logic" package="VSSOP-8" value="74LVC2G86">
<attribute name="NAME"/>
</element>
<element name="C18" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="C20" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="C21" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="C22" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="AMP-A" library="mza-operational-amplifiers" package="SOT-23-6" value="OP-AMP-SOT-23-6">
<attribute name="NAME"/>
</element>
<element name="R42" library="mza-discrete-components-surface-mount" package="0603" value="523">
<attribute name="NAME"/>
</element>
<element name="R53" library="mza-discrete-components-surface-mount" package="0603" value="523">
<attribute name="NAME"/>
</element>
<element name="R54" library="mza-discrete-components-surface-mount" package="0603" value="2.1k"/>
<element name="AMP-B" library="mza-operational-amplifiers" package="SOT-23-6" value="OP-AMP-SOT-23-6">
<attribute name="NAME"/>
</element>
<element name="R55" library="mza-discrete-components-surface-mount" package="0603" value="523">
<attribute name="NAME"/>
</element>
<element name="R56" library="mza-discrete-components-surface-mount" package="0603" value="523">
<attribute name="NAME"/>
</element>
<element name="R57" library="mza-discrete-components-surface-mount" package="0603" value="2.1k">
<attribute name="NAME"/>
</element>
<element name="R58" library="mza-discrete-components-surface-mount" package="0603" value="1k">
<attribute name="NAME"/>
</element>
<element name="R59" library="mza-discrete-components-surface-mount" package="0603" value="1k">
<attribute name="NAME"/>
</element>
<element name="R61" library="mza-discrete-components-surface-mount" package="0603" value="953">
<attribute name="NAME"/>
</element>
<element name="R63" library="mza-discrete-components-surface-mount" package="0603" value="953">
<attribute name="NAME"/>
</element>
<element name="R65" library="mza-discrete-components-surface-mount" package="0603" value="953"/>
<element name="R67" library="mza-discrete-components-surface-mount" package="0603" value="953">
<attribute name="NAME"/>
</element>
<element name="R69" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="CMP-A" library="mza-analog-devices-comparators" package="SC-70-6" value="ADCMP601">
<attribute name="NAME"/>
</element>
<element name="R70" library="mza-discrete-components-surface-mount" package="0603" value="100k">
<attribute name="NAME"/>
</element>
<element name="CMP-B" library="mza-analog-devices-comparators" package="SC-70-6" value="ADCMP601">
<attribute name="NAME"/>
</element>
<element name="MPEX-A" library="mza-fairchild-multiplexers" package="TSSOP-14" value="FHP3194"/>
<element name="MPEX-B" library="mza-fairchild-multiplexers" package="TSSOP-14" value="FHP3194">
<attribute name="NAME"/>
</element>
<element name="R71" library="mza-discrete-components-surface-mount" package="0603" value="1.5k">
<attribute name="NAME"/>
</element>
<element name="R72" library="mza-discrete-components-surface-mount" package="0603" value="3.92M">
<attribute name="NAME"/>
</element>
<element name="R73" library="mza-discrete-components-surface-mount" package="0603" value="3.83M">
<attribute name="NAME"/>
</element>
<element name="R74" library="mza-discrete-components-surface-mount" package="0603" value="3.65M">
<attribute name="NAME"/>
</element>
<element name="R75" library="mza-discrete-components-surface-mount" package="0603" value="2.55M">
<attribute name="NAME"/>
</element>
<element name="R76" library="mza-discrete-components-surface-mount" package="0603" value="1.5M">
<attribute name="NAME"/>
</element>
<element name="R77" library="mza-discrete-components-surface-mount" package="0603" value="374k">
<attribute name="NAME"/>
</element>
<element name="R78" library="mza-discrete-components-surface-mount" package="0603" value="187k">
<attribute name="NAME"/>
</element>
<element name="R79" library="mza-discrete-components-surface-mount" package="0603" value="46.4k">
<attribute name="NAME"/>
</element>
<element name="D4" library="mza-diodes" package="SOT-23" value="DIODE-SCHOTTKY-PAIR-ANODE-TO-CATHODE">
<attribute name="NAME"/>
</element>
<element name="D5" library="mza-diodes" package="SOT-23" value="DIODE-SCHOTTKY-PAIR-ANODE-TO-CATHODE"/>
<element name="D6" library="mza-diodes" package="SOT-23" value="DIODE-SCHOTTKY-PAIR-ANODE-TO-CATHODE"/>
<element name="D7" library="mza-diodes" package="SOT-23" value="DIODE-SCHOTTKY-PAIR-ANODE-TO-CATHODE">
<attribute name="NAME"/>
</element>
<element name="R80" library="mza-discrete-components-surface-mount" package="0603" value="1.5k">
<attribute name="NAME"/>
</element>
<element name="R81" library="mza-discrete-components-surface-mount" package="0603" value="3.92M">
<attribute name="NAME"/>
</element>
<element name="R82" library="mza-discrete-components-surface-mount" package="0603" value="3.83M">
<attribute name="NAME"/>
</element>
<element name="R83" library="mza-discrete-components-surface-mount" package="0603" value="3.65M">
<attribute name="NAME"/>
</element>
<element name="R84" library="mza-discrete-components-surface-mount" package="0603" value="2.55M">
<attribute name="NAME"/>
</element>
<element name="R85" library="mza-discrete-components-surface-mount" package="0603" value="1.5M">
<attribute name="NAME"/>
</element>
<element name="R86" library="mza-discrete-components-surface-mount" package="0603" value="374k">
<attribute name="NAME"/>
</element>
<element name="R87" library="mza-discrete-components-surface-mount" package="0603" value="187k">
<attribute name="NAME"/>
</element>
<element name="R88" library="mza-discrete-components-surface-mount" package="0603" value="46.4k">
<attribute name="NAME"/>
</element>
<element name="D8" library="mza-diodes" package="SOT-23" value="DIODE-SCHOTTKY-PAIR-ANODE-TO-CATHODE">
<attribute name="NAME"/>
</element>
<element name="D9" library="mza-diodes" package="SOT-23" value="DIODE-SCHOTTKY-PAIR-ANODE-TO-CATHODE">
<attribute name="NAME"/>
</element>
<element name="D10" library="mza-diodes" package="SOT-23" value="DIODE-SCHOTTKY-PAIR-ANODE-TO-CATHODE"/>
<element name="D11" library="mza-diodes" package="SOT-23" value="DIODE-SCHOTTKY-PAIR-ANODE-TO-CATHODE">
<attribute name="NAME"/>
</element>
<element name="TRIGGER-B" library="mza-osram-leds" package="0603" value="LED">
<attribute name="NAME"/>
</element>
<element name="TRIGGER-A" library="mza-osram-leds" package="0603" value="LED">
<attribute name="NAME"/>
</element>
<element name="R89" library="mza-discrete-components-surface-mount" package="0603" value="750">
<attribute name="NAME"/>
</element>
<element name="R90" library="mza-discrete-components-surface-mount" package="0603" value="750">
<attribute name="NAME"/>
</element>
<element name="L4" library="mza-tdk-inductors" package="1210" value="10uH">
<attribute name="NAME"/>
</element>
<element name="4DACS" library="mza-analog-devices-dacs" package="TSSOP-14" value="AD56X5R">
<attribute name="NAME"/>
</element>
<element name="CH-A" library="mza-molex-connectors" package="SMA-SHORT-BARREL-SD-73251-115" value="SMA-SHORT-BARREL-SD-73251-115"/>
<element name="CH-B" library="mza-molex-connectors" package="SMA-SHORT-BARREL-SD-73251-115" value="SMA-SHORT-BARREL-SD-73251-115"/>
<element name="LEVEL-SHIFT" library="mza-texas-instruments-voltage-level-translators" package="TSSOP-48" value="SN74CB3T16210">
<attribute name="NAME"/>
</element>
<element name="C23" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="C24" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C25" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C26" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C27" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="C31" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="C44" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C45" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C46" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C47" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C50" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C51" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C52" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="U$176" library="mza-screw-holes" package="MOUNTING-HOLE-4-40-SHCS" value=""/>
<element name="U$177" library="mza-screw-holes" package="MOUNTING-HOLE-4-40-SHCS" value=""/>
<element name="U$178" library="mza-screw-holes" package="MOUNTING-HOLE-4-40-SHCS" value=""/>
<element name="U$179" library="mza-screw-holes" package="MOUNTING-HOLE-4-40-SHCS" value=""/>
<element name="C53" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C54" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="C55" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C56" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="OSC2" library="mza-linear-oscillators" package="SOT-23-5" value="LTC6905"/>
<element name="BUF1" library="mza-texas-instruments-logic" package="SC-70-5" value="SN74LVC1G34">
<attribute name="NAME"/>
</element>
<element name="C57" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C58" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R60" library="mza-discrete-components-surface-mount" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="C59" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="ROT1" library="mza-panasonic-rotary-encoders" package="EVQWK4" value="EVQWK4"/>
<element name="ROT2" library="mza-panasonic-rotary-encoders" package="EVQWK4" value="EVQWK4"/>
<element name="R62" library="mza-discrete-components-surface-mount" package="0603" value="750"/>
<element name="C60" library="mza-discrete-components-surface-mount" package="0603" value="6pF">
<attribute name="NAME"/>
</element>
<element name="GPIO2" library="mza-nxp-i2c-gpio-extenders" package="TSSOP-16" value="PCA9554">
<attribute name="NAME"/>
</element>
<element name="C61" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="CAL" library="mza-test-points" package="TEST-POINT-THROUGH-HOLE" value="TEST-POINTTHROUGH-HOLE">
<attribute name="NAME"/>
</element>
<element name="GND" library="mza-test-points" package="TEST-POINT-THROUGH-HOLE" value="TEST-POINTTHROUGH-HOLE"/>
<element name="U$6" library="mza-screw-holes" package="MOUNTING-HOLE-4-40-SHCS" value=""/>
<element name="U$37" library="mza-screw-holes" package="MOUNTING-HOLE-4-40-SHCS" value=""/>
<element name="U$59" library="mza-screw-holes" package="MOUNTING-HOLE-4-40-SHCS" value=""/>
<element name="U$77" library="mza-screw-holes" package="MOUNTING-HOLE-4-40-SHCS" value=""/>
<element name="GPIO3" library="mza-nxp-i2c-gpio-extenders" package="TSSOP-16" value="PCA9554">
<attribute name="NAME"/>
</element>
<element name="C62" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="GPIO1" library="mza-nxp-i2c-gpio-extenders" package="MSOP-8-OR-TSSOP-8" value="PCA9536">
<attribute name="NAME"/>
</element>
<element name="C63" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C64" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF"/>
<element name="C65" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="R64" library="mza-discrete-components-surface-mount" package="0603" value="20k"/>
<element name="R66" library="mza-discrete-components-surface-mount" package="0603" value="10k"/>
<element name="R68" library="mza-discrete-components-surface-mount" package="0603" value="20k"/>
<element name="R91" library="mza-discrete-components-surface-mount" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="L5" library="mza-tdk-inductors" package="1210" value="10uH">
<attribute name="NAME"/>
</element>
<element name="L6" library="mza-tdk-inductors" package="1210" value="10uH">
<attribute name="NAME"/>
</element>
<element name="C66" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF"/>
<element name="R92" library="mza-discrete-components-surface-mount" package="0603" value="30.1k">
<attribute name="NAME"/>
</element>
<element name="D1" library="mza-discrete-components-surface-mount" package="1005-DIODE-SCHOTTKY" value="DIODE-SCHOTTKY1005">
<attribute name="NAME"/>
</element>
<element name="D3" library="mza-discrete-components-surface-mount" package="1005-DIODE-SCHOTTKY" value="DIODE-SCHOTTKY1005">
<attribute name="NAME"/>
</element>
<element name="D2" library="mza-discrete-components-surface-mount" package="1005-DIODE-SCHOTTKY" value="DIODE-SCHOTTKY1005">
<attribute name="NAME"/>
</element>
<element name="C67" library="mza-discrete-components-surface-mount" package="0603" value="100pF">
<attribute name="NAME"/>
</element>
<element name="C68" library="mza-discrete-components-surface-mount" package="0603" value="4.7pF">
<attribute name="NAME"/>
</element>
<element name="C69" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C70" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF"/>
<element name="C71" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="R93" library="mza-discrete-components-surface-mount" package="0603" value="10k"/>
<element name="R94" library="mza-discrete-components-surface-mount" package="0603" value="30.9k">
<attribute name="NAME"/>
</element>
<element name="R95" library="mza-discrete-components-surface-mount" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="+-5VDC" library="mza-linear-technology-voltage-regulators" package="MSOP-10" value="LT1945">
<attribute name="NAME"/>
</element>
<element name="BUTTON-1" library="mza-discrete-components-surface-mount" package="B3U-1000P" value="B3U-1000P">
<attribute name="NAME"/>
</element>
<element name="BUTTON-2" library="mza-discrete-components-surface-mount" package="B3U-1000P" value="B3U-1000P">
<attribute name="NAME"/>
</element>
<element name="C72" library="mza-discrete-components-surface-mount" package="0603" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C73" library="mza-discrete-components-surface-mount" package="0603" value="1uF"/>
<element name="C74" library="mza-discrete-components-surface-mount" package="0603" value="10nF"/>
<element name="1.25VDC" library="mza-texas-instruments-voltage-regulators" package="SOT-23-5" value="TPS731XX">
<attribute name="NAME"/>
</element>
<element name="R96" library="mza-discrete-components-surface-mount" package="0603" value="4.22k"/>
<element name="R97" library="mza-discrete-components-surface-mount" package="0603" value="750"/>
<element name="R98" library="mza-discrete-components-surface-mount" package="0603" value="750"/>
<element name="R99" library="mza-discrete-components-surface-mount" package="0603" value="4.22k"/>
<element name="C75" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C76" library="mza-discrete-components-surface-mount" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C77" library="mza-discrete-components-surface-mount" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="UC" pad="079"/>
<contactref element="UC" pad="075"/>
<contactref element="UC" pad="071"/>
<contactref element="UC" pad="060"/>
<contactref element="UC" pad="039"/>
<contactref element="UC" pad="031"/>
<contactref element="UC" pad="025"/>
<contactref element="UC" pad="016"/>
<contactref element="UC" pad="001"/>
<contactref element="USB" pad="GND"/>
<contactref element="OSC1" pad="2"/>
<contactref element="C29" pad="1"/>
<contactref element="JTAG" pad="5"/>
<contactref element="C49" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="7-18VDC" pad="2"/>
<contactref element="C42" pad="1"/>
<contactref element="U$71" pad="1"/>
<contactref element="C36" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="R50" pad="1"/>
<contactref element="LTV" pad="1"/>
<contactref element="R38" pad="1"/>
<contactref element="R39" pad="1"/>
<contactref element="R37" pad="1"/>
<contactref element="MPEX" pad="16"/>
<contactref element="MPEX" pad="14"/>
<contactref element="MPEX" pad="15"/>
<contactref element="C37" pad="1"/>
<contactref element="U$72" pad="1"/>
<contactref element="CHRG" pad="BOTTOM-PAD"/>
<contactref element="C13" pad="1"/>
<contactref element="BAT" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="R24" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="R28" pad="1"/>
<contactref element="OLED" pad="3"/>
<contactref element="Z1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="LAB3" pad="099"/>
<contactref element="LAB3" pad="097"/>
<contactref element="LAB3" pad="095"/>
<contactref element="LAB3" pad="093"/>
<contactref element="LAB3" pad="091"/>
<contactref element="LAB3" pad="089"/>
<contactref element="LAB3" pad="086"/>
<contactref element="LAB3" pad="085"/>
<contactref element="LAB3" pad="076"/>
<contactref element="LAB3" pad="067"/>
<contactref element="LAB3" pad="059"/>
<contactref element="LAB3" pad="056"/>
<contactref element="LAB3" pad="053"/>
<contactref element="LAB3" pad="046"/>
<contactref element="LAB3" pad="041"/>
<contactref element="LAB3" pad="039"/>
<contactref element="LAB3" pad="028"/>
<contactref element="LAB3" pad="026"/>
<contactref element="LAB3" pad="023"/>
<contactref element="LAB3" pad="003"/>
<contactref element="LAB3" pad="013"/>
<contactref element="RESET" pad="1"/>
<contactref element="WAKEUP" pad="1"/>
<contactref element="3.3VDC" pad="5"/>
<contactref element="R13" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="U$70" pad="1"/>
<contactref element="C35" pad="1"/>
<contactref element="2.5VDC" pad="2"/>
<contactref element="C17" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="U$69" pad="1"/>
<contactref element="C38" pad="1"/>
<contactref element="RTC" pad="4"/>
<contactref element="C30" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="LAB3" pad="044"/>
<contactref element="LAB3" pad="045"/>
<contactref element="FET2" pad="04"/>
<contactref element="C20" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="AMP-A" pad="3"/>
<contactref element="AMP-B" pad="3"/>
<contactref element="LAB3" pad="024"/>
<contactref element="LAB3" pad="019"/>
<contactref element="LAB3" pad="014"/>
<contactref element="LAB3" pad="006"/>
<contactref element="LAB3" pad="001"/>
<contactref element="CMP-A" pad="2"/>
<contactref element="CMP-B" pad="2"/>
<contactref element="R69" pad="1"/>
<contactref element="R70" pad="1"/>
<contactref element="MPEX-A" pad="02"/>
<contactref element="MPEX-A" pad="04"/>
<contactref element="MPEX-A" pad="10"/>
<contactref element="MPEX-B" pad="02"/>
<contactref element="MPEX-B" pad="04"/>
<contactref element="MPEX-B" pad="10"/>
<contactref element="R79" pad="1"/>
<contactref element="R76" pad="1"/>
<contactref element="R77" pad="1"/>
<contactref element="R78" pad="1"/>
<contactref element="R88" pad="1"/>
<contactref element="R85" pad="1"/>
<contactref element="R86" pad="1"/>
<contactref element="R87" pad="1"/>
<contactref element="TRIGGER-A" pad="C"/>
<contactref element="TRIGGER-B" pad="C"/>
<contactref element="LAB3" pad="002"/>
<contactref element="LAB3" pad="007"/>
<contactref element="LAB3" pad="015"/>
<contactref element="LAB3" pad="020"/>
<contactref element="LAB3" pad="025"/>
<contactref element="4DACS" pad="01"/>
<contactref element="4DACS" pad="06"/>
<contactref element="4DACS" pad="08"/>
<contactref element="4DACS" pad="02"/>
<contactref element="4DACS" pad="12"/>
<contactref element="CH-A" pad="GND@1"/>
<contactref element="CH-B" pad="GND@1"/>
<contactref element="LEVEL-SHIFT" pad="48"/>
<contactref element="LEVEL-SHIFT" pad="47"/>
<contactref element="LEVEL-SHIFT" pad="41"/>
<contactref element="LEVEL-SHIFT" pad="32"/>
<contactref element="LEVEL-SHIFT" pad="17"/>
<contactref element="LEVEL-SHIFT" pad="08"/>
<contactref element="C23" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="C47" pad="1"/>
<contactref element="C50" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="C52" pad="1"/>
<contactref element="C53" pad="1"/>
<contactref element="XOR" pad="4"/>
<contactref element="FFB" pad="2"/>
<contactref element="FFA" pad="2"/>
<contactref element="C55" pad="1"/>
<contactref element="C54" pad="1"/>
<contactref element="C56" pad="1"/>
<contactref element="BUF1" pad="3"/>
<contactref element="C57" pad="1"/>
<contactref element="OSC2" pad="2"/>
<contactref element="C58" pad="1"/>
<contactref element="R60" pad="1"/>
<contactref element="C59" pad="1"/>
<contactref element="C60" pad="1"/>
<contactref element="GPIO2" pad="08"/>
<contactref element="GPIO2" pad="01"/>
<contactref element="GPIO2" pad="02"/>
<contactref element="GPIO2" pad="03"/>
<contactref element="C61" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="GPIO3" pad="08"/>
<contactref element="GPIO3" pad="03"/>
<contactref element="C62" pad="1"/>
<contactref element="GPIO3" pad="01"/>
<contactref element="GPIO1" pad="4"/>
<contactref element="C63" pad="1"/>
<contactref element="C65" pad="1"/>
<contactref element="C64" pad="1"/>
<contactref element="ROT1" pad="COM"/>
<contactref element="ROT1" pad="SW1@3"/>
<contactref element="ROT2" pad="SW1@3"/>
<contactref element="ROT2" pad="COM"/>
<contactref element="ROT2" pad="SW1@5"/>
<contactref element="ROT1" pad="SW1@5"/>
<contactref element="+-5VDC" pad="3"/>
<contactref element="+-5VDC" pad="7"/>
<contactref element="+-5VDC" pad="9"/>
<contactref element="R95" pad="2"/>
<contactref element="C71" pad="2"/>
<contactref element="D2" pad="P$2"/>
<contactref element="R93" pad="1"/>
<contactref element="C70" pad="1"/>
<contactref element="C69" pad="1"/>
<contactref element="CH-A" pad="GND@2"/>
<contactref element="CH-A" pad="GND@3"/>
<contactref element="CH-A" pad="GND@4"/>
<contactref element="CH-B" pad="GND@2"/>
<contactref element="CH-B" pad="GND@3"/>
<contactref element="CH-B" pad="GND@4"/>
<contactref element="BUTTON-1" pad="2"/>
<contactref element="BUTTON-2" pad="2"/>
<contactref element="1.25VDC" pad="2"/>
<contactref element="C73" pad="1"/>
<contactref element="C74" pad="1"/>
<contactref element="C72" pad="1"/>
<contactref element="R97" pad="1"/>
<contactref element="R98" pad="2"/>
<contactref element="MPEX-B" pad="11"/>
<contactref element="MPEX-A" pad="11"/>
<contactref element="C76" pad="1"/>
<contactref element="C77" pad="1"/>
<contactref element="C75" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="UC" pad="077"/>
<contactref element="UC" pad="078"/>
<contactref element="UC" pad="100"/>
<contactref element="UC" pad="088"/>
<contactref element="UC" pad="061"/>
<contactref element="UC" pad="038"/>
<contactref element="UC" pad="015"/>
<contactref element="FET1" pad="04"/>
<contactref element="OSC1" pad="4"/>
<contactref element="R6" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="JTAG" pad="6"/>
<contactref element="C36" pad="2"/>
<contactref element="U$71" pad="3"/>
<contactref element="LTV" pad="2"/>
<contactref element="MPEX" pad="02"/>
<contactref element="C37" pad="2"/>
<contactref element="U$72" pad="3"/>
<contactref element="OLED" pad="27"/>
<contactref element="OLED" pad="4"/>
<contactref element="C16" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R41" pad="2"/>
<contactref element="U$70" pad="4"/>
<contactref element="3.3V" pad="1"/>
<contactref element="U$70" pad="3"/>
<contactref element="C35" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="U$69" pad="3"/>
<contactref element="R49" pad="2"/>
<contactref element="R48" pad="2"/>
<contactref element="FFB" pad="3"/>
<contactref element="FFA" pad="3"/>
<contactref element="C18" pad="2"/>
<contactref element="CMP-A" pad="6"/>
<contactref element="CMP-B" pad="6"/>
<contactref element="4DACS" pad="03"/>
<contactref element="4DACS" pad="09"/>
<contactref element="C25" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C53" pad="2"/>
<contactref element="FFA" pad="5"/>
<contactref element="XOR" pad="8"/>
<contactref element="FFB" pad="5"/>
<contactref element="C56" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="C55" pad="2"/>
<contactref element="OSC2" pad="1"/>
<contactref element="OSC2" pad="4"/>
<contactref element="C58" pad="2"/>
<contactref element="C59" pad="2"/>
<contactref element="GPIO2" pad="16"/>
<contactref element="C61" pad="2"/>
<contactref element="GPIO3" pad="16"/>
<contactref element="C62" pad="2"/>
<contactref element="GPIO3" pad="02"/>
<contactref element="GPIO1" pad="8"/>
</signal>
<signal name="1.8V">
<contactref element="UC" pad="017"/>
<contactref element="UC" pad="099"/>
<contactref element="UC" pad="059"/>
<contactref element="UC" pad="040"/>
<contactref element="UC" pad="072"/>
<contactref element="C20" pad="2"/>
</signal>
<signal name="VDISPLAY">
<contactref element="R18" pad="2"/>
<contactref element="U$71" pad="4"/>
<contactref element="VDISP" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="OLED" pad="29"/>
<contactref element="OLED" pad="2"/>
</signal>
<signal name="+V">
<contactref element="7-18VDC" pad="6"/>
<contactref element="C32" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="L3" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="U$72" pad="4"/>
<contactref element="VOUT" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="3.3VDC" pad="7"/>
<contactref element="C33" pad="2"/>
<contactref element="2.5VDC" pad="1"/>
<contactref element="C17" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="RTC" pad="8"/>
<contactref element="C30" pad="2"/>
<contactref element="+-5VDC" pad="8"/>
<contactref element="L5" pad="1"/>
<contactref element="L6" pad="1"/>
<contactref element="C69" pad="2"/>
</signal>
<signal name="VDISPLAY-CURRENT">
<contactref element="U$71" pad="2"/>
<contactref element="MPEX" pad="10"/>
</signal>
<signal name="VBUS">
<contactref element="USB" pad="VBUS"/>
<contactref element="VBUS" pad="1"/>
<contactref element="R35" pad="2"/>
<contactref element="CHRG" pad="11"/>
<contactref element="R20" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="VBATTERY">
<contactref element="R36" pad="2"/>
<contactref element="CHRG" pad="09"/>
<contactref element="BAT" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="VBAT" pad="1"/>
</signal>
<signal name="3.3V-ALWAYS">
<contactref element="UC" pad="026"/>
<contactref element="MPEX" pad="13"/>
<contactref element="C14" pad="2"/>
<contactref element="CHRG" pad="03"/>
<contactref element="3.3V-ALWAYS" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R62" pad="2"/>
</signal>
<signal name="N$72">
<contactref element="R29" pad="2"/>
<contactref element="USB" pad="D+"/>
<contactref element="D+" pad="1"/>
</signal>
<signal name="N$73">
<contactref element="USB" pad="D-"/>
<contactref element="R30" pad="2"/>
<contactref element="D-" pad="1"/>
</signal>
<signal name="N$74">
<contactref element="R29" pad="1"/>
<contactref element="UC" pad="098"/>
</signal>
<signal name="N$75">
<contactref element="R30" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="UC" pad="097"/>
</signal>
<signal name="N$48">
<contactref element="FET1" pad="12"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="VOUT-CURRENT">
<contactref element="MPEX" pad="07"/>
<contactref element="U$72" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="OSC1" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="MAIN_OSCILLATOR">
<contactref element="OSC1" pad="3"/>
<contactref element="UC" pad="074"/>
</signal>
<signal name="N$76">
<contactref element="JTAG" pad="1"/>
<contactref element="UC" pad="068"/>
</signal>
<signal name="N$77">
<contactref element="JTAG" pad="2"/>
<contactref element="UC" pad="067"/>
</signal>
<signal name="N$79">
<contactref element="JTAG" pad="3"/>
<contactref element="UC" pad="070"/>
</signal>
<signal name="N$81">
<contactref element="JTAG" pad="4"/>
<contactref element="UC" pad="069"/>
</signal>
<signal name="N$68">
<contactref element="R47" pad="2"/>
<contactref element="C49" pad="2"/>
<contactref element="UC" pad="076"/>
</signal>
<signal name="N$71">
<contactref element="C48" pad="2"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="DISPLAY_VOLTAGE_ENABLE">
<contactref element="R44" pad="1"/>
<contactref element="R50" pad="2"/>
<contactref element="UC" pad="044"/>
</signal>
<signal name="N$56">
<contactref element="R32" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="7-18VDC" pad="3"/>
</signal>
<signal name="N$54">
<contactref element="7-18VDC" pad="1"/>
<contactref element="L3" pad="2"/>
</signal>
<signal name="N$83">
<contactref element="R9" pad="3-CW"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="N$84">
<contactref element="R44" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="7-18VDC" pad="4"/>
</signal>
<signal name="TWCK">
<contactref element="MPEX" pad="01"/>
<contactref element="UC" pad="022"/>
<contactref element="RTC" pad="6"/>
<contactref element="R48" pad="1"/>
<contactref element="4DACS" pad="14"/>
<contactref element="GPIO2" pad="14"/>
<contactref element="GPIO3" pad="14"/>
<contactref element="GPIO1" pad="6"/>
</signal>
<signal name="TWD">
<contactref element="MPEX" pad="03"/>
<contactref element="UC" pad="021"/>
<contactref element="RTC" pad="7"/>
<contactref element="R49" pad="1"/>
<contactref element="4DACS" pad="13"/>
<contactref element="GPIO2" pad="15"/>
<contactref element="GPIO3" pad="15"/>
<contactref element="GPIO1" pad="7"/>
</signal>
<signal name="3.3V-CURRENT">
<contactref element="MPEX" pad="11"/>
<contactref element="U$70" pad="2"/>
</signal>
<signal name="AMBIENT-LIGHT">
<contactref element="LTV" pad="3"/>
<contactref element="MPEX" pad="09"/>
</signal>
<signal name="VDISPLAY-DIVIDED">
<contactref element="R34" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="MPEX" pad="04"/>
</signal>
<signal name="VBUS-DIVIDED">
<contactref element="R35" pad="1"/>
<contactref element="R38" pad="2"/>
<contactref element="MPEX" pad="05"/>
</signal>
<signal name="VBATTERY-DIVIDED">
<contactref element="R36" pad="1"/>
<contactref element="R39" pad="2"/>
<contactref element="MPEX" pad="06"/>
</signal>
<signal name="ANALOG">
<contactref element="ANALOG" pad="1"/>
<contactref element="MPEX" pad="08"/>
<contactref element="UC" pad="082"/>
</signal>
<signal name="N$62">
<contactref element="CHRG" pad="12"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="CHRG">
<contactref element="CHARGE" pad="C"/>
<contactref element="CHRG" pad="07"/>
</signal>
<signal name="N$61">
<contactref element="R20" pad="1"/>
<contactref element="CHRG" pad="01"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$65">
<contactref element="C10" pad="2"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$66">
<contactref element="R22" pad="1"/>
<contactref element="CHRG" pad="02"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="CHRG" pad="06"/>
<contactref element="CHRG" pad="05"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="R25" pad="1"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="LTC4088-D0">
<contactref element="R26" pad="2"/>
<contactref element="CHRG" pad="13"/>
</signal>
<signal name="LTC4088-D1">
<contactref element="R27" pad="2"/>
<contactref element="CHRG" pad="14"/>
</signal>
<signal name="LTC4088-D2">
<contactref element="R28" pad="2"/>
<contactref element="CHRG" pad="04"/>
</signal>
<signal name="N$34">
<contactref element="OLED" pad="5"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="OLED" pad="8"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="OLED" pad="7"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="OLED" pad="6"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="OLED" pad="9"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="OLED" pad="28"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="OLED" pad="26"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="R5" pad="1"/>
<contactref element="Z1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="1"/>
<contactref element="OLED" pad="14"/>
</signal>
<signal name="N$31">
<contactref element="R2" pad="1"/>
<contactref element="OLED" pad="13"/>
</signal>
<signal name="N$32">
<contactref element="R3" pad="1"/>
<contactref element="OLED" pad="10"/>
</signal>
<signal name="D/C#">
<contactref element="OLED" pad="11"/>
<contactref element="UC" pad="014"/>
</signal>
<signal name="OLED_CS#">
<contactref element="OLED" pad="12"/>
<contactref element="UC" pad="018"/>
</signal>
<signal name="WR#">
<contactref element="OLED" pad="15"/>
<contactref element="UC" pad="019"/>
</signal>
<signal name="RD#">
<contactref element="OLED" pad="16"/>
<contactref element="UC" pad="020"/>
</signal>
<signal name="2.5V">
<contactref element="LAB3" pad="074"/>
<contactref element="LAB3" pad="008"/>
<contactref element="LAB3" pad="100"/>
<contactref element="LAB3" pad="079"/>
<contactref element="LAB3" pad="087"/>
<contactref element="LAB3" pad="088"/>
<contactref element="LAB3" pad="090"/>
<contactref element="LAB3" pad="092"/>
<contactref element="LAB3" pad="094"/>
<contactref element="LAB3" pad="096"/>
<contactref element="LAB3" pad="098"/>
<contactref element="LAB3" pad="066"/>
<contactref element="LAB3" pad="058"/>
<contactref element="LAB3" pad="048"/>
<contactref element="LAB3" pad="042"/>
<contactref element="LAB3" pad="040"/>
<contactref element="LAB3" pad="029"/>
<contactref element="LAB3" pad="027"/>
<contactref element="LAB3" pad="018"/>
<contactref element="R40" pad="2"/>
<contactref element="U$69" pad="4"/>
<contactref element="2.5V" pad="1"/>
<contactref element="R46" pad="2"/>
<contactref element="R51" pad="2"/>
<contactref element="LAB3" pad="055"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="LEVEL-SHIFT" pad="15"/>
<contactref element="C23" pad="2"/>
<contactref element="BUF1" pad="5"/>
<contactref element="C57" pad="2"/>
<contactref element="1.25VDC" pad="1"/>
<contactref element="C74" pad="2"/>
<contactref element="1.25VDC" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="RESET" pad="2"/>
<contactref element="UC" pad="002"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="UC" pad="027"/>
<contactref element="WAKEUP" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="WKUP0">
<contactref element="R11" pad="1"/>
<contactref element="UC" pad="028"/>
<contactref element="RTC" pad="1"/>
</signal>
<signal name="WKUP1">
<contactref element="UC" pad="029"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="SHUTDOWN#">
<contactref element="R10" pad="1"/>
<contactref element="UC" pad="030"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R13" pad="2"/>
<contactref element="3.3VDC" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="R14" pad="2"/>
<contactref element="3.3VDC" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="L2" pad="1"/>
<contactref element="3.3VDC" pad="3"/>
</signal>
<signal name="N$29">
<contactref element="L2" pad="2"/>
<contactref element="3.3VDC" pad="4"/>
</signal>
<signal name="N$30">
<contactref element="R17" pad="1"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="3.3VDC" pad="10"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$50">
<contactref element="3.3VDC" pad="9"/>
<contactref element="R15" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$80">
<contactref element="R15" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="3.3VDC" pad="6"/>
<contactref element="U$70" pad="5"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="N$85">
<contactref element="R45" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="3.3VDC" pad="8"/>
</signal>
<signal name="N$51">
<contactref element="2.5VDC" pad="4"/>
<contactref element="R40" pad="1"/>
<contactref element="U$69" pad="5"/>
<contactref element="C38" pad="2"/>
<contactref element="L4" pad="2"/>
</signal>
<signal name="N$82">
<contactref element="R43" pad="2"/>
<contactref element="2.5VDC" pad="3"/>
<contactref element="C41" pad="2"/>
</signal>
<signal name="2.5V-CURRENT">
<contactref element="U$69" pad="2"/>
<contactref element="MPEX" pad="12"/>
</signal>
<signal name="2.5V-ENABLE">
<contactref element="R43" pad="1"/>
<contactref element="UC" pad="052"/>
</signal>
<signal name="N$52">
<contactref element="RTC" pad="3"/>
<contactref element="U$41" pad="P$1"/>
<contactref element="C60" pad="2"/>
</signal>
<signal name="N$53">
<contactref element="U$41" pad="P$2"/>
<contactref element="RTC" pad="2"/>
</signal>
<signal name="LAB3-DATA11">
<contactref element="LAB3" pad="060"/>
<contactref element="UC" pad="095"/>
</signal>
<signal name="LAB3-DATA10">
<contactref element="LAB3" pad="061"/>
<contactref element="UC" pad="094"/>
</signal>
<signal name="LAB3-DATA9">
<contactref element="LAB3" pad="062"/>
<contactref element="UC" pad="093"/>
</signal>
<signal name="LAB3-DATA8">
<contactref element="LAB3" pad="063"/>
<contactref element="UC" pad="092"/>
</signal>
<signal name="LAB3-DATA7">
<contactref element="LAB3" pad="064"/>
<contactref element="UC" pad="091"/>
</signal>
<signal name="LAB3-DATA6">
<contactref element="LAB3" pad="065"/>
<contactref element="UC" pad="090"/>
</signal>
<signal name="LAB3-DATA5">
<contactref element="LAB3" pad="068"/>
<contactref element="UC" pad="089"/>
</signal>
<signal name="LAB3-DATA4">
<contactref element="LAB3" pad="069"/>
<contactref element="UC" pad="087"/>
</signal>
<signal name="LAB3-DATA3">
<contactref element="LAB3" pad="070"/>
<contactref element="UC" pad="086"/>
</signal>
<signal name="LAB3-DATA2">
<contactref element="LAB3" pad="071"/>
<contactref element="UC" pad="085"/>
</signal>
<signal name="LAB3-DATA1">
<contactref element="LAB3" pad="072"/>
<contactref element="UC" pad="084"/>
</signal>
<signal name="LAB3-DATA0">
<contactref element="LAB3" pad="073"/>
<contactref element="UC" pad="083"/>
</signal>
<signal name="N$55">
<contactref element="R46" pad="1"/>
<contactref element="LAB3" pad="050"/>
</signal>
<signal name="N$57">
<contactref element="R51" pad="1"/>
<contactref element="LAB3" pad="047"/>
<contactref element="FET2" pad="12"/>
</signal>
<signal name="N$58">
<contactref element="C6" pad="2"/>
<contactref element="LAB3" pad="051"/>
</signal>
<signal name="N$59">
<contactref element="LAB3" pad="011"/>
<contactref element="4DACS" pad="04"/>
</signal>
<signal name="N$63">
<contactref element="LAB3" pad="012"/>
<contactref element="4DACS" pad="05"/>
</signal>
<signal name="RCO-2.5">
<contactref element="UC" pad="006"/>
<contactref element="LAB3" pad="057"/>
</signal>
<signal name="HITBUS-2.5">
<contactref element="LAB3" pad="075"/>
<contactref element="UC" pad="096"/>
</signal>
<signal name="N$49">
<contactref element="LAB3" pad="052"/>
<contactref element="R52" pad="3-CW"/>
</signal>
<signal name="TRIGGER-A">
<contactref element="FFA" pad="4"/>
<contactref element="R90" pad="2"/>
<contactref element="UC" pad="007"/>
<contactref element="R64" pad="1"/>
</signal>
<signal name="TRIGGER-B">
<contactref element="FFB" pad="4"/>
<contactref element="R89" pad="2"/>
<contactref element="UC" pad="008"/>
<contactref element="R68" pad="1"/>
</signal>
<signal name="VRAMPMON">
<contactref element="LAB3" pad="049"/>
<contactref element="VRAMP" pad="1"/>
</signal>
<signal name="CMPBIAS-SHORT">
<contactref element="FET2" pad="08"/>
<contactref element="GPIO3" pad="07"/>
</signal>
<signal name="N$88">
<contactref element="XOR" pad="7"/>
<contactref element="FFA" pad="1"/>
</signal>
<signal name="N$89">
<contactref element="FFB" pad="1"/>
<contactref element="XOR" pad="3"/>
</signal>
<signal name="POLARITY-SELECT">
<contactref element="XOR" pad="5"/>
<contactref element="XOR" pad="1"/>
<contactref element="GPIO1" pad="1"/>
</signal>
<signal name="TRIGGER-CLEAR">
<contactref element="FFB" pad="6"/>
<contactref element="FFA" pad="6"/>
<contactref element="GPIO1" pad="2"/>
</signal>
<signal name="N$70">
<contactref element="XOR" pad="2"/>
<contactref element="CMP-A" pad="1"/>
</signal>
<signal name="N$90">
<contactref element="XOR" pad="6"/>
<contactref element="CMP-B" pad="1"/>
</signal>
<signal name="VDISPLAY-PRIME">
<contactref element="7-18VDC" pad="5"/>
<contactref element="U$71" pad="5"/>
<contactref element="R18" pad="1"/>
<contactref element="C40" pad="2"/>
<contactref element="R9" pad="1-CCW"/>
</signal>
<signal name="N$92">
<contactref element="R53" pad="2"/>
<contactref element="AMP-A" pad="4"/>
<contactref element="R42" pad="1"/>
<contactref element="R54" pad="2"/>
</signal>
<signal name="-5V">
<contactref element="AMP-A" pad="2"/>
<contactref element="R54" pad="1"/>
<contactref element="AMP-B" pad="2"/>
<contactref element="R57" pad="1"/>
<contactref element="MPEX-A" pad="06"/>
<contactref element="MPEX-B" pad="06"/>
<contactref element="C52" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C63" pad="2"/>
<contactref element="C65" pad="2"/>
<contactref element="R92" pad="2"/>
<contactref element="D1" pad="P$1"/>
<contactref element="C67" pad="2"/>
<contactref element="C70" pad="2"/>
<contactref element="R99" pad="1"/>
<contactref element="C76" pad="2"/>
<contactref element="C77" pad="2"/>
</signal>
<signal name="5V">
<contactref element="AMP-A" pad="6"/>
<contactref element="AMP-B" pad="6"/>
<contactref element="MPEX-A" pad="14"/>
<contactref element="MPEX-B" pad="14"/>
<contactref element="C51" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="C64" pad="2"/>
<contactref element="C71" pad="1"/>
<contactref element="R94" pad="1"/>
<contactref element="C68" pad="1"/>
<contactref element="D3" pad="P$2"/>
<contactref element="R96" pad="2"/>
<contactref element="AMP-A" pad="5"/>
<contactref element="AMP-B" pad="5"/>
<contactref element="C75" pad="2"/>
</signal>
<signal name="N$94">
<contactref element="R56" pad="2"/>
<contactref element="AMP-B" pad="4"/>
<contactref element="R55" pad="1"/>
<contactref element="R57" pad="2"/>
</signal>
<signal name="CHANNEL-B">
<contactref element="R59" pad="2"/>
<contactref element="LAB3" pad="021"/>
</signal>
<signal name="CHANNEL-A">
<contactref element="R58" pad="2"/>
<contactref element="LAB3" pad="004"/>
</signal>
<signal name="N$97">
<contactref element="LAB3" pad="005"/>
<contactref element="R61" pad="1"/>
</signal>
<signal name="N$99">
<contactref element="LAB3" pad="010"/>
<contactref element="R63" pad="1"/>
</signal>
<signal name="N$101">
<contactref element="LAB3" pad="017"/>
<contactref element="R65" pad="1"/>
</signal>
<signal name="N$103">
<contactref element="LAB3" pad="022"/>
<contactref element="R67" pad="1"/>
</signal>
<signal name="N$105">
<contactref element="CMP-A" pad="5"/>
<contactref element="R69" pad="2"/>
</signal>
<signal name="N$106">
<contactref element="CMP-B" pad="5"/>
<contactref element="R70" pad="2"/>
</signal>
<signal name="N$109">
<contactref element="MPEX-A" pad="13"/>
<contactref element="R71" pad="2"/>
<contactref element="R53" pad="1"/>
</signal>
<signal name="N$110">
<contactref element="MPEX-A" pad="12"/>
<contactref element="R71" pad="1"/>
</signal>
<signal name="N$111">
<contactref element="R72" pad="2"/>
<contactref element="MPEX-A" pad="01"/>
<contactref element="R79" pad="2"/>
<contactref element="D4" pad="12"/>
</signal>
<signal name="N$113">
<contactref element="R74" pad="2"/>
<contactref element="MPEX-A" pad="05"/>
<contactref element="R77" pad="2"/>
<contactref element="D6" pad="12"/>
</signal>
<signal name="N$114">
<contactref element="R75" pad="2"/>
<contactref element="MPEX-A" pad="07"/>
<contactref element="R76" pad="2"/>
<contactref element="D7" pad="12"/>
</signal>
<signal name="VIN-CHANNEL-A">
<contactref element="R72" pad="1"/>
<contactref element="R75" pad="1"/>
<contactref element="R74" pad="1"/>
<contactref element="R73" pad="1"/>
<contactref element="CH-A" pad="SIGNAL"/>
</signal>
<signal name="N$116">
<contactref element="R80" pad="2"/>
<contactref element="R56" pad="1"/>
<contactref element="MPEX-B" pad="13"/>
</signal>
<signal name="N$117">
<contactref element="R80" pad="1"/>
<contactref element="MPEX-B" pad="12"/>
</signal>
<signal name="N$118">
<contactref element="R81" pad="2"/>
<contactref element="R88" pad="2"/>
<contactref element="D8" pad="12"/>
<contactref element="MPEX-B" pad="01"/>
</signal>
<signal name="N$119">
<contactref element="R82" pad="2"/>
<contactref element="R87" pad="2"/>
<contactref element="D9" pad="12"/>
<contactref element="MPEX-B" pad="03"/>
</signal>
<signal name="N$120">
<contactref element="R83" pad="2"/>
<contactref element="R86" pad="2"/>
<contactref element="D10" pad="12"/>
<contactref element="MPEX-B" pad="05"/>
</signal>
<signal name="N$121">
<contactref element="R84" pad="2"/>
<contactref element="R85" pad="2"/>
<contactref element="D11" pad="12"/>
<contactref element="MPEX-B" pad="07"/>
</signal>
<signal name="VIN-CHANNEL-B">
<contactref element="R83" pad="1"/>
<contactref element="R84" pad="1"/>
<contactref element="R81" pad="1"/>
<contactref element="R82" pad="1"/>
<contactref element="CH-B" pad="SIGNAL"/>
</signal>
<signal name="N$126">
<contactref element="2.5VDC" pad="5"/>
<contactref element="L4" pad="1"/>
</signal>
<signal name="N$125">
<contactref element="R90" pad="1"/>
<contactref element="TRIGGER-A" pad="A"/>
</signal>
<signal name="N$127">
<contactref element="R89" pad="1"/>
<contactref element="TRIGGER-B" pad="A"/>
</signal>
<signal name="VREF">
<contactref element="4DACS" pad="07"/>
</signal>
<signal name="N$96">
<contactref element="CMP-B" pad="4"/>
<contactref element="4DACS" pad="10"/>
</signal>
<signal name="OLED-DATA0">
<contactref element="UC" pad="032"/>
<contactref element="OLED" pad="17"/>
</signal>
<signal name="OLED-DATA1">
<contactref element="UC" pad="033"/>
<contactref element="OLED" pad="18"/>
</signal>
<signal name="OLED-DATA2">
<contactref element="UC" pad="034"/>
<contactref element="OLED" pad="19"/>
</signal>
<signal name="OLED-DATA3">
<contactref element="UC" pad="035"/>
<contactref element="OLED" pad="20"/>
</signal>
<signal name="OLED-DATA4">
<contactref element="UC" pad="036"/>
<contactref element="OLED" pad="21"/>
</signal>
<signal name="OLED-DATA5">
<contactref element="UC" pad="037"/>
<contactref element="OLED" pad="22"/>
</signal>
<signal name="OLED-DATA6">
<contactref element="UC" pad="041"/>
<contactref element="OLED" pad="23"/>
</signal>
<signal name="OLED-DATA7">
<contactref element="UC" pad="042"/>
<contactref element="OLED" pad="24"/>
</signal>
<signal name="OLED-DATA8">
<contactref element="UC" pad="043"/>
<contactref element="OLED" pad="25"/>
</signal>
<signal name="GCCLOCK-GATE">
<contactref element="UC" pad="081"/>
<contactref element="OSC2" pad="3"/>
</signal>
<signal name="RAMP-3.3">
<contactref element="UC" pad="080"/>
<contactref element="LEVEL-SHIFT" pad="24"/>
</signal>
<signal name="CHANNEL-A-MULTIPLEXER-A0">
<contactref element="MPEX-A" pad="08"/>
<contactref element="GPIO1" pad="3"/>
</signal>
<signal name="CHANNEL-A-MULTIPLEXER-A1">
<contactref element="MPEX-A" pad="09"/>
<contactref element="GPIO1" pad="5"/>
</signal>
<signal name="CHANNEL-B-MULTIPLEXER-A0">
<contactref element="MPEX-B" pad="08"/>
<contactref element="GPIO3" pad="09"/>
</signal>
<signal name="CHANNEL-B-MULTIPLEXER-A1">
<contactref element="MPEX-B" pad="09"/>
<contactref element="GPIO3" pad="10"/>
</signal>
<signal name="NRUN-3.3">
<contactref element="UC" pad="005"/>
<contactref element="LEVEL-SHIFT" pad="46"/>
</signal>
<signal name="NRUN-2.5">
<contactref element="LAB3" pad="084"/>
<contactref element="LEVEL-SHIFT" pad="02"/>
</signal>
<signal name="GCCLEAR-2.5">
<contactref element="LAB3" pad="077"/>
<contactref element="LEVEL-SHIFT" pad="07"/>
</signal>
<signal name="RAMP-2.5">
<contactref element="LAB3" pad="054"/>
<contactref element="LEVEL-SHIFT" pad="25"/>
</signal>
<signal name="GCCLOCK-2.5">
<contactref element="LAB3" pad="078"/>
<contactref element="BUF1" pad="4"/>
</signal>
<signal name="SELMAIN-2.5">
<contactref element="LAB3" pad="030"/>
<contactref element="LEVEL-SHIFT" pad="28"/>
</signal>
<signal name="SELTAIL-2.5">
<contactref element="LAB3" pad="043"/>
<contactref element="LEVEL-SHIFT" pad="27"/>
</signal>
<signal name="CA00-2.5">
<contactref element="LAB3" pad="083"/>
<contactref element="LEVEL-SHIFT" pad="03"/>
</signal>
<signal name="CA01-2.5">
<contactref element="LAB3" pad="082"/>
<contactref element="LEVEL-SHIFT" pad="04"/>
</signal>
<signal name="CA02-2.5">
<contactref element="LAB3" pad="081"/>
<contactref element="LEVEL-SHIFT" pad="05"/>
</signal>
<signal name="CA03-2.5">
<contactref element="LAB3" pad="080"/>
<contactref element="LEVEL-SHIFT" pad="06"/>
</signal>
<signal name="SA00-2.5">
<contactref element="LAB3" pad="031"/>
<contactref element="LEVEL-SHIFT" pad="39"/>
</signal>
<signal name="SA02-2.5">
<contactref element="LAB3" pad="033"/>
<contactref element="LEVEL-SHIFT" pad="37"/>
</signal>
<signal name="SA03-2.5">
<contactref element="LAB3" pad="034"/>
<contactref element="LEVEL-SHIFT" pad="36"/>
</signal>
<signal name="SA04-2.5">
<contactref element="LAB3" pad="035"/>
<contactref element="LEVEL-SHIFT" pad="35"/>
</signal>
<signal name="SA06-2.5">
<contactref element="LAB3" pad="037"/>
<contactref element="LEVEL-SHIFT" pad="30"/>
</signal>
<signal name="SA05-2.5">
<contactref element="LAB3" pad="036"/>
<contactref element="LEVEL-SHIFT" pad="34"/>
</signal>
<signal name="SA07-2.5">
<contactref element="LAB3" pad="038"/>
<contactref element="LEVEL-SHIFT" pad="29"/>
</signal>
<signal name="1.25V">
<contactref element="R61" pad="2"/>
<contactref element="R63" pad="2"/>
<contactref element="R65" pad="2"/>
<contactref element="R67" pad="2"/>
<contactref element="R66" pad="1"/>
<contactref element="R91" pad="1"/>
<contactref element="1.25VDC" pad="5"/>
<contactref element="C73" pad="2"/>
</signal>
<signal name="CHANNEL-A-RAW">
<contactref element="R42" pad="2"/>
<contactref element="AMP-A" pad="1"/>
<contactref element="R58" pad="1"/>
<contactref element="CMP-A" pad="3"/>
</signal>
<signal name="CHANNEL-B-RAW">
<contactref element="R55" pad="2"/>
<contactref element="AMP-B" pad="1"/>
<contactref element="R59" pad="1"/>
<contactref element="CMP-B" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="4DACS" pad="11"/>
<contactref element="CMP-A" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="OSC2" pad="5"/>
<contactref element="BUF1" pad="2"/>
</signal>
<signal name="CA00-3.3">
<contactref element="LEVEL-SHIFT" pad="45"/>
<contactref element="UC" pad="012"/>
</signal>
<signal name="CA01-3.3">
<contactref element="LEVEL-SHIFT" pad="44"/>
<contactref element="UC" pad="011"/>
</signal>
<signal name="CA02-3.3">
<contactref element="LEVEL-SHIFT" pad="43"/>
<contactref element="UC" pad="010"/>
</signal>
<signal name="CA03-3.3">
<contactref element="LEVEL-SHIFT" pad="42"/>
<contactref element="UC" pad="009"/>
</signal>
<signal name="GCCLEAR-3.3">
<contactref element="LEVEL-SHIFT" pad="40"/>
<contactref element="UC" pad="013"/>
</signal>
<signal name="SA01-2.5">
<contactref element="LEVEL-SHIFT" pad="38"/>
<contactref element="LAB3" pad="032"/>
</signal>
<signal name="SA00-3.3">
<contactref element="LEVEL-SHIFT" pad="09"/>
<contactref element="UC" pad="055"/>
</signal>
<signal name="SA01-3.3">
<contactref element="LEVEL-SHIFT" pad="10"/>
<contactref element="UC" pad="056"/>
</signal>
<signal name="SA02-3.3">
<contactref element="LEVEL-SHIFT" pad="11"/>
<contactref element="UC" pad="057"/>
</signal>
<signal name="SA03-3.3">
<contactref element="LEVEL-SHIFT" pad="12"/>
<contactref element="UC" pad="058"/>
</signal>
<signal name="SA04-3.3">
<contactref element="LEVEL-SHIFT" pad="13"/>
<contactref element="UC" pad="062"/>
</signal>
<signal name="SA05-3.3">
<contactref element="LEVEL-SHIFT" pad="14"/>
<contactref element="UC" pad="063"/>
</signal>
<signal name="SA06-3.3">
<contactref element="LEVEL-SHIFT" pad="19"/>
<contactref element="UC" pad="064"/>
</signal>
<signal name="SA07-3.3">
<contactref element="LEVEL-SHIFT" pad="20"/>
<contactref element="UC" pad="065"/>
</signal>
<signal name="SELMAIN-3.3">
<contactref element="LEVEL-SHIFT" pad="21"/>
<contactref element="UC" pad="054"/>
</signal>
<signal name="SELTAIL-3.3">
<contactref element="LEVEL-SHIFT" pad="22"/>
<contactref element="UC" pad="053"/>
</signal>
<signal name="N$5">
<contactref element="R60" pad="2"/>
<contactref element="R52" pad="1-CCW"/>
</signal>
<signal name="N$7">
<contactref element="CHARGE" pad="A"/>
<contactref element="R62" pad="1"/>
</signal>
<signal name="N$10">
</signal>
<signal name="VBAT">
<contactref element="L1" pad="2"/>
<contactref element="CHRG" pad="10"/>
<contactref element="C13" pad="2"/>
<contactref element="U$72" pad="5"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="CAL">
<contactref element="UC" pad="051"/>
<contactref element="CAL" pad="1"/>
</signal>
<signal name="0.75V">
<contactref element="D4" pad="04"/>
<contactref element="D7" pad="04"/>
<contactref element="D6" pad="04"/>
<contactref element="D5" pad="04"/>
<contactref element="D8" pad="04"/>
<contactref element="D11" pad="04"/>
<contactref element="D10" pad="04"/>
<contactref element="D9" pad="04"/>
<contactref element="R97" pad="2"/>
<contactref element="R96" pad="1"/>
</signal>
<signal name="-0.75V">
<contactref element="D4" pad="08"/>
<contactref element="D7" pad="08"/>
<contactref element="D6" pad="08"/>
<contactref element="D5" pad="08"/>
<contactref element="D8" pad="08"/>
<contactref element="D11" pad="08"/>
<contactref element="D10" pad="08"/>
<contactref element="D9" pad="08"/>
<contactref element="R99" pad="2"/>
<contactref element="R98" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R64" pad="2"/>
<contactref element="R66" pad="2"/>
<contactref element="LAB3" pad="009"/>
</signal>
<signal name="N$13">
<contactref element="R91" pad="2"/>
<contactref element="R68" pad="2"/>
<contactref element="LAB3" pad="016"/>
</signal>
<signal name="N$17">
<contactref element="ROT1" pad="SW2"/>
<contactref element="GPIO2" pad="06"/>
</signal>
<signal name="N$15">
<contactref element="ROT1" pad="B"/>
<contactref element="GPIO2" pad="04"/>
</signal>
<signal name="N$16">
<contactref element="ROT1" pad="A"/>
<contactref element="GPIO2" pad="05"/>
</signal>
<signal name="N$19">
<contactref element="ROT2" pad="SW2"/>
<contactref element="GPIO3" pad="06"/>
</signal>
<signal name="N$20">
<contactref element="ROT2" pad="B"/>
<contactref element="GPIO3" pad="04"/>
</signal>
<signal name="N$21">
<contactref element="GPIO3" pad="05"/>
<contactref element="ROT2" pad="A"/>
</signal>
<signal name="USB-PULLUP#">
<contactref element="GPIO2" pad="07"/>
<contactref element="FET1" pad="08"/>
</signal>
<signal name="N$18">
<contactref element="R95" pad="1"/>
<contactref element="R94" pad="2"/>
<contactref element="C68" pad="2"/>
<contactref element="+-5VDC" pad="5"/>
</signal>
<signal name="N$22">
<contactref element="+-5VDC" pad="6"/>
<contactref element="L6" pad="2"/>
<contactref element="D3" pad="P$1"/>
</signal>
<signal name="N$33">
<contactref element="L5" pad="2"/>
<contactref element="+-5VDC" pad="10"/>
<contactref element="C66" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="C66" pad="2"/>
<contactref element="D1" pad="P$2"/>
<contactref element="D2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="C67" pad="1"/>
<contactref element="R92" pad="1"/>
<contactref element="R93" pad="2"/>
<contactref element="+-5VDC" pad="1"/>
</signal>
<signal name="SHUTDOWN#-MINUS-5V">
<contactref element="+-5VDC" pad="2"/>
<contactref element="GPIO3" pad="12"/>
</signal>
<signal name="SHUTDOWN#-PLUS-5V">
<contactref element="+-5VDC" pad="4"/>
<contactref element="GPIO3" pad="11"/>
</signal>
<signal name="N$1234">
<contactref element="R73" pad="2"/>
<contactref element="MPEX-A" pad="03"/>
<contactref element="R78" pad="2"/>
<contactref element="D5" pad="12"/>
</signal>
<signal name="BUTTON1">
<contactref element="UC" pad="023"/>
<contactref element="BUTTON-1" pad="1"/>
</signal>
<signal name="BUTTON2">
<contactref element="UC" pad="024"/>
<contactref element="BUTTON-2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="C72" pad="2"/>
<contactref element="1.25VDC" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
