(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 109)
    (zones 0)
    (modules 5)
    (nets 33)
  )
  (page A4)
  (title_block
    (title "DMX Demonstrator - Receiver IO Module (DMX-RX2)")
    (date 2023-10-28)
    (rev 1.2)
    (company "Sparky Bobo Designs")
    (comment 2 "Designed by: SparkyBobo")
    (comment 3 https://creativecommons.org/licenses/by-sa/4.0/)
    (comment 4 "Released under the Creative Commons Attribution Share-Alike 4.0 License")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 0.9)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "grb"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(A1-Pad32)")
  (net 4 "Net-(A1-Pad31)")
  (net 5 "Net-(A1-Pad1)")
  (net 6 "Net-(A1-Pad2)")
  (net 7 "Net-(A1-Pad3)")
  (net 8 "Net-(A1-Pad4)")
  (net 9 "Net-(A1-Pad8)")
  (net 10 "Net-(A1-Pad30)")
  (net 11 /~WR)
  (net 12 "Net-(A1-Pad11)")
  (net 13 "Net-(A1-Pad12)")
  (net 14 "Net-(A1-Pad13)")
  (net 15 "Net-(A1-Pad14)")
  (net 16 /DMX-RX)
  (net 17 /DMX-TX)
  (net 18 /DMX-DIR)
  (net 19 /SR-OUT)
  (net 20 /SR-CLK)
  (net 21 "Net-(A1-Pad20)")
  (net 22 "Net-(A1-Pad21)")
  (net 23 /A0)
  (net 24 /A1)
  (net 25 "Net-(A1-Pad24)")
  (net 26 "Net-(A1-Pad25)")
  (net 27 "Net-(A1-Pad26)")
  (net 28 "Net-(A1-Pad27)")
  (net 29 /~SR_CLR)
  (net 30 "Net-(A1-Pad28)")
  (net 31 "Net-(J1-Pad12)")
  (net 32 "Net-(J2-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net /A0)
    (add_net /A1)
    (add_net /DMX-DIR)
    (add_net /DMX-RX)
    (add_net /DMX-TX)
    (add_net /SR-CLK)
    (add_net /SR-OUT)
    (add_net /~SR_CLR)
    (add_net /~WR)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad30)")
    (add_net "Net-(A1-Pad31)")
    (add_net "Net-(A1-Pad32)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J2-Pad12)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 1.27)
    (uvia_drill 0.635)
    (diff_pair_width 0.3048)
    (diff_pair_gap 0.3048)
    (add_net +5V)
  )
  (module Connector_IDC:IDC-Header_2x07_P2.54mm_Horizontal (layer F.Cu) (tedit 59DE207F)
    (at 176.276 97.536 180)
    (descr "Through hole angled IDC box header, 2x07, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x07 2.54mm double row")
    (fp_text reference J1 (at 0 -2.413 180) (layer F.SilkS))
    (fp_text value "IO EXTENSION" (at 6.105 21.844 180) (layer F.Fab))
    (fp_text user %R (at 8.805 7.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /~WR))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /SR-OUT))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /A1))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /SR-CLK))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /A0))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /~SR_CLR))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /DMX-RX))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /DMX-DIR))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /DMX-TX))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x07_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x07_P2.54mm_Horizontal (layer F.Cu) (tedit 59DE207F)
    (at 135.001 97.536 180)
    (descr "Through hole angled IDC box header, 2x07, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x07 2.54mm double row")
    (fp_text reference J2 (at 0 -2.413 180) (layer F.SilkS))
    (fp_text value "IO EXTENSION" (at 6.105 21.844 180) (layer F.Fab))
    (fp_text user %R (at 8.805 7.62 270) (layer F.Fab))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /DMX-TX))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /DMX-DIR))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /DMX-RX))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /~SR_CLR))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /A0))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /SR-CLK))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /A1))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /SR-OUT))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /~WR))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x07_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:ARDUINO_R3_NO_HOLES (layer F.Cu) (tedit 5FA36CC6)
    (at 150.622 89.916)
    (descr "ARDUINO UNO R3 FOOTPRINT")
    (tags "ARDUINO UNO R3 FOOTPRINT")
    (attr virtual)
    (fp_text reference A1 (at -32.766 -25.908) (layer F.SilkS) hide)
    (fp_text value Arduino_UNO_R3 (at -29.718 -24.892) (layer F.SilkS) hide)
    (fp_text user SCL (at -15.5194 -20.5232 90) (layer Dwgs.User))
    (fp_text user SDA (at -12.9794 -20.5232 90) (layer Dwgs.User))
    (fp_text user AREF (at -10.4394 -20.9296 90) (layer Dwgs.User))
    (fp_text user GND (at -7.8994 -20.5232 90) (layer Dwgs.User))
    (fp_text user D13 (at -5.3594 -20.5232 90) (layer Dwgs.User))
    (fp_text user D12 (at -2.8194 -20.5232 90) (layer Dwgs.User))
    (fp_text user D11 (at -0.2794 -20.5232 90) (layer Dwgs.User))
    (fp_text user D10 (at 2.2606 -20.5232 90) (layer Dwgs.User))
    (fp_text user D9 (at 4.79806 -20.1168 90) (layer Dwgs.User))
    (fp_text user D8 (at 7.3406 -20.1168 90) (layer Dwgs.User))
    (fp_text user D7 (at 11.4046 -20.1168 90) (layer Dwgs.User))
    (fp_text user D6 (at 13.9446 -20.1168 90) (layer Dwgs.User))
    (fp_text user D5 (at 16.4846 -20.1168 90) (layer Dwgs.User))
    (fp_text user D4 (at 19.0246 -20.1168 90) (layer Dwgs.User))
    (fp_text user D3 (at 21.5646 -20.1168 90) (layer Dwgs.User))
    (fp_text user D2 (at 24.1046 -20.1168 90) (layer Dwgs.User))
    (fp_text user D0/RXI (at 29.05506 -19.2024 90) (layer Dwgs.User))
    (fp_text user D1/TXO (at 26.5176 -19.2024 90) (layer Dwgs.User))
    (fp_text user !RESET! (at -1.6764 20.0152 90) (layer Dwgs.User))
    (fp_text user 3.3V (at 0.8636 21.2344 90) (layer Dwgs.User))
    (fp_text user 5V (at 3.4036 22.0472 90) (layer Dwgs.User))
    (fp_text user GND (at 5.9436 21.6408 90) (layer Dwgs.User))
    (fp_text user GND (at 8.4836 21.6408 90) (layer Dwgs.User))
    (fp_text user VIN (at 11.0236 21.6408 90) (layer Dwgs.User))
    (fp_text user A0 (at 16.1036 22.0472 90) (layer Dwgs.User))
    (fp_text user A1 (at 18.6436 22.0472 90) (layer Dwgs.User))
    (fp_text user A2 (at 21.1836 22.0472 90) (layer Dwgs.User))
    (fp_text user A3 (at 23.7236 22.0472 90) (layer Dwgs.User))
    (fp_text user A4 (at 26.2636 22.0472 90) (layer Dwgs.User))
    (fp_text user A5 (at 28.80106 22.0472 90) (layer Dwgs.User))
    (fp_text user IOREF (at -4.2164 20.828 90) (layer Dwgs.User))
    (pad 4 thru_hole circle (at 1.27 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad4)") (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 3.81 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 16.51 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /A0) (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 19.05 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /A1) (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 21.59 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad11)") (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at 24.13 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad12)") (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at 26.67 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad13)") (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at 29.21 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad14)") (solder_mask_margin 0.1016))
    (pad 30 thru_hole circle (at -10.414 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad30)") (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at 29.21 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /DMX-RX) (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at 26.67 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /DMX-TX) (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at 24.13 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /DMX-DIR) (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at 21.59 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /SR-OUT) (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 19.05 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /SR-CLK) (solder_mask_margin 0.1016))
    (pad 20 thru_hole circle (at 16.51 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad20)") (solder_mask_margin 0.1016))
    (pad 21 thru_hole circle (at 13.97 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad21)") (solder_mask_margin 0.1016))
    (pad 22 thru_hole circle (at 11.43 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /~SR_CLR) (solder_mask_margin 0.1016))
    (pad 23 thru_hole circle (at 7.366 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /~WR) (solder_mask_margin 0.1016))
    (pad 24 thru_hole circle (at 4.826 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad24)") (solder_mask_margin 0.1016))
    (pad 25 thru_hole circle (at 2.286 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad25)") (solder_mask_margin 0.1016))
    (pad 26 thru_hole circle (at -0.254 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad26)") (solder_mask_margin 0.1016))
    (pad 27 thru_hole circle (at -2.794 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad27)") (solder_mask_margin 0.1016))
    (pad 28 thru_hole circle (at -5.334 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(A1-Pad28)") (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 6.35 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 8.89 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 29 thru_hole circle (at -7.874 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -3.81 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -6.35 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad1)") (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -1.27 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad3)") (solder_mask_margin 0.1016))
    (pad 32 thru_hole circle (at -15.494 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad32)") (solder_mask_margin 0.1016))
    (pad 31 thru_hole circle (at -12.954 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad31)") (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 11.43 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad8)") (solder_mask_margin 0.1016))
  )
  (module footprints:OSHW-LOGO-S locked (layer F.Cu) (tedit 200000)
    (at 119.126 114.3)
    (descr "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (tags "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (attr virtual)
    (fp_text reference "" (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
  )
  (module footprints:logo_cr_5x5 locked (layer B.Cu) (tedit 0)
    (at 120.142 109.474 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text "IO Expansion" (at 161.417 90.043 270) (layer F.SilkS))
  (gr_text "IO Expansion" (at 119.507 90.043 270) (layer F.SilkS))
  (gr_arc (start 181.61 115.824) (end 181.61 116.586) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 117.094 115.824) (end 116.332 115.824) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 117.094 64.008) (end 117.094 63.246) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.332 115.824) (end 116.332 64.008) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.61 116.586) (end 117.094 116.586) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 114.046) (end 182.372 115.824) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.912 111.506) (end 182.372 114.046) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.912 78.74) (end 184.912 111.506) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 76.2) (end 184.912 78.74) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 64.77) (end 182.372 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.848 63.246) (end 182.372 64.77) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.094 63.246) (end 180.848 63.246) (layer Edge.Cuts) (width 0.15))
  (gr_text "DMX-RX2, Rev 1.2\nSparky Bobo Designs" (at 125.984 114.3) (layer B.SilkS))
  (gr_text DMX-RX2 (at 126.492 114.3) (layer F.SilkS))
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.586 63.754) (xy 116.84 63.5) (xy 180.848 63.5) (xy 182.118 64.77) (xy 182.118 76.454)
        (xy 184.658 78.994) (xy 184.658 111.252) (xy 182.118 113.792) (xy 182.118 116.078) (xy 181.864 116.332)
        (xy 116.84 116.332) (xy 116.586 116.078)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.586 63.754) (xy 116.84 63.5) (xy 180.848 63.5) (xy 182.118 64.77) (xy 182.118 76.454)
        (xy 184.658 78.994) (xy 184.658 111.252) (xy 182.118 113.792) (xy 182.118 116.078) (xy 181.864 116.332)
        (xy 116.84 116.332) (xy 116.586 116.078)
      )
    )
  )
)
