(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "light APRS")
		(date "2025-09-26")
		(rev "1.5")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+BATT")
	(net 2 "GND")
	(net 3 "unconnected-(U1-RST-Pad6)")
	(net 4 "unconnected-(U1-GND-Pad2)")
	(net 5 "unconnected-(U1-3V3-Pad5)")
	(net 6 "unconnected-(U1-VBat-Pad1)")
	(net 7 "unconnected-(U1-SCL{slash}PC0-Pad7)")
	(net 8 "Net-(D1-K)")
	(net 9 "LED")
	(net 10 "Net-(Q1-D)")
	(net 11 "unconnected-(U1-SDA{slash}PC1-Pad8)")
	(net 12 "unconnected-(U1-MOSI{slash}PB5-Pad11)")
	(net 13 "unconnected-(U1-MISO{slash}PB6-Pad10)")
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 175.25 111.75 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 2 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "light_APRS_v1_5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 9 "LED")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Dave:light_APRS_SMD"
		(layer "F.Cu")
		(at 148.9 129.85)
		(property "Reference" "U1"
			(at -18.4 -49.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "light APRS v1.0"
			(at -11.3 3.65 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "light_APRS_v1_5.kicad_sch")
		(attr smd)
		(fp_text user "3V3"
			(at 7.5 -37.95 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MOSI"
			(at 7.5 -22.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 7.5 -42.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at 7.5 -27.85 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "4V5 to 10V"
			(at -16.9 -57.85 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MISO"
			(at 7.5 -25.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SDA"
			(at 7.5 -30.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "light APRS"
			(at -16.9 -59.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -8.5 -42.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SCL"
			(at 7.4 -32.95 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "RAW"
			(at 7.4 -45 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "RST"
			(at 7.5 -35.45 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "USB"
			(at -7.9 -2.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "RAW"
			(at -8.5 -44.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 10.9 1.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -11.95 -48.85)
			(size 3.2 3.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -11.95 -2.85)
			(size 3.2 3.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 14.85 -48.85)
			(size 3.2 3.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 14.85 -2.85)
			(size 3.2 3.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -10.95 -45.35)
			(size 3.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "unconnected-(U1-VBat-Pad1)")
			(pinfunction "VBat")
			(pintype "power_in+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -14 -42.81)
			(size 3.4 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "unconnected-(U1-GND-Pad2)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 16.75 -45.85)
			(size 3.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+BATT")
			(pinfunction "VBat")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 13.85 -43.31)
			(size 3.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 16.85 -38.7)
			(size 3.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "unconnected-(U1-3V3-Pad5)")
			(pinfunction "3V3")
			(pintype "power_in+no_connect")
		)
		(pad "6" smd rect
			(at 13.95 -36.16)
			(size 3.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "unconnected-(U1-RST-Pad6)")
			(pinfunction "RST")
			(pintype "input+no_connect")
		)
		(pad "7" smd rect
			(at 16.85 -33.62)
			(size 3.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "unconnected-(U1-SCL{slash}PC0-Pad7)")
			(pinfunction "SCL/PC0")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" smd rect
			(at 13.95 -31.08)
			(size 3.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(U1-SDA{slash}PC1-Pad8)")
			(pinfunction "SDA/PC1")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" smd rect
			(at 16.85 -28.54)
			(size 3.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "LED")
			(pinfunction "SCK/PB7")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 13.95 -26)
			(size 3.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(U1-MISO{slash}PB6-Pad10)")
			(pinfunction "MISO/PB6")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" smd rect
			(at 16.85 -23.46)
			(size 3.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(U1-MOSI{slash}PB5-Pad11)")
			(pinfunction "MOSI/PB5")
			(pintype "bidirectional+no_connect")
		)
		(embedded_fonts no)
		(model "M:/KiCAD/light_APRS/Solidworks/lightAPRS.STEP"
			(offset
				(xyz 1.5 25.5 3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 175.1875 83 180)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at -0.25 1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED LTST-C171TGKT"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "light_APRS_v1_5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0 180)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 8 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0 180)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "+BATT")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 175.25 96.75 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "300"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "light_APRS_v1_5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 10 "Net-(Q1-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Dave:ScienceHeads_20mm"
		(layer "F.Cu")
		(at 176.25 72.25)
		(property "Reference" "G***"
			(at -4.5 7.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 175.25 104.5 90)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q1"
			(at 0 -2.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "DMN2005K"
			(at 0 2.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN2056U.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "light_APRS_v1_5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 90)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "LED")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 90)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 90)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(Q1-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Dave:DN_swoop_05mm"
		(layer "F.Cu")
		(at 173.2 126.3)
		(property "Reference" "G***"
			(at 2.7 2.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Dave:BAT_BH4AA-PC"
		(layer "B.Cu")
		(at 155.75 93.83 -90)
		(property "Reference" "BT1"
			(at -23.455 33.209 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "BH4AA-PC"
			(at -13 -29.25 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "E"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "MPD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "15.88mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "light_APRS_v1_5.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at 30.42 -22.5 90)
			(layer "B.SilkS")
		)
		(fp_text user "_"
			(at 30.42 -9.25 90)
			(layer "B.SilkS")
		)
		(pad "" np_thru_hole circle
			(at 0 -27.305 270)
			(size 3.4 3.4)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 27.305 270)
			(size 3.4 3.4)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "+" thru_hole oval
			(at 27.17 -22.67 270)
			(size 1.35 2.7)
			(drill oval 1 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+BATT")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "-" thru_hole oval
			(at 27.17 -9.97 270)
			(size 1.35 2.7)
			(drill oval 1 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "M:/KiCAD/BH4AAPC/BH4AA-PC.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -180)
			)
		)
	)
	(gr_line
		(start 118 79.25)
		(end 118 82.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123 111.25)
		(mid 122.707107 111.957107)
		(end 122 112.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.5 117.250157)
		(end 189.5 117.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 189.5 112.25)
		(mid 188.792893 111.957107)
		(end 188.5 111.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 118 113.25)
		(mid 118.292893 112.542893)
		(end 119 112.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 124.25 131.5)
		(mid 123.366117 131.133883)
		(end 123 130.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119 117.25)
		(mid 118.292893 116.957107)
		(end 118 116.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119 112.25)
		(end 122 112.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123 118.25)
		(end 123 130.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119 83.25)
		(end 122 83.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 193.500157 116.25)
		(mid 193.207218 116.957218)
		(end 192.5 117.250157)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 192.474745 78.25)
		(mid 193.181852 78.542893)
		(end 193.474745 79.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119 78.25)
		(end 122 78.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.5 83.25)
		(end 189.5 83.249843)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118 113.25)
		(end 118 116.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.500966 118.206079)
		(end 188.524754 130.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 122 83.25)
		(mid 122.707107 83.542893)
		(end 123 84.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 187.25 64.025255)
		(mid 188.116025 64.383975)
		(end 188.474745 65.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119 117.25)
		(end 122 117.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 192.5 112.25)
		(mid 193.207107 112.542893)
		(end 193.5 113.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123 84.25)
		(end 123 111.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.25 131.524754)
		(end 124.25 131.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123 77.25)
		(mid 122.707107 77.957107)
		(end 122 78.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 189.474745 78.25)
		(mid 188.767638 77.957107)
		(end 188.474745 77.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 122 117.25)
		(mid 122.707107 117.542893)
		(end 123 118.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.25 64.025255)
		(end 124.25 64)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 188.500966 118.206061)
		(mid 188.808603 117.527526)
		(end 189.5 117.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123 65.25)
		(end 123 77.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 188.524754 130.25)
		(mid 188.151387 131.151387)
		(end 187.25 131.524754)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 188.499843 84.25)
		(mid 188.792782 83.542782)
		(end 189.5 83.249843)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.474745 79.25)
		(end 193.5 82.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 118 79.25)
		(mid 118.292893 78.542893)
		(end 119 78.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 193.5 82.25)
		(mid 193.207107 82.957107)
		(end 192.5 83.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119 83.25)
		(mid 118.292893 82.957107)
		(end 118 82.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.474745 65.25)
		(end 188.474745 77.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123 65.25)
		(mid 123.366117 64.366117)
		(end 124.25 64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.5 112.25)
		(end 189.5 112.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 193.5 113.25)
		(end 193.5 116.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.5 84.25)
		(end 188.5 111.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.474745 78.25)
		(end 189.474745 78.25)
		(layer "Edge.Cuts")
	)
	(gr_text "+"
		(at 180.25 122 0)
		(layer "F.SilkS")
	)
	(gr_text "GNSS"
		(at 177.25 81.8125 0)
		(layer "F.SilkS")
	)
	(gr_text "GND\n"
		(at 167.75 121.75 0)
		(layer "F.SilkS")
	)
	(gr_text "26 Sept 2025"
		(at 186.9 129.7 90)
		(layer "F.SilkS")
	)
	(gr_text "V1.5"
		(at 184.9 129.7 90)
		(layer "F.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "F.SilkS")
		(pts
			(xy 121.5 64) (xy 121.5 131.5)
		)
		(height -25.75)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "67.5"
			(at 94.65 97.75 90)
			(layer "F.SilkS")
		)
	)
	(dimension
		(type orthogonal)
		(layer "F.SilkS")
		(pts
			(xy 123 62.5) (xy 188.5 62.5)
		)
		(height -17.25)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "65.5"
			(at 155.75 44.15 0)
			(layer "F.SilkS")
		)
	)
	(zone
		(net 1)
		(net_name "+BATT")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 187.25 79.5) (xy 124.25 79.5) (xy 124.25 130.25) (xy 187.25 130.25)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1)
		)
		(polygon
			(pts
				(xy 187.25 79.5) (xy 124.25 79.5) (xy 124.25 130.25) (xy 187.25 130.25)
			)
		)
	)
	(embedded_fonts no)
)
