(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 14)
    (no_connects 14)
    (area 139.624999 102.794999 156.285001 124.535001)
    (thickness 1.6)
    (drawings 5)
    (tracks 52)
    (zones 0)
    (modules 3)
    (nets 15)
  )
  (page A)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /j1)
  (net 2 /j2)
  (net 3 /j3)
  (net 4 /j4)
  (net 5 /j5)
  (net 6 /j6)
  (net 7 /j7)
  (net 8 /j8)
  (net 9 /j9)
  (net 10 /j10)
  (net 11 /j11)
  (net 12 /j12)
  (net 13 /j13)
  (net 14 /j14)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /j1)
    (add_net /j10)
    (add_net /j11)
    (add_net /j12)
    (add_net /j13)
    (add_net /j14)
    (add_net /j2)
    (add_net /j3)
    (add_net /j4)
    (add_net /j5)
    (add_net /j6)
    (add_net /j7)
    (add_net /j8)
    (add_net /j9)
  )
  (module Socket_Strips:Socket_Strip_Straight_2x07_Pitch2.54mm (layer F.Cu) (tedit 588DE958)
    (at 153.67 105.41)
    (descr "Through hole straight socket strip, 2x07, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x07 2.54mm double row")
    (fp_text reference J2 (at -1.27 -2.33) (layer F.SilkS))
    (fp_text value CONN_02X07 (at -1.27 17.57) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /j1))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /j2))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /j3))
    (pad 4 thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /j4))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /j5))
    (pad 6 thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /j6))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /j7))
    (pad 8 thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /j8))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /j9))
    (pad 10 thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /j10))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /j11))
    (pad 12 thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /j12))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /j13))
    (pad 14 thru_hole oval (at -2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /j14))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x07_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x07_Pitch2.00mm (layer B.Cu) (tedit 5862ED57)
    (at 145.51 106.68 180)
    (descr "Through hole angled pin header, 2x07, 2.00mm pitch, 4mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x07 2.00mm double row")
    (fp_text reference J1 (at 4 2 180) (layer B.SilkS))
    (fp_text value CONN_02X07 (at 4 -14 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /j1))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /j2))
    (pad 3 thru_hole oval (at 0 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /j3))
    (pad 4 thru_hole oval (at 2 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /j4))
    (pad 5 thru_hole oval (at 0 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /j5))
    (pad 6 thru_hole oval (at 2 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /j6))
    (pad 7 thru_hole oval (at 0 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /j7))
    (pad 8 thru_hole oval (at 2 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /j8))
    (pad 9 thru_hole oval (at 0 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /j9))
    (pad 10 thru_hole oval (at 2 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /j10))
    (pad 11 thru_hole oval (at 0 -10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /j11))
    (pad 12 thru_hole oval (at 2 -10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /j12))
    (pad 13 thru_hole oval (at 0 -12 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /j13))
    (pad 14 thru_hole oval (at 2 -12 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /j14))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x07_Pitch2.00mm.wrl
      (at (xyz 0.03937 -0.23622 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module silkscreens:OSH_0.125in (layer B.Cu) (tedit 599C568F)
    (at 141.5 122.5 180)
    (fp_text reference G*** (at 0 -1.68402 180) (layer B.SilkS) hide)
    (fp_text value OSH_0.125in (at 0 1.68402 180) (layer B.SilkS) hide)
  )
  (gr_text "JTAG Pitch Convertor\nVarun Mehta 2017" (at 155.9 123.19) (layer B.SilkS))
  (gr_line (start 156.21 102.87) (end 139.7 102.87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.21 124.46) (end 156.21 102.87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 124.46) (end 156.21 124.46) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 102.87) (end 139.7 124.46) (layer Edge.Cuts) (width 0.15))
)
