(kicad_pcb (version 4) (host pcbnew 4.0.4+dfsg2-stable)
  (general
    (links 45)
    (no_connects 0)
    (area 124.869999 99.845599 160.075001 120.113601)
    (thickness 1.6)
    (drawings 45)
    (tracks 242)
    (zones 0)
    (modules 8)
    (nets 49)
  )
  (page A4)
  (title_block
    (date 2016-03-06)
    (rev 1)
    (comment 4 Merkurboard2)
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.15)
    (zone_clearance 0.2)
    (zone_45_only yes)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.68)
    (via_drill 0.35)
    (via_min_size 0.6)
    (via_min_drill 0.35)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF4B)
    (pcbplotparams
      (layerselection 0x01050_fffffffe)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror true)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory pics))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(IC1-Pad5)")
  (net 5 "Net-(IC1-Pad6)")
  (net 6 "Net-(IC1-Pad7)")
  (net 7 "Net-(IC1-Pad8)")
  (net 8 "Net-(IC1-Pad9)")
  (net 9 "Net-(IC1-Pad10)")
  (net 10 PE6)
  (net 11 PD3)
  (net 12 PD2)
  (net 13 "Net-(IC1-Pad15)")
  (net 14 PD0)
  (net 15 PD1)
  (net 16 "Net-(IC1-Pad18)")
  (net 17 "Net-(IC1-Pad19)")
  (net 18 PB0)
  (net 19 PB2)
  (net 20 PB1)
  (net 21 PB3)
  (net 22 PB4)
  (net 23 "Net-(IC1-Pad25)")
  (net 24 "Net-(IC1-Pad26)")
  (net 25 "Net-(IC1-Pad27)")
  (net 26 "Net-(IC1-Pad28)")
  (net 27 "Net-(IC1-Pad29)")
  (net 28 "Net-(IC1-Pad30)")
  (net 29 PE3)
  (net 30 PE4)
  (net 31 PE5)
  (net 32 "Net-(IC1-Pad35)")
  (net 33 "Net-(IC1-Pad36)")
  (net 34 "Net-(IC1-Pad37)")
  (net 35 "Net-(IC1-Pad38)")
  (net 36 "Net-(IC1-Pad39)")
  (net 37 PF0)
  (net 38 PF1)
  (net 39 "Net-(IC1-Pad42)")
  (net 40 "Net-(IC1-Pad43)")
  (net 41 "Net-(IC1-Pad45)")
  (net 42 "Net-(IC1-Pad46)")
  (net 43 "Net-(IC1-Pad47)")
  (net 44 "Net-(IC1-Pad48)")
  (net 45 "Net-(IC1-Pad53)")
  (net 46 "Net-(D1-Pad1)")
  (net 47 "Net-(P3-Pad2)")
  (net 48 "Net-(C1-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.68)
    (via_drill 0.35)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad29)")
    (add_net "Net-(IC1-Pad30)")
    (add_net "Net-(IC1-Pad35)")
    (add_net "Net-(IC1-Pad36)")
    (add_net "Net-(IC1-Pad37)")
    (add_net "Net-(IC1-Pad38)")
    (add_net "Net-(IC1-Pad39)")
    (add_net "Net-(IC1-Pad42)")
    (add_net "Net-(IC1-Pad43)")
    (add_net "Net-(IC1-Pad45)")
    (add_net "Net-(IC1-Pad46)")
    (add_net "Net-(IC1-Pad47)")
    (add_net "Net-(IC1-Pad48)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad53)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(P3-Pad2)")
    (add_net PB0)
    (add_net PB1)
    (add_net PB2)
    (add_net PB3)
    (add_net PB4)
    (add_net PD0)
    (add_net PD1)
    (add_net PD2)
    (add_net PD3)
    (add_net PE3)
    (add_net PE4)
    (add_net PE5)
    (add_net PE6)
    (add_net PF0)
    (add_net PF1)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 56FFC3C2)
    (at 154.178 115.57)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.028 -1.42 180) (layer F.SilkS))
    (fp_text value 100n (at 0 -1.397) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module deRFmega:A-M10 (layer F.Cu) (tedit 56F970B8)
    (at 140.335 109.982)
    (descr "55pin LGA package, pitch 0.8mm")
    (tags "6lowpan modules by Dresden Elektronik")
    (fp_text reference IC1 (at -10.668 2.032 90) (layer F.SilkS))
    (fp_text value deRFmega128-22M10 (at 10.16 -8.89) (layer F.SilkS) hide)
    (fp_text user 1 (at -10.414 5.969) (layer F.SilkS))
    (pad 1 smd rect (at -8.4 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -7.6 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at -6.8 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -6 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at -5.2 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at -4.4 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at -3.6 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -2.8 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -1.2 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -0.4 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 PE6))
    (pad 12 smd rect (at 0.4 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 PD3))
    (pad 13 smd rect (at 1.2 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 PD2))
    (pad 14 smd rect (at 2 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 2.8 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad15)"))
    (pad 16 smd rect (at 3.6 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 PD0))
    (pad 17 smd rect (at 4.4 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 PD1))
    (pad 18 smd rect (at 5.2 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad18)"))
    (pad 19 smd rect (at 6 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 6.8 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 PB0))
    (pad 21 smd rect (at 7.6 5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 PB2))
    (pad 22 smd rect (at 8.4 4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 PB1))
    (pad 23 smd rect (at 9 2.8 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 PB3))
    (pad 24 smd rect (at 7.7 2 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 PB4))
    (pad 25 smd rect (at 9 1.2 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 7.7 0.4 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 9 -0.4 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at 7.7 -1.2 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad28)"))
    (pad 29 smd rect (at 9 -2 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad29)"))
    (pad 30 smd rect (at 7.7 -2.8 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad30)"))
    (pad 31 smd rect (at 7.6 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 32 smd rect (at 6.8 -4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 PE3))
    (pad 33 smd rect (at 6 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 PE4))
    (pad 34 smd rect (at 5.2 -4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 PE5))
    (pad 35 smd rect (at 4.4 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad35)"))
    (pad 36 smd rect (at 3.6 -4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad36)"))
    (pad 37 smd rect (at 2.8 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(IC1-Pad37)"))
    (pad 38 smd rect (at 2 -4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(IC1-Pad38)"))
    (pad 39 smd rect (at 1.2 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(IC1-Pad39)"))
    (pad 40 smd rect (at 0.4 -4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 PF0))
    (pad 41 smd rect (at -0.4 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 PF1))
    (pad 42 smd rect (at -1.2 -4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(IC1-Pad42)"))
    (pad 43 smd rect (at -2 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(IC1-Pad43)"))
    (pad 44 smd rect (at -2.8 -4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 45 smd rect (at -3.6 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(IC1-Pad45)"))
    (pad 46 smd rect (at -4.4 -4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(IC1-Pad46)"))
    (pad 47 smd rect (at -5.2 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(IC1-Pad47)"))
    (pad 48 smd rect (at -6 -4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(IC1-Pad48)"))
    (pad 49 smd rect (at -6.8 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 50 smd rect (at -7.6 -4.3 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 51 smd rect (at -8.4 -5.6 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 53 smd circle (at -6.14 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(IC1-Pad53)"))
    (pad 52 smd oval (at -5.8 -1) (size 1.3 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 54 smd oval (at -5.8 1) (size 1.3 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 55 smd oval (at -4.7 0 90) (size 1.3 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 56F970D8)
    (at 158.496 102.87)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value SV3 (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad28)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(IC1-Pad29)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(C1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Header_Straight_1x13 (layer F.Cu) (tedit 56F970BE)
    (at 126.365 118.618 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 2.032 -0.254 180) (layer F.SilkS))
    (fp_text value SV2 (at 0.127 32.639 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 PF0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 PF1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 PE6))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 PD3))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 PD2))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 PD0))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 PD1))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 PB0))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 PB2))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 PB1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 PB3))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 PB4))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x13.wrl
      (at (xyz 0 -0.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 56FFC3D9)
    (at 154.178 105.41)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.028 -1.46 180) (layer F.SilkS))
    (fp_text value 300 (at 0 -1.524) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 PE5))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57013E7D)
    (at 128.524 109.982 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 2.54 -0.762 180) (layer F.SilkS))
    (fp_text value Antenna (at 0 -2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(IC1-Pad53)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 56FFC3CC)
    (at 154.178 107.95)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -0.028 1.4 180) (layer F.SilkS))
    (fp_text value LED (at 0.127 1.524) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module pin-header-mod:Pin_Header_Straight_1x12 (layer F.Cu) (tedit 56F970C9)
    (at 154.305 101.346 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.159 28.194 360) (layer F.SilkS))
    (fp_text value SV1 (at 0 -2.286 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(IC1-Pad29)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad28)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 PE3))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 PE4))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 PE5))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(IC1-Pad39)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(IC1-Pad45)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(IC1-Pad46)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(IC1-Pad47)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(IC1-Pad48)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text D4 (at 156.55 117.5 90) (layer B.SilkS))
  (gr_text MISO (at 154.3 117.6 90) (layer B.SilkS))
  (gr_text MOSI (at 149.25 117.6 90) (layer B.SilkS))
  (gr_text SCK (at 151.75 117.6 90) (layer B.SilkS))
  (gr_text SS (at 146.7 117.6 90) (layer B.SilkS))
  (gr_text SDA (at 144.15 117.6 90) (layer B.SilkS))
  (gr_text SCL (at 141.6 117.6 90) (layer B.SilkS))
  (gr_text RX1 (at 139.05 117.6 90) (layer B.SilkS))
  (gr_text TX1 (at 136.55 117.6 90) (layer B.SilkS))
  (gr_text D3 (at 134 117.6 90) (layer B.SilkS))
  (gr_text RST (at 131.45 117.6 90) (layer B.SilkS))
  (gr_text ADC1 (at 128.9 117.6 90) (layer B.SilkS))
  (gr_text ADC0 (at 126.35 117.6 90) (layer B.SilkS))
  (gr_text 3V3 (at 126.35 102.35 90) (layer B.SilkS))
  (gr_text GND (at 128.9 102.35 90) (layer B.SilkS))
  (gr_text TCK (at 131.45 102.35 90) (layer B.SilkS))
  (gr_text TMS (at 134 102.35 90) (layer B.SilkS))
  (gr_text TDO (at 136.55 102.35 90) (layer B.SilkS))
  (gr_text TDI (at 139.05 102.35 90) (layer B.SilkS))
  (gr_text ARef (at 141.6 102.4 90) (layer B.SilkS))
  (gr_text D2 (at 144.15 102.4 90) (layer B.SilkS))
  (gr_text D1 (at 146.7 102.4 90) (layer B.SilkS))
  (gr_text D0 (at 149.25 102.4 90) (layer B.SilkS))
  (gr_text RX0 (at 151.8 102.4 90) (layer B.SilkS))
  (gr_text TX0 (at 154.3 102.4 90) (layer B.SilkS))
  (gr_text "Merkurboard v2" (at 146.95 110.25) (layer B.SilkS))
  (gr_line (start 125 100) (end 125 120) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160 100) (end 125 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160 120) (end 160 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125 120) (end 160 120) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch full 0.508)
    (priority 1)
    (connect_pads thru_hole_only (clearance 0.22))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.5))
    (polygon
      (pts
        (xy 159.766 119.888) (xy 125.095 119.888) (xy 125.095 100.203) (xy 159.766 100.203)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.5))
    (polygon
      (pts
        (xy 159.8 100.2) (xy 159.75 119.85) (xy 125.15 119.85) (xy 125.2 100.2)
      )
    )
  )
)
