<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.5.1">
<drawing>
<board>
<plain>
<wire x1="7.5" y1="-1.5" x2="102.5" y2="-1.5" width="0" layer="20"/>
<wire x1="110" y1="6.5" x2="110" y2="63.5" width="0" layer="20"/>
<wire x1="102.5" y1="71.5" x2="7.5" y2="71.5" width="0" layer="20"/>
<wire x1="0" y1="63.5" x2="0" y2="6.5" width="0" layer="20"/>
<wire x1="20.5" y1="38.75" x2="20.5" y2="31.5" width="0.1524" layer="20"/>
<wire x1="21.5" y1="30.5" x2="28.5" y2="30.5" width="0.1524" layer="20"/>
<wire x1="29.5" y1="31.5" x2="29.5" y2="38.75" width="0.1524" layer="20"/>
<wire x1="20.5" y1="38.75" x2="21.5" y2="39.5" width="0.1524" layer="20" curve="-90"/>
<wire x1="28.5" y1="39.5" x2="29.5" y2="38.75" width="0.1524" layer="20" curve="-90"/>
<wire x1="29.5" y1="31.5" x2="28.5" y2="30.5" width="0.1524" layer="20" curve="-90"/>
<wire x1="21.5" y1="30.5" x2="20.5" y2="31.5" width="0.1524" layer="20" curve="-90"/>
<text>SET ALL JUMPERS 
TO SHUNT (TPS92661/2)
OR PARALLEL 
(IN2-12 -&gt; OUT2-12)</text>
<text>Shunt mode:
OUT_2: SUP-
OUT_3 - OUT_12: 
Not connected</text>
<text>Parallel mode:
OUT_2: R-
OUT_3: G-
OUT_4: B-
OUT_5: A-
OUT_6: W-
OUT_7: C-
OUT_8: V-
OUT_9: SUP-
OUT_10: IN_10
OUT_11: IN_11
OUT_12: IN_12</text>
<text>Mount holes:
95mm x 57mm
~3.75" x 2.25"</text>
<text>SHNT</text>
<text>SHNT</text>
<text>SHNT</text>
<text>SHNT</text>
<text>SHNT</text>
<text>SHNT</text>
<wire x1="102.5" y1="-1.5" x2="102.5" y2="-0.5" width="0.0254" layer="20"/>
<wire x1="102.5" y1="70.5" x2="102.5" y2="71.5" width="0.0254" layer="20"/>
<wire x1="7.5" y1="70.5" x2="7.5" y2="71.5" width="0.0254" layer="20"/>
<wire x1="7.5" y1="-1.5" x2="7.5" y2="-0.5" width="0.0254" layer="20"/>
<wire x1="7.5" y1="-0.5" x2="0" y2="6.5" width="0.0254" layer="20" curve="-90"/>
<wire x1="7.5" y1="70.5" x2="0" y2="63.5" width="0.0254" layer="20" curve="90"/>
<wire x1="102.5" y1="70.5" x2="110" y2="63.5" width="0.0254" layer="20" curve="-90"/>
<wire x1="102.5" y1="-0.5" x2="110" y2="6.5" width="0.0254" layer="20" curve="90"/>
<text>LZ7-Dual v1
Brooks Talley 2018</text>
<wire x1="21.5" y1="39.5" x2="23.5" y2="39.5" width="0.1524" layer="20"/>
<wire x1="23.5" y1="39.5" x2="24.5" y2="40.5" width="0.1524" layer="20" curve="90"/>
<wire x1="24.5" y1="40.5" x2="24.5" y2="43" width="0.1524" layer="20"/>
<wire x1="24.5" y1="43" x2="25.5" y2="44" width="0.1524" layer="20" curve="-90"/>
<wire x1="25.5" y1="44" x2="26.5" y2="44" width="0.1524" layer="20"/>
<wire x1="26.5" y1="44" x2="27.5" y2="43" width="0.1524" layer="20" curve="-90"/>
<wire x1="28.5" y1="39.5" x2="27.5" y2="40.5" width="0.1524" layer="20" curve="-90"/>
<wire x1="27.5" y1="40.5" x2="27.5" y2="43" width="0.1524" layer="20"/>
<text>CUTOUT</text>
</plain>
<libraries>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,3-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.3 mm, round</description>
</package>
</packages>
</library>
<library name="tangentry">
<packages>
<package name="LZ7-N4M100">
</package>
<package name="LED1-20MM-STAR">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP3Q">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,15/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="H1" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="H2" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="H3" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="H4" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="D1" library="tangentry" package="LZ7-N4M100" value="LZ7-N4M100"/>
<element name="U$1" library="tangentry" package="LED1-20MM-STAR" value="LED1-20MM-STAR">
<attribute name="NAME"/>
</element>
<element name="JP1" library="pinhead" package="1X02" value="LZ7_TEMP">
<attribute name="VALUE"/>
</element>
<element name="CABLE_IN" library="pinhead" package="2X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CABLE_OUT" library="pinhead" package="2X06" value=""/>
<element name="IN_SEL1" library="jumper" package="JP3Q" value=""/>
<element name="OUT_SEL3" library="jumper" package="JP3Q" value=""/>
<element name="OUT_SEL4" library="jumper" package="JP3Q" value=""/>
<element name="OUT_SEL1" library="jumper" package="JP3Q" value=""/>
<element name="OUT_SEL2" library="jumper" package="JP3Q" value=""/>
<element name="LZ7_R+" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_G+" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_B+" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_A+" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_W+" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_C+" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_V+" library="wirepad" package="2,15/1,0" value=""/>
<element name="SUP+" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LZ7_R-" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_G-" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_B-" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_A-" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_W-" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_C-" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_V-" library="wirepad" package="2,15/1,0" value=""/>
<element name="SUP-" library="wirepad" package="2,15/1,0" value=""/>
<element name="LZ7_T1" library="wirepad" package="1,6/0,8" value=""/>
<element name="LZ7_T2" library="wirepad" package="1,6/0,8" value=""/>
<element name="IN_SEL2" library="jumper" package="JP2" value=""/>
<element name="SUP+1" library="wirepad" package="2,15/1,0" value=""/>
<element name="SUP-1" library="wirepad" package="2,15/1,0" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="CABLE_IN" pad="1"/>
<contactref element="H1" pad="B3,3"/>
<contactref element="H2" pad="B3,3"/>
<contactref element="H3" pad="B3,3"/>
<contactref element="H4" pad="B3,3"/>
<contactref element="CABLE_OUT" pad="1"/>
</signal>
<signal name="LED+">
</signal>
<signal name="LED-">
</signal>
<signal name="SUP-">
<contactref element="U$1" pad="L-1"/>
<contactref element="U$1" pad="L-2"/>
<contactref element="OUT_SEL4" pad="4"/>
<contactref element="IN_SEL1" pad="5"/>
<contactref element="SUP-" pad="1"/>
<contactref element="SUP-1" pad="1"/>
</signal>
<signal name="SUP+">
<contactref element="U$1" pad="L+1"/>
<contactref element="U$1" pad="L+2"/>
<contactref element="CABLE_IN" pad="9"/>
<contactref element="OUT_SEL4" pad="5"/>
<contactref element="SUP+" pad="1"/>
<contactref element="SUP+1" pad="1"/>
</signal>
<signal name="LZ7_R+">
<contactref element="D1" pad="1-R+"/>
<contactref element="CABLE_IN" pad="2"/>
<contactref element="LZ7_R+" pad="1"/>
</signal>
<signal name="LZ7_G+">
<contactref element="D1" pad="2-G+"/>
<contactref element="CABLE_IN" pad="3"/>
<contactref element="OUT_SEL1" pad="5"/>
<contactref element="LZ7_G+" pad="1"/>
</signal>
<signal name="LZ7_TEMP1">
<contactref element="D1" pad="1-RT"/>
<contactref element="JP1" pad="2"/>
<contactref element="LZ7_T1" pad="1"/>
</signal>
<signal name="LZ7_TEMP2">
<contactref element="D1" pad="2-RT"/>
<contactref element="JP1" pad="1"/>
<contactref element="LZ7_T2" pad="1"/>
</signal>
<signal name="LZ7_B+">
<contactref element="D1" pad="3-B+"/>
<contactref element="CABLE_IN" pad="4"/>
<contactref element="OUT_SEL1" pad="6"/>
<contactref element="LZ7_B+" pad="1"/>
</signal>
<signal name="LZ7_A+">
<contactref element="D1" pad="4-A+"/>
<contactref element="CABLE_IN" pad="5"/>
<contactref element="IN_SEL1" pad="6"/>
<contactref element="LZ7_A+" pad="1"/>
<contactref element="OUT_SEL2" pad="6"/>
</signal>
<signal name="LZ7_W+">
<contactref element="D1" pad="5-W+"/>
<contactref element="CABLE_IN" pad="6"/>
<contactref element="LZ7_W+" pad="1"/>
<contactref element="OUT_SEL2" pad="5"/>
</signal>
<signal name="LZ7_C-">
<contactref element="D1" pad="6-C-"/>
<contactref element="OUT_SEL3" pad="4"/>
<contactref element="LZ7_C-" pad="1"/>
</signal>
<signal name="LZ7_V+">
<contactref element="D1" pad="7-V+"/>
<contactref element="CABLE_IN" pad="8"/>
<contactref element="OUT_SEL3" pad="6"/>
<contactref element="LZ7_V+" pad="1"/>
<contactref element="IN_SEL2" pad="3"/>
</signal>
<signal name="LZ7_V-">
<contactref element="D1" pad="8-V-"/>
<contactref element="OUT_SEL4" pad="3"/>
<contactref element="LZ7_V-" pad="1"/>
</signal>
<signal name="LZ7_C+">
<contactref element="D1" pad="9-C+"/>
<contactref element="CABLE_IN" pad="7"/>
<contactref element="OUT_SEL3" pad="5"/>
<contactref element="LZ7_C+" pad="1"/>
</signal>
<signal name="LZ7_W-">
<contactref element="D1" pad="10-W-"/>
<contactref element="OUT_SEL3" pad="3"/>
<contactref element="LZ7_W-" pad="1"/>
</signal>
<signal name="LZ7_A-">
<contactref element="D1" pad="11-A-"/>
<contactref element="LZ7_A-" pad="1"/>
<contactref element="OUT_SEL2" pad="3"/>
</signal>
<signal name="LZ7_R-">
<contactref element="D1" pad="14-R-"/>
<contactref element="OUT_SEL1" pad="3"/>
<contactref element="LZ7_R-" pad="1"/>
</signal>
<signal name="LZ7_G-">
<contactref element="D1" pad="13-G-"/>
<contactref element="OUT_SEL1" pad="4"/>
<contactref element="LZ7_G-" pad="1"/>
</signal>
<signal name="LZ7_B-">
<contactref element="D1" pad="12-B-"/>
<contactref element="LZ7_B-" pad="1"/>
<contactref element="OUT_SEL2" pad="4"/>
</signal>
<signal name="OUT_2">
<contactref element="CABLE_OUT" pad="2"/>
<contactref element="OUT_SEL1" pad="1"/>
<contactref element="OUT_SEL4" pad="6"/>
</signal>
<signal name="OUT_4">
<contactref element="CABLE_OUT" pad="4"/>
<contactref element="OUT_SEL2" pad="2"/>
</signal>
<signal name="OUT_6">
<contactref element="CABLE_OUT" pad="6"/>
<contactref element="OUT_SEL3" pad="1"/>
</signal>
<signal name="OUT_8">
<contactref element="CABLE_OUT" pad="8"/>
<contactref element="OUT_SEL4" pad="1"/>
</signal>
<signal name="OUT_10">
<contactref element="CABLE_OUT" pad="10"/>
<contactref element="IN_SEL1" pad="1"/>
</signal>
<signal name="OUT_12">
<contactref element="CABLE_OUT" pad="12"/>
<contactref element="IN_SEL1" pad="2"/>
</signal>
<signal name="OUT_11">
<contactref element="CABLE_OUT" pad="11"/>
<contactref element="IN_SEL2" pad="1"/>
</signal>
<signal name="OUT_9">
<contactref element="CABLE_OUT" pad="9"/>
<contactref element="OUT_SEL4" pad="2"/>
</signal>
<signal name="OUT_7">
<contactref element="CABLE_OUT" pad="7"/>
<contactref element="OUT_SEL3" pad="2"/>
</signal>
<signal name="OUT_5">
<contactref element="CABLE_OUT" pad="5"/>
<contactref element="OUT_SEL2" pad="1"/>
</signal>
<signal name="OUT_3">
<contactref element="CABLE_OUT" pad="3"/>
<contactref element="OUT_SEL1" pad="2"/>
</signal>
<signal name="IN_11">
<contactref element="IN_SEL2" pad="2"/>
<contactref element="CABLE_IN" pad="11"/>
</signal>
<signal name="N$1">
<contactref element="IN_SEL1" pad="3"/>
<contactref element="CABLE_IN" pad="12"/>
</signal>
<signal name="N$2">
<contactref element="IN_SEL1" pad="4"/>
<contactref element="CABLE_IN" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
