(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 126)
    (no_connects 0)
    (area 12.3226 19.325 88.05 55.62658)
    (thickness 1.6)
    (drawings 49)
    (tracks 271)
    (zones 0)
    (modules 43)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 0.889)
    (user_trace_width 1.016)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.22 0.65)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00008_00000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory meta/))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad36)")
  (net 2 "Net-(J1-Pad40)")
  (net 3 "Net-(J1-Pad38)")
  (net 4 "Net-(J1-Pad18)")
  (net 5 "Net-(J1-Pad24)")
  (net 6 "Net-(J1-Pad22)")
  (net 7 "Net-(J1-Pad32)")
  (net 8 "Net-(J1-Pad26)")
  (net 9 "Net-(J1-Pad12)")
  (net 10 "Net-(J1-Pad16)")
  (net 11 "Net-(J1-Pad37)")
  (net 12 "Net-(J1-Pad33)")
  (net 13 "Net-(J1-Pad35)")
  (net 14 "Net-(J1-Pad31)")
  (net 15 "Net-(J1-Pad23)")
  (net 16 "Net-(J1-Pad21)")
  (net 17 "Net-(J1-Pad19)")
  (net 18 "Net-(J1-Pad3)")
  (net 19 "Net-(J1-Pad5)")
  (net 20 "Net-(J1-Pad15)")
  (net 21 "Net-(J1-Pad11)")
  (net 22 GND)
  (net 23 +3V3)
  (net 24 /ID_SC)
  (net 25 /ID_SD)
  (net 26 /W1)
  (net 27 "Net-(R4-Pad2)")
  (net 28 /TC1-)
  (net 29 /TC1+)
  (net 30 /TC2-)
  (net 31 /TC2+)
  (net 32 /TC3-)
  (net 33 /TC3+)
  (net 34 /TC4-)
  (net 35 /TC4+)
  (net 36 +5V)
  (net 37 "Net-(BZ1-Pad2)")
  (net 38 /ALERT)
  (net 39 "Net-(J1-Pad29)")
  (net 40 "Net-(J1-Pad10)")
  (net 41 "Net-(J1-Pad8)")
  (net 42 +3.3VA)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3.3VA)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ALERT)
    (add_net /ID_SC)
    (add_net /ID_SD)
    (add_net /TC1+)
    (add_net /TC1-)
    (add_net /TC2+)
    (add_net /TC2-)
    (add_net /TC3+)
    (add_net /TC3-)
    (add_net /TC4+)
    (add_net /TC4-)
    (add_net /W1)
    (add_net GND)
    (add_net "Net-(BZ1-Pad2)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad29)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad31)")
    (add_net "Net-(J1-Pad32)")
    (add_net "Net-(J1-Pad33)")
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J1-Pad37)")
    (add_net "Net-(J1-Pad38)")
    (add_net "Net-(J1-Pad40)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(R4-Pad2)")
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58E7946C)
    (at 21.5 41.25 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 2.2uF (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 2.455 -0.335 360) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 22 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 42 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.00mm (layer F.Cu) (tedit 58C9CED9)
    (at 20.5 49.5 90)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (fp_text reference P6 (at 0 -2.25 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 6.12 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 +3.3VA))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /W1))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 67.31 50.8 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58CC2367)
    (at 29.21 45.085 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0.254 1.397 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.254 1.397 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 /TC1+))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 /TC1-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58C9CEF7)
    (at 60.96 47.625 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P4 (at -0.125 -2.54 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.93 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /TC4+))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /TC4-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DFN_QFN_ML:TDFN-10-1EP_3x4mm_Pitch0.5mm (layer F.Cu) (tedit 58C34657)
    (at 29.845 40.005 90)
    (descr "10-Lead Thin Dual Flatpack No Leads, Exposed Pad")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0.005 -2.845 360) (layer F.SilkS))
    (fp_text value MAX31850K (at 0 2.575 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.92 -1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at -1.92 -0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /TC1-))
    (pad 3 smd rect (at -1.92 0 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /TC1+))
    (pad 4 smd rect (at -1.92 0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 5 smd rect (at -1.92 1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /W1))
    (pad 6 smd rect (at 1.92 1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 7 smd rect (at 1.92 0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 8 smd rect (at 1.92 0 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 9 smd rect (at 1.92 -0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 10 smd rect (at 1.92 -1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.65 0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at 0.65 -0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.65 0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.65 -0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CCB)
    (at 16 51)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217C7B)
    (at 74 28)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CCB)
    (at 74 51)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CA2)
    (at 16 28)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58CC235F)
    (at 31.75 43.18 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at -2.286 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58CC2338)
    (at 41.91 43.18 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -2.34 -0.07 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at -2.34 -0.07 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E30E40)
    (at 39.37 45.085 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0.254 1.397 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.254 1.397 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 /TC2+))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 /TC2-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58CC23D8)
    (at 52.07 43.18 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at -2.286 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58CC247B)
    (at 69.5 40)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.25 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at -2.25 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58CC23F9)
    (at 49.53 45.085 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0.254 1.397 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.254 1.397 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 /TC3+))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 32 /TC3-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58CC2482)
    (at 62.23 43.18 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -2.286 -0.07 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at -2.286 -0.07 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58CC23ED)
    (at 59.69 45.085 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0.254 1.397 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.254 1.397 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 /TC4+))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 /TC4-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58CC239A)
    (at 25.5 43.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 2 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /W1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58CC2450)
    (at 63.5 36)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2 -0.5) (layer F.SilkS))
    (fp_text value 3.9k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at -2 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /ID_SC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58CC2458)
    (at 63.5 34.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2 -0.5) (layer F.SilkS))
    (fp_text value 3.9k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at -2 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /ID_SD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58CC2447)
    (at 63.5 37.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2 -0.5) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at -2 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_B3U-3000P-B (layer F.Cu) (tedit 58C9CF68)
    (at 76 36.5 270)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, without Ground Terminal, with Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 3.505 0.435 540) (layer F.SilkS))
    (fp_text value Write (at 0 2.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 3.505 0.435 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.7 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad2)"))
    (pad 2 smd rect (at 1.7 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module Housings_DFN_QFN_ML:TDFN-10-1EP_3x4mm_Pitch0.5mm (layer F.Cu) (tedit 58C34654)
    (at 40.005 40.005 90)
    (descr "10-Lead Thin Dual Flatpack No Leads, Exposed Pad")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U3 (at 0.005 -2.755 360) (layer F.SilkS))
    (fp_text value MAX31850K (at 0 2.575 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.92 -1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at -1.92 -0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /TC2-))
    (pad 3 smd rect (at -1.92 0 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /TC2+))
    (pad 4 smd rect (at -1.92 0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 5 smd rect (at -1.92 1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /W1))
    (pad 6 smd rect (at 1.92 1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 7 smd rect (at 1.92 0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 8 smd rect (at 1.92 0 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 9 smd rect (at 1.92 -0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 10 smd rect (at 1.92 -1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.65 0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at 0.65 -0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.65 0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.65 -0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN_ML:TDFN-10-1EP_3x4mm_Pitch0.5mm (layer F.Cu) (tedit 58C34651)
    (at 50.165 40 90)
    (descr "10-Lead Thin Dual Flatpack No Leads, Exposed Pad")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U4 (at 0 -2.915 360) (layer F.SilkS))
    (fp_text value MAX31850K (at 0 2.575 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.92 -1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at -1.92 -0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /TC3-))
    (pad 3 smd rect (at -1.92 0 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /TC3+))
    (pad 4 smd rect (at -1.92 0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 5 smd rect (at -1.92 1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /W1))
    (pad 6 smd rect (at 1.92 1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 7 smd rect (at 1.92 0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 8 smd rect (at 1.92 0 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 9 smd rect (at 1.92 -0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 10 smd rect (at 1.92 -1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.65 0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at 0.65 -0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.65 0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.65 -0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58C9CF06)
    (at 69.5 36.5 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 0 3.5 180) (layer F.SilkS))
    (fp_text value AT24CS32 (at 0 3.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /ID_SD))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /ID_SC))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN_ML:TDFN-10-1EP_3x4mm_Pitch0.5mm (layer F.Cu) (tedit 58C3464D)
    (at 60.325 40.005 90)
    (descr "10-Lead Thin Dual Flatpack No Leads, Exposed Pad")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U6 (at 0.005 -2.825 360) (layer F.SilkS))
    (fp_text value MAX31850K (at 0 2.575 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.92 -1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at -1.92 -0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 /TC4-))
    (pad 3 smd rect (at -1.92 0 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /TC4+))
    (pad 4 smd rect (at -1.92 0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 5 smd rect (at -1.92 1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /W1))
    (pad 6 smd rect (at 1.92 1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 7 smd rect (at 1.92 0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 8 smd rect (at 1.92 0 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 9 smd rect (at 1.92 -0.5 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 10 smd rect (at 1.92 -1 90) (size 0.79 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.65 0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at 0.65 -0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.65 0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.65 -0.575 90) (size 1.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 22 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58C9CEDD)
    (at 30.48 47.625 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at -0.125 -2.52 540) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.93 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /TC1+))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /TC1-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58C9CEE1)
    (at 40.64 47.625 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P2 (at -0.125 -2.36 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.93 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /TC2+))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /TC2-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58C9CEEC)
    (at 50.8 47.625 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 0 -2.39 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.93 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /TC3+))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /TC3-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module cui-ml:CMI-9655S-SMT (layer F.Cu) (tedit 58CC22FF)
    (at 19 36.25)
    (descr "Buzzer, Magnetic Indicator")
    (tags CUI)
    (fp_text reference BZ1 (at -5.5 -3.25 90) (layer F.SilkS))
    (fp_text value Buzzer (at 0 6) (layer F.Fab) hide)
    (fp_text user + (at -5.5 4) (layer F.Fab))
    (fp_text user %R (at 5.588 4.876 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -4 0) (size 3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 36 +5V))
    (pad 2 smd rect (at 4 0) (size 3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(BZ1-Pad2)"))
    (model Buzzers_Beepers.3dshapes/MagneticBuzzer_Kingstate_KCG0601.wrl
      (at (xyz 0.124803 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23 (layer F.Cu) (tedit 58C9CF1D)
    (at 26 34.5 180)
    (descr "3-pin TSOT23 package, http://www.analog.com.tw/pdf/All_In_One.pdf")
    (tags TSOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.584 180) (layer F.SilkS))
    (fp_text value NUD3124 (at 0 2.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.31 -0.95 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 38 /ALERT))
    (pad 2 smd rect (at -1.31 0.95 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 3 smd rect (at 1.31 0 180) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(BZ1-Pad2)"))
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 67.31 50.8)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module raspberry-ml:Pin_Header_Straight_2x20 locked (layer F.Cu) (tedit 58C9CF2F)
    (at 45 28 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at -3.496 0.212 360) (layer F.SilkS))
    (fp_text value RPi_GPIO (at -1.27 -27.23 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 +3V3))
    (pad 2 thru_hole oval (at 1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 +5V))
    (pad 3 thru_hole oval (at -1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 +5V))
    (pad 5 thru_hole oval (at -1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GND))
    (pad 7 thru_hole oval (at -1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /W1))
    (pad 8 thru_hole oval (at 1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at -1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GND))
    (pad 10 thru_hole oval (at 1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at -1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at -1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /ALERT))
    (pad 14 thru_hole oval (at 1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GND))
    (pad 15 thru_hole oval (at -1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at -1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 +3V3))
    (pad 18 thru_hole oval (at 1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad18)"))
    (pad 19 thru_hole oval (at -1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad19)"))
    (pad 20 thru_hole oval (at 1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GND))
    (pad 21 thru_hole oval (at -1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad21)"))
    (pad 22 thru_hole oval (at 1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad22)"))
    (pad 23 thru_hole oval (at -1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad23)"))
    (pad 24 thru_hole oval (at 1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad24)"))
    (pad 25 thru_hole oval (at -1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GND))
    (pad 26 thru_hole oval (at 1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad26)"))
    (pad 27 thru_hole oval (at -1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /ID_SD))
    (pad 28 thru_hole oval (at 1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /ID_SC))
    (pad 29 thru_hole oval (at -1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J1-Pad29)"))
    (pad 30 thru_hole oval (at 1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GND))
    (pad 31 thru_hole oval (at -1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad31)"))
    (pad 32 thru_hole oval (at 1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad32)"))
    (pad 33 thru_hole oval (at -1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad33)"))
    (pad 34 thru_hole oval (at 1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GND))
    (pad 35 thru_hole oval (at -1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad35)"))
    (pad 36 thru_hole oval (at 1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad36)"))
    (pad 37 thru_hole oval (at -1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad37)"))
    (pad 38 thru_hole oval (at 1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad38)"))
    (pad 39 thru_hole oval (at -1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GND))
    (pad 40 thru_hole oval (at 1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad40)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D7F78C)
    (at 22.479 47.752)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -3.729 -0.002 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 2.921 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D8025A)
    (at 29.083 33.782 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.02184 -0.00508 540) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at -1.778 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 /ALERT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58D80231)
    (at 21.21 46.5)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U2 (at 1.29 -3.25) (layer F.SilkS))
    (fp_text value DS18S20 (at 1.25 3) (layer F.Fab) hide)
    (fp_text user %R (at 4.698 -1.288) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 26 /W1))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 42 +3.3VA))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 22 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E79470)
    (at 31.75 44.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 2.794 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 2.794 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E79473)
    (at 41.91 44.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 2.84 0.05) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 2.794 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E79479)
    (at 52.07 44.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 2.794 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 2.794 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E7947C)
    (at 62.23 44.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 2.794 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 2.794 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 +3.3VA))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58E7945F)
    (at 15 41.25 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -1.5 270) (layer B.SilkS))
    (fp_text value 2.2uF (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at -0.125 1.505 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 22 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 36 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer B.Cu) (tedit 58E79852)
    (at 18.25 41.75 270)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3 Housing ")
    (attr smd)
    (fp_text reference U7 (at -3 0 360) (layer B.SilkS))
    (fp_text value MCP1754ST (at 0.45 -3.25 270) (layer B.Fab) hide)
    (fp_text user %R (at 0.38 0 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.48 1.5) (size 1 1.5) (layers B.Cu B.Paste B.Mask)
      (net 36 +5V))
    (pad 2 smd rect (at -1.48 0) (size 1 1.5) (layers B.Cu B.Paste B.Mask)
      (net 22 GND))
    (pad 3 smd rect (at -1.48 -1.5) (size 1 1.5) (layers B.Cu B.Paste B.Mask)
      (net 42 +3.3VA))
    (pad 2 smd rect (at 1.48 0) (size 2 3) (layers B.Cu B.Paste B.Mask)
      (net 22 GND))
    (pad 2 smd trapezoid (at -0.37 0 180) (size 1.5 0.75) (rect_delta 0 -0.5 ) (layers B.Cu B.Paste B.Mask)
      (net 22 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0.02 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "by Mike Lawrence" (at 60.452 39.116) (layer B.SilkS))
  (gr_text "Thermocouple pHat" (at 37.465 33.655) (layer F.SilkS))
  (gr_text Write (at 74.93 33.02) (layer F.SilkS))
  (gr_text DQ (at 22.5 51 90) (layer B.SilkS))
  (gr_text GND (at 24.5 51 90) (layer B.SilkS))
  (gr_text VDD (at 20.5 51 90) (layer B.SilkS))
  (gr_text TC1 (at 29.21 52.578) (layer B.SilkS))
  (gr_text - (at 27.94 50.292) (layer B.SilkS))
  (gr_text + (at 30.48 50.292) (layer B.SilkS))
  (gr_text TC3 (at 49.53 52.578) (layer B.SilkS))
  (gr_text + (at 50.8 50.038) (layer B.SilkS))
  (gr_text - (at 48.26 50.038) (layer B.SilkS))
  (gr_text TC2 (at 39.37 52.578) (layer B.SilkS))
  (gr_text + (at 40.64 50.038) (layer B.SilkS))
  (gr_text - (at 38.1 50.292) (layer B.SilkS))
  (gr_text TC4 (at 59.69 52.578) (layer B.SilkS))
  (gr_text - (at 58.42 50.038) (layer B.SilkS))
  (gr_text + (at 60.96 50.038) (layer B.SilkS))
  (gr_text "Apr 2017" (at 75.75 45.5) (layer B.SilkS))
  (gr_text "Rev 1.2" (at 76 42.75) (layer B.SilkS))
  (gr_text "Thermocouple pHat" (at 60.452 35.56) (layer B.SilkS))
  (gr_text "Apr 2017" (at 66.75 45.25) (layer F.SilkS))
  (gr_text "Rev 1.2" (at 66.75 43) (layer F.SilkS))
  (gr_text "by Mike Lawrence" (at 37.338 35.56) (layer F.SilkS))
  (gr_text GND (at 24.5 51 90) (layer F.SilkS))
  (gr_text DQ (at 22.5 51 90) (layer F.SilkS))
  (gr_text VDD (at 20.5 51 90) (layer F.SilkS))
  (gr_text - (at 58.42 50.038) (layer F.SilkS))
  (gr_text - (at 48.26 50.038) (layer F.SilkS))
  (gr_text - (at 38.1 50.292) (layer F.SilkS))
  (gr_text + (at 60.96 50.038) (layer F.SilkS))
  (gr_text + (at 50.8 50.038) (layer F.SilkS))
  (gr_text + (at 40.64 50.038) (layer F.SilkS))
  (gr_text - (at 27.94 50.292) (layer F.SilkS))
  (gr_text + (at 30.48 50.292) (layer F.SilkS))
  (gr_text TC4 (at 59.69 52.578) (layer F.SilkS))
  (gr_text TC3 (at 49.53 52.578) (layer F.SilkS))
  (gr_text TC2 (at 39.37 52.578) (layer F.SilkS))
  (gr_text TC1 (at 29.21 52.578) (layer F.SilkS))
  (dimension 30 (width 0.15) (layer F.Fab)
    (gr_text "30.000 mm" (at 81.55 39.5 270) (layer F.Fab))
    (feature1 (pts (xy 78.5 54.5) (xy 82.6 54.5)))
    (feature2 (pts (xy 78.5 24.5) (xy 82.6 24.5)))
    (crossbar (pts (xy 80.5 24.5) (xy 80.5 54.5)))
    (arrow1a (pts (xy 80.5 54.5) (xy 79.913579 53.373496)))
    (arrow1b (pts (xy 80.5 54.5) (xy 81.086421 53.373496)))
    (arrow2a (pts (xy 80.5 24.5) (xy 79.913579 25.626504)))
    (arrow2b (pts (xy 80.5 24.5) (xy 81.086421 25.626504)))
  )
  (dimension 65 (width 0.15) (layer F.Fab)
    (gr_text "65.000 mm" (at 45 20.45) (layer F.Fab))
    (feature1 (pts (xy 77.5 23.5) (xy 77.5 19.4)))
    (feature2 (pts (xy 12.5 23.5) (xy 12.5 19.4)))
    (crossbar (pts (xy 12.5 21.5) (xy 77.5 21.5)))
    (arrow1a (pts (xy 77.5 21.5) (xy 76.373496 22.086421)))
    (arrow1b (pts (xy 77.5 21.5) (xy 76.373496 20.913579)))
    (arrow2a (pts (xy 12.5 21.5) (xy 13.626504 22.086421)))
    (arrow2b (pts (xy 12.5 21.5) (xy 13.626504 20.913579)))
  )
  (gr_arc (start 74.5 51.5) (end 77.5 51.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 15.5 51.5) (end 15.5 54.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 15.5 27.5) (end 12.5 27.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 74.5 27.5) (end 74.5 24.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 12.5 27.5) (end 12.5 51.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 15.5 54.5) (end 74.5 54.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 77.5 27.5) (end 77.5 51.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 15.5 24.5) (end 74.5 24.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 22) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 12.5 24.5) (xy 77.5 24.5) (xy 77.5 54.5) (xy 12.5 54.5)
      )
    )
  )
  (zone (net 42) (net_name +3.3VA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 12.5 24.5) (xy 77.5 24.5) (xy 77.5 54.5) (xy 12.5 54.5)
      )
    )
  )
)
