(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 89)
    (no_connects 0)
    (area 166.294999 102.794999 207.085001 130.885001)
    (thickness 1.6)
    (drawings 5)
    (tracks 605)
    (zones 0)
    (modules 24)
    (nets 62)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.125 1.125)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF1F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U2-Pad5)")
  (net 2 "Net-(U3-Pad5)")
  (net 3 "Net-(U4-Pad5)")
  (net 4 "Net-(U5-Pad5)")
  (net 5 "Net-(U1-Pad7)")
  (net 6 "Net-(U1-Pad8)")
  (net 7 "Net-(U1-Pad29)")
  (net 8 /OE)
  (net 9 /A0)
  (net 10 /A1)
  (net 11 /A2)
  (net 12 /A3)
  (net 13 /A4)
  (net 14 /A5)
  (net 15 /A6)
  (net 16 /A7)
  (net 17 /A8)
  (net 18 /A9)
  (net 19 /A10)
  (net 20 /A11)
  (net 21 /GND)
  (net 22 /LE)
  (net 23 /A12)
  (net 24 /A13)
  (net 25 /A14)
  (net 26 /A15)
  (net 27 /MOSI)
  (net 28 /MISO)
  (net 29 /SCK)
  (net 30 /RESET)
  (net 31 /VCC)
  (net 32 "Net-(J2-Pad6)")
  (net 33 "Net-(J2-Pad7)")
  (net 34 "Net-(J2-Pad8)")
  (net 35 /An0)
  (net 36 "Net-(Q1-Pad2)")
  (net 37 /An1)
  (net 38 "Net-(Q2-Pad2)")
  (net 39 /An2)
  (net 40 "Net-(Q3-Pad2)")
  (net 41 /An3)
  (net 42 "Net-(Q4-Pad2)")
  (net 43 "Net-(R1-Pad2)")
  (net 44 "Net-(R2-Pad2)")
  (net 45 "Net-(R3-Pad2)")
  (net 46 "Net-(R4-Pad2)")
  (net 47 /Ca)
  (net 48 "Net-(R5-Pad2)")
  (net 49 /Cb)
  (net 50 "Net-(R6-Pad2)")
  (net 51 /Cc)
  (net 52 "Net-(R7-Pad2)")
  (net 53 /Cd)
  (net 54 "Net-(R8-Pad2)")
  (net 55 /Ce)
  (net 56 "Net-(R9-Pad2)")
  (net 57 /Cf)
  (net 58 "Net-(R10-Pad2)")
  (net 59 /Cg)
  (net 60 "Net-(R11-Pad2)")
  (net 61 /DVCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /An0)
    (add_net /An1)
    (add_net /An2)
    (add_net /An3)
    (add_net /Ca)
    (add_net /Cb)
    (add_net /Cc)
    (add_net /Cd)
    (add_net /Ce)
    (add_net /Cf)
    (add_net /Cg)
    (add_net /DVCC)
    (add_net /GND)
    (add_net /LE)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /OE)
    (add_net /RESET)
    (add_net /SCK)
    (add_net /VCC)
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U5-Pad5)")
  )
  (module Local:VDMR10A1 (layer F.Cu) (tedit 5A997519)
    (at 167.64 109.22)
    (tags VDMR10A1)
    (fp_text reference U2 (at 3.8 11.3) (layer F.SilkS))
    (fp_text value 7SEGMENT_CA (at 3.8 3.5) (layer F.Fab))
    (pad 7 smd rect (at 5.7 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 47 /Ca))
    (pad 6 smd rect (at 7.6 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 49 /Cb))
    (pad 1 smd rect (at 0 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 55 /Ce))
    (pad 2 smd rect (at 1.9 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 53 /Cd))
    (pad 3 smd rect (at 3.8 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q1-Pad2)"))
    (pad 4 smd rect (at 5.7 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 51 /Cc))
    (pad 5 smd rect (at 7.6 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U2-Pad5)"))
    (pad 8 smd rect (at 3.8 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q1-Pad2)"))
    (pad 9 smd rect (at 1.9 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 57 /Cf))
    (pad 10 smd rect (at 0 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 59 /Cg))
    (model /Users/travis/Documents/vdmx10a1.wrl
      (at (xyz -0.05 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_QFP:TQFP-44-1EP_10x10mm_Pitch0.8mm (layer B.Cu) (tedit 5A9B4F9C)
    (at 186.69 116.84 315)
    (descr "44-Lead Plastic Thin Quad Flatpack (MW) - 10x10x1.0 mm Body [TQFP] With 4.5x4.5 mm Exposed Pad (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 7.45 315) (layer B.SilkS))
    (fp_text value ATMEGA164A-AU (at 0 -7.45 315) (layer B.Fab))
    (fp_text user %R (at 0 0 315) (layer B.Fab))
    (pad 1 smd rect (at -5.7 4 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 27 /MOSI))
    (pad 2 smd rect (at -5.7 3.2 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 28 /MISO))
    (pad 3 smd rect (at -5.7 2.4 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 29 /SCK))
    (pad 4 smd rect (at -5.7 1.6 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 30 /RESET))
    (pad 5 smd rect (at -5.7 0.8 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 31 /VCC))
    (pad 6 smd rect (at -5.7 0 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 /GND))
    (pad 7 smd rect (at -5.7 -0.8 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at -5.7 -1.6 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -5.7 -2.4 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R5-Pad2)"))
    (pad 10 smd rect (at -5.7 -3.2 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R6-Pad2)"))
    (pad 11 smd rect (at -5.7 -4 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(R7-Pad2)"))
    (pad 12 smd rect (at -4 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(R8-Pad2)"))
    (pad 13 smd rect (at -3.2 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(R9-Pad2)"))
    (pad 14 smd rect (at -2.4 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(R10-Pad2)"))
    (pad 15 smd rect (at -1.6 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R11-Pad2)"))
    (pad 16 smd rect (at -0.8 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 22 /LE))
    (pad 17 smd rect (at 0 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 31 /VCC))
    (pad 18 smd rect (at 0.8 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 /GND))
    (pad 19 smd rect (at 1.6 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 17 /A8))
    (pad 20 smd rect (at 2.4 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 18 /A9))
    (pad 21 smd rect (at 3.2 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 19 /A10))
    (pad 22 smd rect (at 4 -5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 20 /A11))
    (pad 23 smd rect (at 5.7 -4 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 23 /A12))
    (pad 24 smd rect (at 5.7 -3.2 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 24 /A13))
    (pad 25 smd rect (at 5.7 -2.4 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 25 /A14))
    (pad 26 smd rect (at 5.7 -1.6 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 26 /A15))
    (pad 27 smd rect (at 5.7 -0.8 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 31 /VCC))
    (pad 28 smd rect (at 5.7 0 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 /GND))
    (pad 29 smd rect (at 5.7 0.8 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 5.7 1.6 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 16 /A7))
    (pad 31 smd rect (at 5.7 2.4 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 15 /A6))
    (pad 32 smd rect (at 5.7 3.2 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 14 /A5))
    (pad 33 smd rect (at 5.7 4 315) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 13 /A4))
    (pad 34 smd rect (at 4 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 12 /A3))
    (pad 35 smd rect (at 3.2 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 11 /A2))
    (pad 36 smd rect (at 2.4 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 10 /A1))
    (pad 37 smd rect (at 1.6 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 9 /A0))
    (pad 38 smd rect (at 0.8 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 31 /VCC))
    (pad 39 smd rect (at 0 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 /GND))
    (pad 40 smd rect (at -0.8 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(R1-Pad2)"))
    (pad 41 smd rect (at -1.6 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(R2-Pad2)"))
    (pad 42 smd rect (at -2.4 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R3-Pad2)"))
    (pad 43 smd rect (at -3.2 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R4-Pad2)"))
    (pad 44 smd rect (at -4 5.7 225) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /OE))
    (pad 45 smd rect (at 1.6875 -1.6875 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 1.6875 -0.5625 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 1.6875 0.5625 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 1.6875 1.6875 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 0.5625 -1.6875 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 0.5625 -0.5625 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 0.5625 0.5625 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 0.5625 1.6875 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -0.5625 -1.6875 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -0.5625 -0.5625 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -0.5625 0.5625 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -0.5625 1.6875 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -1.6875 -1.6875 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -1.6875 -0.5625 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -1.6875 0.5625 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -1.6875 1.6875 315) (size 1.125 1.125) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-44-1EP_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Local:VDMR10A1 (layer F.Cu) (tedit 5A997519)
    (at 198.12 109.22)
    (tags VDMR10A1)
    (fp_text reference U5 (at 3.8 11.3) (layer F.SilkS))
    (fp_text value 7SEGMENT_CA (at 3.8 3.5) (layer F.Fab))
    (pad 7 smd rect (at 5.7 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 47 /Ca))
    (pad 6 smd rect (at 7.6 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 49 /Cb))
    (pad 1 smd rect (at 0 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 55 /Ce))
    (pad 2 smd rect (at 1.9 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 53 /Cd))
    (pad 3 smd rect (at 3.8 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(Q4-Pad2)"))
    (pad 4 smd rect (at 5.7 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 51 /Cc))
    (pad 5 smd rect (at 7.6 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U5-Pad5)"))
    (pad 8 smd rect (at 3.8 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(Q4-Pad2)"))
    (pad 9 smd rect (at 1.9 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 57 /Cf))
    (pad 10 smd rect (at 0 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 59 /Cg))
    (model /Users/travis/Documents/vdmx10a1.wrl
      (at (xyz -0.05 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 90))
    )
  )
  (module Local:VDMR10A1 (layer F.Cu) (tedit 5A997519)
    (at 187.96 109.22)
    (tags VDMR10A1)
    (fp_text reference U4 (at 3.8 11.3) (layer F.SilkS))
    (fp_text value 7SEGMENT_CA (at 3.8 3.5) (layer F.Fab))
    (pad 7 smd rect (at 5.7 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 47 /Ca))
    (pad 6 smd rect (at 7.6 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 49 /Cb))
    (pad 1 smd rect (at 0 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 55 /Ce))
    (pad 2 smd rect (at 1.9 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 53 /Cd))
    (pad 3 smd rect (at 3.8 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(Q3-Pad2)"))
    (pad 4 smd rect (at 5.7 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 51 /Cc))
    (pad 5 smd rect (at 7.6 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U4-Pad5)"))
    (pad 8 smd rect (at 3.8 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(Q3-Pad2)"))
    (pad 9 smd rect (at 1.9 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 57 /Cf))
    (pad 10 smd rect (at 0 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 59 /Cg))
    (model /Users/travis/Documents/vdmx10a1.wrl
      (at (xyz -0.05 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 90))
    )
  )
  (module Local:VDMR10A1 (layer F.Cu) (tedit 5A997519)
    (at 177.8 109.22)
    (tags VDMR10A1)
    (fp_text reference U3 (at 3.8 11.3) (layer F.SilkS))
    (fp_text value 7SEGMENT_CA (at 3.8 3.5) (layer F.Fab))
    (pad 7 smd rect (at 5.7 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 47 /Ca))
    (pad 6 smd rect (at 7.6 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 49 /Cb))
    (pad 1 smd rect (at 0 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 55 /Ce))
    (pad 2 smd rect (at 1.9 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 53 /Cd))
    (pad 3 smd rect (at 3.8 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Q2-Pad2)"))
    (pad 4 smd rect (at 5.7 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 51 /Cc))
    (pad 5 smd rect (at 7.6 15) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U3-Pad5)"))
    (pad 8 smd rect (at 3.8 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Q2-Pad2)"))
    (pad 9 smd rect (at 1.9 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 57 /Cf))
    (pad 10 smd rect (at 0 0) (size 1.65 3) (layers F.Cu F.Paste F.Mask)
      (net 59 /Cg))
    (model /Users/travis/Documents/vdmx10a1.wrl
      (at (xyz -0.05 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 170.18 129.54 270)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x14 (at 0 -35.35 270) (layer B.Fab))
    (fp_text user %R (at 0 -16.51 540) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /OE))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /A0))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A1))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A2))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /A3))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A4))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A5))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A6))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A7))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /A8))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A9))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A10))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /A11))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 203.2 104.14 90)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 90) (layer B.SilkS))
    (fp_text value Conn_01x14 (at 0 -35.35 90) (layer B.Fab))
    (fp_text user %R (at 0 -16.51 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /LE))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /A12))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /A13))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /A14))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /A15))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 /DVCC))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /RESET))
    (pad 11 thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /SCK))
    (pad 12 thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /MISO))
    (pad 13 thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /MOSI))
    (pad 14 thru_hole oval (at 0 -33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23 (layer B.Cu) (tedit 58CE4E80)
    (at 171.8056 111.5568 180)
    (descr "3-pin TSOT23 package, http://www.analog.com.tw/pdf/All_In_One.pdf")
    (tags TSOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 2.45 180) (layer B.SilkS))
    (fp_text value MMBT3906 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1.31 0.95 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 35 /An0))
    (pad 2 smd rect (at -1.31 -0.95 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 1.31 0 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 61 /DVCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23 (layer B.Cu) (tedit 58CE4E80)
    (at 171.8056 115.0366 180)
    (descr "3-pin TSOT23 package, http://www.analog.com.tw/pdf/All_In_One.pdf")
    (tags TSOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 2.45 180) (layer B.SilkS))
    (fp_text value MMBT3906 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1.31 0.95 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 37 /An1))
    (pad 2 smd rect (at -1.31 -0.95 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(Q2-Pad2)"))
    (pad 3 smd rect (at 1.31 0 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 61 /DVCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23 (layer B.Cu) (tedit 58CE4E80)
    (at 171.8056 118.5418 180)
    (descr "3-pin TSOT23 package, http://www.analog.com.tw/pdf/All_In_One.pdf")
    (tags TSOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 2.45 180) (layer B.SilkS))
    (fp_text value MMBT3906 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1.31 0.95 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 39 /An2))
    (pad 2 smd rect (at -1.31 -0.95 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(Q3-Pad2)"))
    (pad 3 smd rect (at 1.31 0 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 61 /DVCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23 (layer B.Cu) (tedit 58CE4E80)
    (at 171.8056 122.047 180)
    (descr "3-pin TSOT23 package, http://www.analog.com.tw/pdf/All_In_One.pdf")
    (tags TSOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 2.45 180) (layer B.SilkS))
    (fp_text value MMBT3906 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1.31 0.95 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 41 /An3))
    (pad 2 smd rect (at -1.31 -0.95 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(Q4-Pad2)"))
    (pad 3 smd rect (at 1.31 0 180) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 61 /DVCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 176.1744 123.5202)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.45) (layer B.SilkS))
    (fp_text value 300 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 41 /An3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 176.1744 122.047)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.45) (layer B.SilkS))
    (fp_text value 300 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 39 /An2))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 176.1744 120.5738)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.45) (layer B.SilkS))
    (fp_text value 300 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 37 /An1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5A9ADC64)
    (at 176.1744 119.1006)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.45) (layer B.SilkS))
    (fp_text value 300 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 35 /An0))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 182.3212 107.7722 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 115 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 /Ca))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 203.835 113.1062 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 115 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 /Cb))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 203.835 120.2436 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value 115 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 51 /Cc))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 200.0504 125.4506 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value 115 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 53 /Cd))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 198.1454 124.8156 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value 115 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 55 /Ce))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 200.0504 108.0262 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 115 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 57 /Cf))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 198.0946 110.3122 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value 115 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 /Cg))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 198.0946 114.173 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.5 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 21 /GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 31 /VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 168.656 114.7318 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.5 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 21 /GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 31 /VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 166.37 102.87) (end 166.37 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 130.81) (end 166.37 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207.01 130.81) (end 166.37 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207.01 102.87) (end 207.01 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 102.87) (end 207.01 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 21) (net_name /GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 102.87) (xy 207.01 102.87) (xy 207.01 130.81) (xy 166.37 130.81) (xy 166.37 103.505)
      )
    )
  )
  (zone (net 21) (net_name /GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 102.87) (xy 207.01 102.87) (xy 207.01 130.81) (xy 166.37 130.81) (xy 166.37 103.505)
      )
    )
  )
  (zone (net 21) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 102.87) (xy 207.01 102.87) (xy 207.01 130.81) (xy 166.37 130.81)
      )
    )
  )
  (zone (net 21) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 102.87) (xy 207.01 102.87) (xy 207.01 130.81) (xy 166.37 130.81)
      )
    )
  )
)
