(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(U1-Pad1)")
  (net 2 "unconnected-(U1-Pad2)")
  (net 3 "unconnected-(U1-Pad3)")
  (net 4 "unconnected-(U1-Pad4)")
  (net 5 "unconnected-(U1-Pad5)")
  (net 6 "unconnected-(U1-Pad6)")
  (net 7 "unconnected-(U1-Pad7)")
  (net 8 "unconnected-(U1-Pad8)")
  (net 9 "unconnected-(U1-Pad9)")
  (net 10 "unconnected-(U1-Pad10)")
  (net 11 "unconnected-(U1-Pad11)")
  (net 12 "unconnected-(U1-Pad12)")
  (net 13 "unconnected-(U1-Pad13)")
  (net 14 "unconnected-(U1-Pad14)")
  (net 15 "unconnected-(U1-Pad15)")
  (net 16 "unconnected-(U1-Pad16)")
  (net 17 "unconnected-(U1-Pad17)")
  (net 18 "unconnected-(U1-Pad18)")
  (net 19 "unconnected-(U1-Pad19)")
  (net 20 "unconnected-(U1-Pad20)")
  (net 21 "unconnected-(U1-Pad21)")
  (net 22 "unconnected-(U1-Pad22)")
  (net 23 "unconnected-(U1-Pad23)")
  (net 24 "unconnected-(U1-Pad24)")
  (net 25 "unconnected-(U1-Pad25)")
  (net 26 "unconnected-(U1-Pad26)")
  (net 27 "unconnected-(U1-Pad27)")
  (net 28 "unconnected-(U1-Pad28)")
  (net 29 "unconnected-(U1-Pad29)")
  (net 30 "unconnected-(U1-Pad30)")
  (footprint "DMACK_FOOTPRINTS_primary:DOIT_ESP32_DevKit_v1_Breadboard_Adaptor" (layer "F.Cu")
    (tedit 63B886AA)
    (at 152.4 101.6)
    (property "Sheetfile" "DOIT_ESP32_Breadboard_Adaptor.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "DOIT ESP32 DevKit v1" (at 0 -22.86) (layer "F.SilkS"))
    (fp_text value "DOIT_ESP32_DevKit_v1" (at 0 0 90) (layer "F.Fab"))
    (fp_text user "GND" (at 11 15.24 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO25" (at -11 0 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO27" (at -11 5.08 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at -11 15.24 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO23" (at 11 -17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO18" (at 11 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO5" (at 11 0 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO13" (at -11 12.7 unlocked) (layer "F.SilkS"))
    (fp_text user "EN" (at -11 -17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO4" (at 11 7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO3" (at 11 -10.16 unlocked) (layer "F.SilkS"))
    (fp_text user "3V3" (at 11 17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO34" (at -11 -10.16 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO17" (at 11 2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO32" (at -11 -5.08 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO39" (at -11 -12.7 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO16" (at 11 5.08 unlocked) (layer "F.SilkS"))
    (fp_text user "USB" (at 0 22.86 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO22" (at 11 -15.24 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO35" (at -11 -7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO14" (at -11 7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO15" (at 11 12.7 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO19" (at 11 -5.08 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO21" (at 11 -7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO26" (at -11 2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO12" (at -11 10.16 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO36" (at -11 -15.24 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO2" (at 11 10.16 unlocked) (layer "F.SilkS"))
    (fp_text user "VIN" (at -11 17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO1" (at 11 -12.7 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO33" (at -11 -2.54 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -12.7 -17.78) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "unconnected-(U1-Pad1)") (pinfunction "EN") (pintype "unspecified"))
    (pad "1" thru_hole circle (at -3.81 -17.78 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 "unconnected-(U1-Pad1)") (pinfunction "EN") (pintype "unspecified"))
    (pad "1" thru_hole circle (at -3.81 -17.78) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "unconnected-(U1-Pad1)") (pinfunction "EN") (pintype "unspecified"))
    (pad "2" thru_hole circle (at -12.7 -15.24) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "unconnected-(U1-Pad2)") (pinfunction "GPIO36") (pintype "unspecified"))
    (pad "2" thru_hole circle (at -3.81 -15.24) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "unconnected-(U1-Pad2)") (pinfunction "GPIO36") (pintype "unspecified"))
    (pad "2" thru_hole circle (at -3.81 -15.24 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 "unconnected-(U1-Pad2)") (pinfunction "GPIO36") (pintype "unspecified"))
    (pad "3" thru_hole circle (at -3.81 -12.7) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 3 "unconnected-(U1-Pad3)") (pinfunction "GPIO39") (pintype "unspecified"))
    (pad "3" thru_hole circle (at -3.81 -12.7 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 "unconnected-(U1-Pad3)") (pinfunction "GPIO39") (pintype "unspecified"))
    (pad "3" thru_hole circle (at -12.7 -12.7) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 3 "unconnected-(U1-Pad3)") (pinfunction "GPIO39") (pintype "unspecified"))
    (pad "4" thru_hole circle (at -3.81 -10.16) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 4 "unconnected-(U1-Pad4)") (pinfunction "GPIO34") (pintype "unspecified"))
    (pad "4" thru_hole circle (at -12.7 -10.16) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 4 "unconnected-(U1-Pad4)") (pinfunction "GPIO34") (pintype "unspecified"))
    (pad "4" thru_hole circle (at -3.81 -10.16 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 "unconnected-(U1-Pad4)") (pinfunction "GPIO34") (pintype "unspecified"))
    (pad "5" thru_hole circle (at -3.81 -7.62) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 5 "unconnected-(U1-Pad5)") (pinfunction "GPIO35") (pintype "unspecified"))
    (pad "5" thru_hole circle (at -3.81 -7.62 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 "unconnected-(U1-Pad5)") (pinfunction "GPIO35") (pintype "unspecified"))
    (pad "5" thru_hole circle (at -12.7 -7.62) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 5 "unconnected-(U1-Pad5)") (pinfunction "GPIO35") (pintype "unspecified"))
    (pad "6" thru_hole circle (at -3.81 -5.08) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 6 "unconnected-(U1-Pad6)") (pinfunction "GPIO32") (pintype "unspecified"))
    (pad "6" thru_hole circle (at -12.7 -5.08) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 6 "unconnected-(U1-Pad6)") (pinfunction "GPIO32") (pintype "unspecified"))
    (pad "6" thru_hole circle (at -3.81 -5.08 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 "unconnected-(U1-Pad6)") (pinfunction "GPIO32") (pintype "unspecified"))
    (pad "7" thru_hole circle (at -3.81 -2.54) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 7 "unconnected-(U1-Pad7)") (pinfunction "GPIO33") (pintype "unspecified"))
    (pad "7" thru_hole circle (at -3.81 -2.54 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 "unconnected-(U1-Pad7)") (pinfunction "GPIO33") (pintype "unspecified"))
    (pad "7" thru_hole circle (at -12.7 -2.54) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 7 "unconnected-(U1-Pad7)") (pinfunction "GPIO33") (pintype "unspecified"))
    (pad "8" thru_hole circle (at -12.7 0) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 8 "unconnected-(U1-Pad8)") (pinfunction "GPIO25") (pintype "unspecified"))
    (pad "8" thru_hole circle (at -3.81 0) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 8 "unconnected-(U1-Pad8)") (pinfunction "GPIO25") (pintype "unspecified"))
    (pad "8" thru_hole circle (at -3.81 0 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 "unconnected-(U1-Pad8)") (pinfunction "GPIO25") (pintype "unspecified"))
    (pad "9" thru_hole circle (at -3.81 2.54) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 9 "unconnected-(U1-Pad9)") (pinfunction "GPIO26") (pintype "unspecified"))
    (pad "9" thru_hole circle (at -12.7 2.54) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 9 "unconnected-(U1-Pad9)") (pinfunction "GPIO26") (pintype "unspecified"))
    (pad "9" thru_hole circle (at -3.81 2.54 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 "unconnected-(U1-Pad9)") (pinfunction "GPIO26") (pintype "unspecified"))
    (pad "10" thru_hole circle (at -3.81 5.08 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 "unconnected-(U1-Pad10)") (pinfunction "GPIO27") (pintype "unspecified"))
    (pad "10" thru_hole circle (at -12.7 5.08) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 10 "unconnected-(U1-Pad10)") (pinfunction "GPIO27") (pintype "unspecified"))
    (pad "10" thru_hole circle (at -3.81 5.08) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 10 "unconnected-(U1-Pad10)") (pinfunction "GPIO27") (pintype "unspecified"))
    (pad "11" thru_hole circle (at -3.81 7.62 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 "unconnected-(U1-Pad11)") (pinfunction "GPIO14") (pintype "unspecified"))
    (pad "11" thru_hole circle (at -3.81 7.62) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 11 "unconnected-(U1-Pad11)") (pinfunction "GPIO14") (pintype "unspecified"))
    (pad "11" thru_hole circle (at -12.7 7.62) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 11 "unconnected-(U1-Pad11)") (pinfunction "GPIO14") (pintype "unspecified"))
    (pad "12" thru_hole circle (at -3.81 10.16) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 12 "unconnected-(U1-Pad12)") (pinfunction "GPIO12") (pintype "unspecified"))
    (pad "12" thru_hole circle (at -3.81 10.16 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 "unconnected-(U1-Pad12)") (pinfunction "GPIO12") (pintype "unspecified"))
    (pad "12" thru_hole circle (at -12.7 10.16) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 12 "unconnected-(U1-Pad12)") (pinfunction "GPIO12") (pintype "unspecified"))
    (pad "13" thru_hole circle (at -3.81 12.7 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "unconnected-(U1-Pad13)") (pinfunction "GPIO13") (pintype "unspecified"))
    (pad "13" thru_hole circle (at -3.81 12.7) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 13 "unconnected-(U1-Pad13)") (pinfunction "GPIO13") (pintype "unspecified"))
    (pad "13" thru_hole circle (at -12.7 12.7) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 13 "unconnected-(U1-Pad13)") (pinfunction "GPIO13") (pintype "unspecified"))
    (pad "14" thru_hole circle (at -3.81 15.24) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 14 "unconnected-(U1-Pad14)") (pinfunction "GND") (pintype "passive"))
    (pad "14" thru_hole circle (at -12.7 15.24) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 14 "unconnected-(U1-Pad14)") (pinfunction "GND") (pintype "passive"))
    (pad "14" thru_hole circle (at -3.81 15.24 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 "unconnected-(U1-Pad14)") (pinfunction "GND") (pintype "passive"))
    (pad "15" thru_hole circle (at -3.81 17.78 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 "unconnected-(U1-Pad15)") (pinfunction "VIN") (pintype "passive"))
    (pad "15" thru_hole circle (at -3.81 17.78) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 15 "unconnected-(U1-Pad15)") (pinfunction "VIN") (pintype "passive"))
    (pad "15" thru_hole circle (at -12.7 17.78) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 15 "unconnected-(U1-Pad15)") (pinfunction "VIN") (pintype "passive"))
    (pad "16" thru_hole circle (at 3.81 17.78 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 "unconnected-(U1-Pad16)") (pinfunction "3V3") (pintype "passive"))
    (pad "16" thru_hole circle (at 3.81 17.78) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 16 "unconnected-(U1-Pad16)") (pinfunction "3V3") (pintype "passive"))
    (pad "16" thru_hole circle (at 12.7 17.78) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 16 "unconnected-(U1-Pad16)") (pinfunction "3V3") (pintype "passive"))
    (pad "17" thru_hole circle (at 3.81 15.24) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 17 "unconnected-(U1-Pad17)") (pinfunction "GND") (pintype "passive"))
    (pad "17" thru_hole circle (at 12.7 15.24) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 17 "unconnected-(U1-Pad17)") (pinfunction "GND") (pintype "passive"))
    (pad "17" thru_hole circle (at 3.81 15.24 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 "unconnected-(U1-Pad17)") (pinfunction "GND") (pintype "passive"))
    (pad "18" thru_hole circle (at 12.7 12.7) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 18 "unconnected-(U1-Pad18)") (pinfunction "GPIO15") (pintype "unspecified"))
    (pad "18" thru_hole circle (at 3.81 12.7 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 "unconnected-(U1-Pad18)") (pinfunction "GPIO15") (pintype "unspecified"))
    (pad "18" thru_hole circle (at 3.81 12.7) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 18 "unconnected-(U1-Pad18)") (pinfunction "GPIO15") (pintype "unspecified"))
    (pad "19" thru_hole circle (at 3.81 10.16 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 "unconnected-(U1-Pad19)") (pinfunction "GPIO2") (pintype "unspecified"))
    (pad "19" thru_hole circle (at 3.81 10.16) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 19 "unconnected-(U1-Pad19)") (pinfunction "GPIO2") (pintype "unspecified"))
    (pad "19" thru_hole circle (at 12.7 10.16) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 19 "unconnected-(U1-Pad19)") (pinfunction "GPIO2") (pintype "unspecified"))
    (pad "20" thru_hole circle (at 3.81 7.62 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 "unconnected-(U1-Pad20)") (pinfunction "GPIO4") (pintype "unspecified"))
    (pad "20" thru_hole circle (at 3.81 7.62) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 20 "unconnected-(U1-Pad20)") (pinfunction "GPIO4") (pintype "unspecified"))
    (pad "20" thru_hole circle (at 12.7 7.62) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 20 "unconnected-(U1-Pad20)") (pinfunction "GPIO4") (pintype "unspecified"))
    (pad "21" thru_hole circle (at 3.81 5.08 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 21 "unconnected-(U1-Pad21)") (pinfunction "GPIO16") (pintype "unspecified"))
    (pad "21" thru_hole circle (at 3.81 5.08) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 21 "unconnected-(U1-Pad21)") (pinfunction "GPIO16") (pintype "unspecified"))
    (pad "21" thru_hole circle (at 12.7 5.08) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 21 "unconnected-(U1-Pad21)") (pinfunction "GPIO16") (pintype "unspecified"))
    (pad "22" thru_hole circle (at 3.81 2.54) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 22 "unconnected-(U1-Pad22)") (pinfunction "GPIO17") (pintype "unspecified"))
    (pad "22" thru_hole circle (at 12.7 2.54) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 22 "unconnected-(U1-Pad22)") (pinfunction "GPIO17") (pintype "unspecified"))
    (pad "22" thru_hole circle (at 3.81 2.54 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 "unconnected-(U1-Pad22)") (pinfunction "GPIO17") (pintype "unspecified"))
    (pad "23" thru_hole circle (at 3.81 0 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U1-Pad23)") (pinfunction "GPIO5") (pintype "unspecified"))
    (pad "23" thru_hole circle (at 3.81 0) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 23 "unconnected-(U1-Pad23)") (pinfunction "GPIO5") (pintype "unspecified"))
    (pad "23" thru_hole circle (at 12.7 0) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 23 "unconnected-(U1-Pad23)") (pinfunction "GPIO5") (pintype "unspecified"))
    (pad "24" thru_hole circle (at 3.81 -2.54) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 24 "unconnected-(U1-Pad24)") (pinfunction "GPIO18") (pintype "unspecified"))
    (pad "24" thru_hole circle (at 3.81 -2.54 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 24 "unconnected-(U1-Pad24)") (pinfunction "GPIO18") (pintype "unspecified"))
    (pad "24" thru_hole circle (at 12.7 -2.54) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 24 "unconnected-(U1-Pad24)") (pinfunction "GPIO18") (pintype "unspecified"))
    (pad "25" thru_hole circle (at 12.7 -5.08) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 25 "unconnected-(U1-Pad25)") (pinfunction "GPIO19") (pintype "unspecified"))
    (pad "25" thru_hole circle (at 3.81 -5.08) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 25 "unconnected-(U1-Pad25)") (pinfunction "GPIO19") (pintype "unspecified"))
    (pad "25" thru_hole circle (at 3.81 -5.08 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 25 "unconnected-(U1-Pad25)") (pinfunction "GPIO19") (pintype "unspecified"))
    (pad "26" thru_hole circle (at 3.81 -7.62) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 26 "unconnected-(U1-Pad26)") (pinfunction "GPIO21") (pintype "unspecified"))
    (pad "26" thru_hole circle (at 3.81 -7.62 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 26 "unconnected-(U1-Pad26)") (pinfunction "GPIO21") (pintype "unspecified"))
    (pad "26" thru_hole circle (at 12.7 -7.62) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 26 "unconnected-(U1-Pad26)") (pinfunction "GPIO21") (pintype "unspecified"))
    (pad "27" thru_hole circle (at 3.81 -10.16) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 27 "unconnected-(U1-Pad27)") (pinfunction "GPIO3") (pintype "unspecified"))
    (pad "27" thru_hole circle (at 3.81 -10.16 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 27 "unconnected-(U1-Pad27)") (pinfunction "GPIO3") (pintype "unspecified"))
    (pad "27" thru_hole circle (at 12.7 -10.16) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 27 "unconnected-(U1-Pad27)") (pinfunction "GPIO3") (pintype "unspecified"))
    (pad "28" thru_hole circle (at 12.7 -12.7) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 28 "unconnected-(U1-Pad28)") (pinfunction "GPIO1") (pintype "unspecified"))
    (pad "28" thru_hole circle (at 3.81 -12.7) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 28 "unconnected-(U1-Pad28)") (pinfunction "GPIO1") (pintype "unspecified"))
    (pad "28" thru_hole circle (at 3.81 -12.7 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 28 "unconnected-(U1-Pad28)") (pinfunction "GPIO1") (pintype "unspecified"))
    (pad "29" thru_hole circle (at 3.81 -15.24) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 29 "unconnected-(U1-Pad29)") (pinfunction "GPIO22") (pintype "unspecified"))
    (pad "29" thru_hole circle (at 3.81 -15.24 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 "unconnected-(U1-Pad29)") (pinfunction "GPIO22") (pintype "unspecified"))
    (pad "29" thru_hole circle (at 12.7 -15.24) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 29 "unconnected-(U1-Pad29)") (pinfunction "GPIO22") (pintype "unspecified"))
    (pad "30" thru_hole circle (at 3.81 -17.78 270) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 "unconnected-(U1-Pad30)") (pinfunction "GPIO23") (pintype "unspecified"))
    (pad "30" thru_hole circle (at 3.81 -17.78) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 30 "unconnected-(U1-Pad30)") (pinfunction "GPIO23") (pintype "unspecified"))
    (pad "30" thru_hole circle (at 12.7 -17.78) (size 1.9 1.9) (drill 1.02) (layers *.Cu *.Mask "F.SilkS")
      (net 30 "unconnected-(U1-Pad30)") (pinfunction "GPIO23") (pintype "unspecified"))
  )
  (gr_line (start 138.43 127) (end 138.43 76.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 166.37 76.2) (end 166.37 127) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 166.37 127) (end 138.43 127) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.43 76.2) (end 166.37 76.2) (layer "Edge.Cuts") (width 0.1))
  (gr_text "DMack, January 6, 2023" (at 152.4 101.6 90) (layer "B.SilkS"))
  (gr_text "Breadboard Adaptor" (at 152.4 80.5) (layer "F.SilkS"))
)
