(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 24)
    (no_connects 0)
    (area 25.299999 25.299999 91.540001 67.410001)
    (thickness 1.6)
    (drawings 20)
    (tracks 60)
    (zones 0)
    (modules 18)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.54 2.54)
    (pad_drill 2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 /RESET)
  (net 2 "Net-(J1-Pad2)")
  (net 3 /SWCLK)
  (net 4 /SWDIO)
  (net 5 VCC)
  (net 6 /RXD)
  (net 7 "Net-(J2-Pad2)")
  (net 8 "Net-(J2-Pad3)")
  (net 9 /TXD)
  (net 10 "Net-(J3-Pad1)")
  (net 11 GND)
  (net 12 "Net-(J3-Pad3)")
  (net 13 "Net-(J4-Pad1)")
  (net 14 "Net-(J4-Pad2)")
  (net 15 "Net-(J4-Pad3)")
  (net 16 "Net-(J5-Pad1)")
  (net 17 "Net-(J5-Pad2)")
  (net 18 "Net-(J5-Pad3)")
  (net 19 "Net-(J6-Pad2)")
  (net 20 "Net-(J8-Pad1)")
  (net 21 "Net-(J9-Pad2)")
  (net 22 "Net-(J10-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /RESET)
    (add_net /RXD)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /TXD)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J10-Pad6)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad2)")
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 33.02 58.42 180)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value SERSEL (at 1.27 4.87 180) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /RXD))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /TXD))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A092FFA)
    (at 83.82 38.1 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 2.54 2.54 360) (layer F.SilkS))
    (fp_text value GND (at -2.54 2.54 360) (layer F.Fab))
    (fp_text user %R (at 0 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A092FFE)
    (at 71.12 38.1 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 2.54 2.54 360) (layer F.SilkS))
    (fp_text value Marker (at -2.54 2.54 360) (layer F.Fab))
    (fp_text user %R (at 0 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A093002)
    (at 62.23 38.1 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 2.54 2.54 360) (layer F.SilkS))
    (fp_text value Marker (at -2.54 2.54 360) (layer F.Fab))
    (fp_text user %R (at 0 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A09301A)
    (at 34.29 38.1 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Serial (at -2.54 2.54 360) (layer F.Fab))
    (fp_text user %R (at 0 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A0931C3)
    (at 40.894 58.8518 45)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 45) (layer F.SilkS))
    (fp_text value SHOE_SWD (at 2.370788 2.658156 135) (layer F.Fab))
    (fp_text user %R (at 3.681905 1.885854 135) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 45) (size 1.7 1.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole oval (at 0 2.54 45) (size 1.7 1.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /SWCLK))
    (pad 3 thru_hole oval (at 0 5.079999 45) (size 1.7 1.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /SWDIO))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A09300B)
    (at 65.6336 47.9552)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J8 (at -2.3622 -0.1016 90) (layer F.SilkS))
    (fp_text value SHOE_P0.20 (at 6.7564 0.3048 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 20 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch1.27mm (layer B.Cu) (tedit 5A09EDA2)
    (at 53.34 62.23 90)
    (descr "Through hole straight pin header, 2x03, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 1.27mm double row")
    (fp_text reference J9 (at 0.8382 2.54 90) (layer B.SilkS))
    (fp_text value SHOE_SERIAL (at 3.81 -1.27 360) (layer B.Fab))
    (fp_text user %R (at 5.08 -0.635 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 21 "Net-(J9-Pad2)"))
    (pad 3 thru_hole oval (at 0 -1.27 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 /RXD))
    (pad 4 thru_hole oval (at 1.27 -1.27 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 /TXD))
    (pad 5 thru_hole oval (at 0 -2.54 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 6 thru_hole oval (at 1.27 -2.54 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 /RESET))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch1.27mm (layer B.Cu) (tedit 5A08F720)
    (at 39.37 34.29)
    (descr "Through hole straight pin header, 2x03, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 1.27mm double row")
    (fp_text reference J10 (at 0.9398 2.5146) (layer B.SilkS))
    (fp_text value AREA_SWD (at -2.3114 -0.381 270) (layer B.Fab))
    (fp_text user %R (at 3.429 -1.5494 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 1.27 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /SWDIO))
    (pad 3 thru_hole oval (at 0 -1.27) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 /RESET))
    (pad 4 thru_hole oval (at 1.27 -1.27) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /SWCLK))
    (pad 5 thru_hole oval (at 0 -2.54) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 6 thru_hole oval (at 1.27 -2.54) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "Net-(J10-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A092FEB)
    (at 73.66 27.94 90)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J1 (at -2.54 2.54 180) (layer F.SilkS))
    (fp_text value SWD (at -2.54 5.08 180) (layer F.Fab))
    (fp_text user %R (at -2.54 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /RESET))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /SWCLK))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SWDIO))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 35.2298 32.4104 180)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Nailbed_Mount (at 0 2.33 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.54 2.54) (drill 2) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 35.2298 47.498)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J12 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Nailbed_Mount (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 2) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A095892)
    (at 84.7344 32.4104 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J13 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Nailbed_Mount (at -3.0226 2.032 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 2) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A0957AE)
    (at 69.85 53.848)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J14 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Shoe_Mount (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 2) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 50.8 41.275)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J15 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Extra_Via (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 31.115 42.545)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J16 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Extra_Via (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 52.07 30.48)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J17 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Extra_Via (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 59.055 47.625)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J18 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Extra_Via (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 25.4 67.31) (end 25.4 25.4) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 91.44 67.31) (end 25.4 67.31) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 91.44 25.4) (end 91.44 67.31) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 25.4 25.4) (end 91.44 25.4) (angle 90) (layer Edge.Cuts) (width 0.2))
  (zone (net 11) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.9 66.04) (xy 26.67 66.04) (xy 26.67 26.67) (xy 88.9 26.67)
      )
    )
  )
  (zone (net 11) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.9 66.04) (xy 26.67 66.04) (xy 26.67 26.67) (xy 88.9 26.67)
      )
    )
  )
)
