<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="73" y2="0" width="0.1" layer="20"/>
<wire x1="73" y1="0" x2="73" y2="17" width="0.1" layer="20"/>
<wire x1="73" y1="17" x2="71.5" y2="17" width="0.1" layer="20"/>
<wire x1="71.5" y1="17" x2="71.5" y2="32" width="0.1" layer="20"/>
<wire x1="71.5" y1="32" x2="73" y2="32" width="0.1" layer="20"/>
<wire x1="73" y1="32" x2="73" y2="39" width="0.1" layer="20"/>
<wire x1="73" y1="39" x2="0" y2="39" width="0.1" layer="20"/>
<wire x1="0" y1="39" x2="0" y2="32" width="0.1" layer="20"/>
<wire x1="0" y1="32" x2="1.5" y2="32" width="0.1" layer="20"/>
<wire x1="1.5" y1="32" x2="1.5" y2="17" width="0.1" layer="20"/>
<wire x1="1.5" y1="17" x2="0" y2="17" width="0.1" layer="20"/>
<wire x1="0" y1="17" x2="0" y2="0" width="0.1" layer="20"/>
<text>D:/DECODE/Cadsoft EAGLE/projects/RF Projects/EME103B/EME103B_TG.bmp</text>
<text>EME103B2 L/S-BAND LNA
TAG67 FEB 2018</text>
<hole x="42.65" y="31.9" drill="2.2"/>
<text>1000MHz H.P.F.
CUT TO DISCONNECT</text>
</plain>
<libraries>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
</elements>
<signals>
<signal name="S2">
</signal>
<signal name="RF2">
</signal>
<signal name="RF3">
</signal>
<signal name="RFOUT">
</signal>
<signal name="S13">
</signal>
<signal name="S14">
</signal>
<signal name="S7B">
</signal>
<signal name="S11">
</signal>
<signal name="S15">
</signal>
<signal name="GND">
</signal>
<signal name="S4B">
</signal>
<signal name="RF1">
</signal>
<signal name="S$1">
</signal>
<signal name="S56">
</signal>
<signal name="S57">
</signal>
<signal name="S4C">
</signal>
</signals>
</board>
</drawing>
</eagle>
