(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(A1-Pad1)")
  (net 2 "unconnected-(A1-Pad2)")
  (net 3 "unconnected-(A1-Pad3)")
  (net 4 "unconnected-(A1-Pad4)")
  (net 5 "/EYE_PT1")
  (net 6 "unconnected-(A1-Pad15)")
  (net 7 "unconnected-(A1-Pad16)")
  (net 8 "unconnected-(A1-Pad21)")
  (net 9 "unconnected-(A1-Pad23)")
  (net 10 "unconnected-(A1-Pad28)")
  (net 11 "unconnected-(A1-Pad30)")
  (net 12 "unconnected-(A1-Pad31)")
  (net 13 "unconnected-(A1-Pad32)")
  (net 14 "+5V")
  (net 15 "GND")
  (net 16 "/EYE_PT2")
  (net 17 "+12V")
  (net 18 "unconnected-(A1-Pad11)")
  (net 19 "/DATAIN")
  (net 20 "unconnected-(A1-Pad18)")
  (net 21 "unconnected-(A1-Pad24)")
  (net 22 "unconnected-(A1-Pad25)")
  (net 23 "unconnected-(J1-Pad9)")
  (net 24 "Net-(A1-Pad12)")
  (net 25 "/SDA")
  (net 26 "/SCL")
  (net 27 "Net-(A1-Pad19)")
  (net 28 "unconnected-(A1-Pad26)")
  (net 29 "unconnected-(A1-Pad27)")
  (net 30 "unconnected-(A1-Pad20)")
  (net 31 "Net-(A1-Pad22)")
  (net 32 "Net-(D7-Pad1)")
  (net 33 "Net-(D4-Pad1)")
  (net 34 "/5VFUSED")
  (net 35 "unconnected-(J3-Pad4)")
  (net 36 "unconnected-(J6-Pad2)")
  (footprint "footprints:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 186.615 95.75)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "PT1" (at -3.735 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(A1-Pad19)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 186.69 88.265)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 0 1.27) (layer "F.Fab"))
    (fp_text value "1K" (at 2.54 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(D4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 186.69 90.805)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 1.27) (layer "F.Fab"))
    (fp_text value "1K" (at 2.54 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 186.436 118.0065 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 0 0 90) (layer "F.Fab"))
    (fp_text value "4K7" (at 3.1925 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/5VFUSED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_PicoBlade_53047-0610_1x06_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 5B783167)
    (at 172.508972 105.86)
    (descr "Molex PicoBlade Connector System, 53047-0610, 6 Pins per row (http://www.molex.com/pdm_docs/sd/530470610_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade side entry")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 3.12 -3.25) (layer "F.Fab"))
    (fp_text value "40826 CHARGER" (at 5.486707 3.384262) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.12 -1.35) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 15 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.25 0) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.5 0) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 "/SDA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 3.75 0) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 26 "/SCL") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 5 0) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 "/5VFUSED") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 6.25 0) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 "/5VFUSED") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KIPRJMOD}/3D/530470610.stp"
      (offset (xyz 3 -1.5 5.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 186.69 83.185 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "4K7" (at -2.8975 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/5VFUSED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/EYE_PT2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Harwin_Gecko-G125-FVX1605L0X_2x08_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 5A16AFEB)
    (at 172.72 83.22)
    (descr "Harwin Gecko Connector, 16 pins, dual row female, vertical entry, PN:G125-FVX1605L0X")
    (tags "connector harwin gecko")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 12.7 0.635) (layer "F.Fab"))
    (fp_text value "40672 EYE" (at 2.602668 5.218298) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.375 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 34 "/5VFUSED") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 34 "/5VFUSED") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 34 "/5VFUSED") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.75 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 34 "/5VFUSED") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 34 "/5VFUSED") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 19 "/DATAIN") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 7.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 8.75 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J1-Pad9)") (pinfunction "Pin_9") (pintype "passive+no_connect"))
    (pad "10" thru_hole circle (at 1.25 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 2.5 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 3.75 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 5 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 5 "/EYE_PT1") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 6.25 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at 7.5 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 16 "/EYE_PT2") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at 8.75 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-FVX1605L0X_2x08_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D/g125-fv11605l0p.stp"
      (offset (xyz 4.5 -0.5 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 186.69 85.598 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "4K7" (at -2.8975 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/5VFUSED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/EYE_PT1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 188.976 118.11 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 0 0 90) (layer "F.Fab"))
    (fp_text value "4K7" (at 3.1925 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/5VFUSED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 5A16AFEB)
    (at 172.74 93.99)
    (descr "Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X")
    (tags "connector harwin gecko")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.25 4.3) (layer "F.Fab"))
    (fp_text value "40675 STRIP" (at 3.536 5.07) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 19 "/DATAIN") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 0 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 34 "/5VFUSED") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 1.25 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 5 "/EYE_PT1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.5 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KIPRJMOD}/3D/G125-FV10605L0_asm.stp"
      (offset (xyz 1.25 -0.75 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 182.88 118.04 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.65 90) (layer "F.Fab"))
    (fp_text value "1A" (at -2.89 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 34 "/5VFUSED") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 14 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SAMTEC_UMPS-04-03.5-G-V-S-W-FR" (layer "F.Cu")
    (tedit 68964D2D)
    (at 205.105 85.344)
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at -2.8575 -4.1275) (layer "F.SilkS") hide)
    (fp_text value "AG102384-001 EYES" (at -1.905 5.08) (layer "F.SilkS"))
    (pad "1" smd rect (at -3 0) (size 1.3 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/5VFUSED") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -1 0) (size 1.3 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "GND") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" smd rect (at 1 0) (size 1.3 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/DATAIN") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 3 0) (size 1.3 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "S1" thru_hole circle (at -5 -1.5) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (solder_mask_margin 0.102))
    (pad "S2" thru_hole circle (at 5 -1) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (solder_mask_margin 0.102))
    (pad "S3" thru_hole circle (at -5 0.5) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (solder_mask_margin 0.102))
    (pad "S4" thru_hole circle (at 5 1) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (solder_mask_margin 0.102))
  )
  (footprint "footprints:SW_PUSH_6mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 207.01 119.765 90)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 3.25 -2 90) (layer "F.Fab"))
    (fp_text value "INPUT" (at -2.54 1.905 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad12)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad12)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 186.69 93.345)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D7" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "PT2" (at -3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D7-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(A1-Pad22)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Logo" (layer "F.Cu")
    (tedit 0)
    (at 200.152 102.616)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Connector_Molex:Molex_CLIK-Mate_502382-0470_1x04-1MP_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD89)
    (at 175.26 117.094)
    (descr "Molex CLIK-Mate series connector, 502382-0470 (http://www.molex.com/pdm_docs/sd/5023820270_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex CLIK-Mate side entry")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J6" (at 0 -0.762) (layer "F.SilkS") hide)
    (fp_text value "AG104368-001 TORSO" (at 5.588 4.318) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.77) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.875 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -0.625 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "unconnected-(J6-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" smd roundrect (at 0.625 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/DATAIN") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.875 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/5VFUSED") (pinfunction "Pin_4") (pintype "passive"))
    (pad "MP" smd roundrect (at -3.725 -1.4) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "MP" smd roundrect (at 3.725 -1.4) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_CLIK-Mate_502382-0470_1x04-1MP_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Arduino_UNO_R3" locked (layer "B.Cu")
    (tedit 58AB60FC)
    (at 177.165 125.73)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (property "Sheetfile" "LED_Shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "A1" (at -9.525 0.635 180) (layer "F.Fab"))
    (fp_text value "Arduino_UNO_R3" (at 0 -22.86 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -20.32 180) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "unconnected-(A1-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" thru_hole oval locked (at 2.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "unconnected-(A1-Pad2)") (pinfunction "IOREF") (pintype "output"))
    (pad "3" thru_hole oval locked (at 5.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(A1-Pad3)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "4" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(A1-Pad4)") (pinfunction "3V3") (pintype "power_out"))
    (pad "5" thru_hole oval locked (at 10.16 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "+5V") (pintype "power_out"))
    (pad "6" thru_hole oval locked (at 12.7 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole oval locked (at 15.24 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval locked (at 17.78 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "+12V") (pinfunction "VIN") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 22.86 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/EYE_PT1") (pinfunction "A0") (pintype "bidirectional"))
    (pad "10" thru_hole oval locked (at 25.4 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/EYE_PT2") (pinfunction "A1") (pintype "bidirectional"))
    (pad "11" thru_hole oval locked (at 27.94 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(A1-Pad11)") (pinfunction "A2") (pintype "bidirectional"))
    (pad "12" thru_hole oval locked (at 30.48 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad12)") (pinfunction "A3") (pintype "bidirectional"))
    (pad "13" thru_hole oval locked (at 33.02 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/SDA") (pinfunction "SDA/A4") (pintype "bidirectional"))
    (pad "14" thru_hole oval locked (at 35.56 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/SCL") (pinfunction "SCL/A5") (pintype "bidirectional"))
    (pad "15" thru_hole oval locked (at 35.56 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "unconnected-(A1-Pad15)") (pinfunction "D0/RX") (pintype "bidirectional"))
    (pad "16" thru_hole oval locked (at 33.02 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "unconnected-(A1-Pad16)") (pinfunction "D1/TX") (pintype "bidirectional"))
    (pad "17" thru_hole oval locked (at 30.48 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/DATAIN") (pinfunction "D2") (pintype "bidirectional"))
    (pad "18" thru_hole oval locked (at 27.94 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "unconnected-(A1-Pad18)") (pinfunction "D3") (pintype "bidirectional"))
    (pad "19" thru_hole oval locked (at 25.4 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad19)") (pinfunction "D4") (pintype "bidirectional"))
    (pad "20" thru_hole oval locked (at 22.86 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 30 "unconnected-(A1-Pad20)") (pinfunction "D5") (pintype "bidirectional"))
    (pad "21" thru_hole oval locked (at 20.32 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "unconnected-(A1-Pad21)") (pinfunction "D6") (pintype "bidirectional"))
    (pad "22" thru_hole oval locked (at 17.78 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(A1-Pad22)") (pinfunction "D7") (pintype "bidirectional"))
    (pad "23" thru_hole oval locked (at 13.72 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "unconnected-(A1-Pad23)") (pinfunction "D8") (pintype "bidirectional"))
    (pad "24" thru_hole oval locked (at 11.18 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(A1-Pad24)") (pinfunction "D9") (pintype "bidirectional"))
    (pad "25" thru_hole oval locked (at 8.64 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "unconnected-(A1-Pad25)") (pinfunction "D10") (pintype "bidirectional"))
    (pad "26" thru_hole oval locked (at 6.1 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 28 "unconnected-(A1-Pad26)") (pinfunction "D11") (pintype "bidirectional"))
    (pad "27" thru_hole oval locked (at 3.56 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 29 "unconnected-(A1-Pad27)") (pinfunction "D12") (pintype "bidirectional"))
    (pad "28" thru_hole oval locked (at 1.02 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(A1-Pad28)") (pinfunction "D13") (pintype "bidirectional"))
    (pad "29" thru_hole oval locked (at -1.52 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole oval locked (at -4.06 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(A1-Pad30)") (pinfunction "AREF") (pintype "input"))
    (pad "31" thru_hole oval locked (at -6.6 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(A1-Pad31)") (pinfunction "SDA/A4") (pintype "bidirectional"))
    (pad "32" thru_hole oval locked (at -9.14 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(A1-Pad32)") (pinfunction "SCL/A5") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/Arduino_UNO_R3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 167.64 128.27) (mid 165.843949 127.526051) (end 165.1 125.73) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 215.9 125.73) (mid 215.156051 127.526051) (end 213.36 128.27) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 215.9 77.47) (end 215.9 87.63) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 165.1 77.47) (end 165.1 125.73) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 215.9 87.63) (end 218.44 90.17) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 218.44 90.17) (end 218.44 123.19) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 167.64 74.93) (end 213.36 74.93) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 213.36 74.93) (mid 215.156051 75.673949) (end 215.9 77.47) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 213.36 128.27) (end 212.09 128.27) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 167.64 128.27) (end 212.09 128.27) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 165.1 77.47) (mid 165.843949 75.673949) (end 167.64 74.93) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 218.44 123.19) (end 215.9 125.73) (layer "Edge.Cuts") (width 0.1))
  (gr_text "D2 DATAIN\nD4 PT1 LED\nD7 PT2 LED\nA0 PT1\nA1 PT2\nA3 INPUT\n\n0X32 LP55231 A\n0X33 LP55231 B\n0X34 LP55231 C" (at 210.058 99.568) (layer "B.SilkS"))
  (gr_text "Rev 0.2  Sep 25" (at 181.61 122.555) (layer "B.SilkS"))
  (gr_text "5V\nGND\nGND\n12V" (at 191.135 123.19 90) (layer "B.SilkS"))
  (gr_text "(Use 40795 Harness)" (at 178.308 110.998) (layer "F.SilkS"))
  (gr_text "AG102387-001 STRIP" (at 202.946 92.71) (layer "F.SilkS"))
  (gr_text "(Use AG103304 Harness)" (at 179.578 123.19) (layer "F.SilkS"))
  (dimension (type aligned) (layer "User.1")
    (pts (xy 188.214 104.648) (xy 213.106 104.648))
    (height 5.587999)
    (gr_text "24.8920 mm" (at 200.66 109.085999) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 15) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 220.98 132.08)
        (xy 162.56 132.08)
        (xy 162.56 73.66)
        (xy 220.98 73.66)
      )
    )
  )
  (zone (net 15) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.52 134.62)
        (xy 160.02 134.62)
        (xy 160.02 71.12)
        (xy 223.52 71.12)
      )
    )
  )
)
