(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 73)
    (zones 0)
    (modules 21)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(J1-Pad16)")
  (net 4 "Net-(J1-Pad14)")
  (net 5 "Net-(J1-Pad12)")
  (net 6 "Net-(J1-Pad10)")
  (net 7 "Net-(J1-Pad8)")
  (net 8 "Net-(J1-Pad6)")
  (net 9 "Net-(J1-Pad4)")
  (net 10 "Net-(J1-Pad2)")
  (net 11 "Net-(SW1-Pad2)")
  (net 12 "Net-(SW8-Pad2)")
  (net 13 "Net-(SW7-Pad2)")
  (net 14 "Net-(SW6-Pad2)")
  (net 15 "Net-(SW5-Pad2)")
  (net 16 "Net-(SW4-Pad2)")
  (net 17 "Net-(SW3-Pad2)")
  (net 18 "Net-(SW2-Pad2)")
  (net 19 +VDC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +VDC)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(SW3-Pad2)")
    (add_net "Net-(SW4-Pad2)")
    (add_net "Net-(SW5-Pad2)")
    (add_net "Net-(SW6-Pad2)")
    (add_net "Net-(SW7-Pad2)")
    (add_net "Net-(SW8-Pad2)")
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H5mm (layer F.Cu) (tedit 5A02FE31)
    (at 114.3 79.756 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 -2 90) (layer F.SilkS))
    (fp_text value SW_Push_SPDT (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(SW1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H5mm (layer F.Cu) (tedit 5A02FE31)
    (at 105.664 79.756 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW2 (at 3.25 -2 90) (layer F.SilkS))
    (fp_text value SW_Push_SPDT (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(SW2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(SW2-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H5mm (layer F.Cu) (tedit 5A02FE31)
    (at 97.028 79.756 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW3 (at 3.25 -2 90) (layer F.SilkS))
    (fp_text value SW_Push_SPDT (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(SW3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(SW3-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H5mm (layer F.Cu) (tedit 5A02FE31)
    (at 88.392 79.756 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW4 (at 3.25 -2 90) (layer F.SilkS))
    (fp_text value SW_Push_SPDT (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(SW4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(SW4-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H5mm (layer F.Cu) (tedit 5A02FE31)
    (at 79.756 79.756 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW5 (at 3.25 -2 90) (layer F.SilkS))
    (fp_text value SW_Push_SPDT (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(SW5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(SW5-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H5mm (layer F.Cu) (tedit 5A02FE31)
    (at 71.12 79.756 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW6 (at 3.25 -2 90) (layer F.SilkS))
    (fp_text value SW_Push_SPDT (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(SW6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(SW6-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H5mm (layer F.Cu) (tedit 5A02FE31)
    (at 62.484 79.756 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW7 (at 3.25 -2 90) (layer F.SilkS))
    (fp_text value SW_Push_SPDT (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(SW7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(SW7-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H5mm (layer F.Cu) (tedit 5A02FE31)
    (at 53.848 79.756 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW8 (at 3.25 -2 90) (layer F.SilkS))
    (fp_text value SW_Push_SPDT (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(SW8-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(SW8-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_BarrelJack:BarrelJack_Horizontal (layer F.Cu) (tedit 5A1DBF6A)
    (at 108.204 57.912 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J2 (at -8.45 5.75 270) (layer F.SilkS))
    (fp_text value Barrel_Jack (at -6.2 -5.5 270) (layer F.Fab))
    (fp_text user %R (at -3 -2.95 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 19 +VDC))
    (pad 2 thru_hole roundrect (at -6 0 270) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 thru_hole roundrect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 59DE0341)
    (at 85.344 47.244 270)
    (descr "Through hole straight IDC box header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x08 2.54mm double row")
    (fp_text reference J1 (at 1.27 -6.604 270) (layer F.SilkS))
    (fp_text value "IDC 16 pin" (at 1.27 24.384 270) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad16)"))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 85.344 59.436 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference U1 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value NSI50010YT1G (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(SW1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 82.804 59.436 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference U2 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value NSI50010YT1G (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(SW2-Pad2)"))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 80.264 59.436 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference U3 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value NSI50010YT1G (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(SW3-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 77.724 59.436 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference U4 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value NSI50010YT1G (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(SW4-Pad2)"))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 75.184 59.436 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference U5 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value NSI50010YT1G (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(SW5-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 72.644 59.436 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference U6 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value NSI50010YT1G (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(SW6-Pad2)"))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad12)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 70.104 59.436 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference U7 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value NSI50010YT1G (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad14)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(SW7-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 67.564 59.436 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference U8 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value "NSI50010YT1G x 8" (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(SW8-Pad2)"))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad16)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 87.884 59.436 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference U9 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value NSI50010YT1G (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 +VDC))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 96.012 58.928 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at -3.556 0 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo_7.5x8mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 57.912 59.944)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_7.5x8mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (gr_text larsskj-005-01 (at 117.856 54.864 90) (layer F.SilkS))
  (gr_text 1 (at 116.332 69.088) (layer F.SilkS))
  (gr_text 2 (at 108.204 69.088) (layer F.SilkS))
  (gr_text 3 (at 99.06 69.088) (layer F.SilkS))
  (gr_text 4 (at 90.932 69.088) (layer F.SilkS))
  (gr_text 5 (at 81.788 69.088) (layer F.SilkS))
  (gr_text 6 (at 73.66 69.088) (layer F.SilkS))
  (gr_text 7 (at 65.024 69.088) (layer F.SilkS))
  (gr_text 8 (at 56.388 69.088) (layer F.SilkS))
  (gr_line (start 50.292 42.164) (end 50.292 83.312) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.428 42.164) (end 50.292 42.164) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.428 83.312) (end 122.428 42.164) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.292 83.312) (end 122.428 83.312) (layer Edge.Cuts) (width 0.15))
  (zone (net 19) (net_name +VDC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.292 42.164) (xy 122.428 42.164) (xy 122.428 83.312) (xy 50.292 83.312)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.292 42.164) (xy 122.428 42.164) (xy 122.428 83.312) (xy 50.292 83.312)
      )
    )
  )
)
