(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 1133)
    (zones 0)
    (modules 64)
    (nets 163)
  )
  (page USLetter portrait)
  (title_block
    (title "TTL Clock")
    (date 2020-12-03)
    (rev 1.1)
    (company "Sergey Kiselev")
    (comment 1 "License: GPLv3")
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.3556)
    (user_trace_width 1.1176)
    (trace_clearance 0.254)
    (zone_clearance 0.3556)
    (zone_45_only no)
    (trace_min 0.254)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.254)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.778 1.778)
    (pad_drill 1.27)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 /1Hz)
  (net 2 /2Hz)
  (net 3 /HOURS)
  (net 4 /HOURS_OUT)
  (net 5 /MINUTES)
  (net 6 /MINUTES_OUT)
  (net 7 /SECONDS_RESET)
  (net 8 GND)
  (net 9 VCC)
  (net 10 "Net-(C18-Pad1)")
  (net 11 "Net-(C19-Pad1)")
  (net 12 "Net-(R1-Pad1)")
  (net 13 "Net-(R2-Pad1)")
  (net 14 "Net-(R3-Pad1)")
  (net 15 "Net-(R4-Pad1)")
  (net 16 "Net-(R5-Pad1)")
  (net 17 "Net-(R6-Pad1)")
  (net 18 "Net-(RP1-Pad1)")
  (net 19 "Net-(RP1-Pad2)")
  (net 20 "Net-(RP1-Pad3)")
  (net 21 "Net-(RP1-Pad4)")
  (net 22 "Net-(RP1-Pad5)")
  (net 23 "Net-(RP1-Pad6)")
  (net 24 "Net-(RP1-Pad7)")
  (net 25 "Net-(RP2-Pad1)")
  (net 26 "Net-(RP2-Pad2)")
  (net 27 "Net-(RP2-Pad3)")
  (net 28 "Net-(RP2-Pad4)")
  (net 29 "Net-(RP2-Pad5)")
  (net 30 "Net-(RP2-Pad6)")
  (net 31 "Net-(RP2-Pad7)")
  (net 32 "Net-(RP3-Pad1)")
  (net 33 "Net-(RP3-Pad2)")
  (net 34 "Net-(RP3-Pad3)")
  (net 35 "Net-(RP3-Pad4)")
  (net 36 "Net-(RP3-Pad5)")
  (net 37 "Net-(RP3-Pad6)")
  (net 38 "Net-(RP3-Pad7)")
  (net 39 "Net-(RP4-Pad1)")
  (net 40 "Net-(RP4-Pad2)")
  (net 41 "Net-(RP4-Pad3)")
  (net 42 "Net-(RP4-Pad4)")
  (net 43 "Net-(RP4-Pad5)")
  (net 44 "Net-(RP4-Pad6)")
  (net 45 "Net-(RP4-Pad7)")
  (net 46 "Net-(RP5-Pad1)")
  (net 47 "Net-(RP5-Pad2)")
  (net 48 "Net-(RP5-Pad3)")
  (net 49 "Net-(RP5-Pad4)")
  (net 50 "Net-(RP5-Pad5)")
  (net 51 "Net-(RP5-Pad6)")
  (net 52 "Net-(RP5-Pad7)")
  (net 53 "Net-(RP6-Pad1)")
  (net 54 "Net-(RP6-Pad2)")
  (net 55 "Net-(RP6-Pad3)")
  (net 56 "Net-(RP6-Pad4)")
  (net 57 "Net-(RP6-Pad5)")
  (net 58 "Net-(RP6-Pad6)")
  (net 59 "Net-(RP6-Pad7)")
  (net 60 "Net-(U1-Pad1)")
  (net 61 "Net-(U1-Pad2)")
  (net 62 "Net-(U1-Pad4)")
  (net 63 "Net-(U1-Pad5)")
  (net 64 "Net-(U1-Pad6)")
  (net 65 "Net-(U1-Pad7)")
  (net 66 "Net-(U1-Pad9)")
  (net 67 "Net-(U1-Pad13)")
  (net 68 "Net-(U1-Pad14)")
  (net 69 "Net-(U1-Pad15)")
  (net 70 "Net-(U2-Pad2)")
  (net 71 "Net-(U2-Pad12)")
  (net 72 "Net-(U2-Pad8)")
  (net 73 "Net-(U2-Pad11)")
  (net 74 "Net-(U3-Pad2)")
  (net 75 "Net-(U3-Pad12)")
  (net 76 "Net-(U3-Pad8)")
  (net 77 "Net-(U3-Pad11)")
  (net 78 "Net-(U12-Pad9)")
  (net 79 "Net-(U4-Pad3)")
  (net 80 "Net-(U11-Pad9)")
  (net 81 "Net-(U11-Pad8)")
  (net 82 "Net-(U5-Pad4)")
  (net 83 "Net-(U11-Pad11)")
  (net 84 "Net-(U11-Pad1)")
  (net 85 "Net-(U6-Pad4)")
  (net 86 "Net-(U12-Pad11)")
  (net 87 "Net-(U12-Pad1)")
  (net 88 "Net-(U13-Pad9)")
  (net 89 "Net-(U13-Pad8)")
  (net 90 "Net-(U7-Pad4)")
  (net 91 "Net-(U13-Pad11)")
  (net 92 "Net-(U13-Pad1)")
  (net 93 "Net-(U14-Pad3)")
  (net 94 "Net-(U8-Pad4)")
  (net 95 "Net-(U14-Pad11)")
  (net 96 "Net-(U14-Pad1)")
  (net 97 "Net-(U15-Pad9)")
  (net 98 "Net-(U15-Pad2)")
  (net 99 "Net-(U9-Pad4)")
  (net 100 "Net-(U15-Pad11)")
  (net 101 "Net-(U15-Pad1)")
  (net 102 "Net-(U10-Pad1)")
  (net 103 "Net-(U10-Pad2)")
  (net 104 "Net-(U10-Pad4)")
  (net 105 "Net-(U10-Pad7)")
  (net 106 "Net-(D1-Pad1)")
  (net 107 "Net-(D2-Pad1)")
  (net 108 "Net-(D3-Pad1)")
  (net 109 "Net-(D4-Pad1)")
  (net 110 "Net-(RP1-Pad8)")
  (net 111 "Net-(RP1-Pad9)")
  (net 112 "Net-(RP1-Pad10)")
  (net 113 "Net-(RP1-Pad11)")
  (net 114 "Net-(RP1-Pad12)")
  (net 115 "Net-(RP1-Pad13)")
  (net 116 "Net-(RP1-Pad14)")
  (net 117 "Net-(RP2-Pad14)")
  (net 118 "Net-(RP2-Pad13)")
  (net 119 "Net-(RP2-Pad12)")
  (net 120 "Net-(RP2-Pad11)")
  (net 121 "Net-(RP2-Pad10)")
  (net 122 "Net-(RP3-Pad14)")
  (net 123 "Net-(RP3-Pad13)")
  (net 124 "Net-(RP3-Pad12)")
  (net 125 "Net-(RP3-Pad11)")
  (net 126 "Net-(RP3-Pad10)")
  (net 127 "Net-(RP4-Pad10)")
  (net 128 "Net-(RP4-Pad11)")
  (net 129 "Net-(RP4-Pad12)")
  (net 130 "Net-(RP4-Pad13)")
  (net 131 "Net-(RP4-Pad14)")
  (net 132 "Net-(RP5-Pad10)")
  (net 133 "Net-(RP5-Pad11)")
  (net 134 "Net-(RP5-Pad12)")
  (net 135 "Net-(RP5-Pad13)")
  (net 136 "Net-(RP5-Pad14)")
  (net 137 "Net-(RP6-Pad8)")
  (net 138 "Net-(RP6-Pad9)")
  (net 139 "Net-(RP6-Pad10)")
  (net 140 "Net-(RP6-Pad11)")
  (net 141 "Net-(RP6-Pad12)")
  (net 142 "Net-(RP6-Pad13)")
  (net 143 "Net-(RP6-Pad14)")
  (net 144 "Net-(U17-Pad4)")
  (net 145 "Net-(U17-Pad9)")
  (net 146 "Net-(U18-Pad9)")
  (net 147 "Net-(U18-Pad4)")
  (net 148 "Net-(U19-Pad4)")
  (net 149 "Net-(U19-Pad9)")
  (net 150 "Net-(RP1-Pad16)")
  (net 151 "Net-(RP1-Pad15)")
  (net 152 "Net-(RP2-Pad15)")
  (net 153 "Net-(RP3-Pad15)")
  (net 154 "Net-(RP4-Pad15)")
  (net 155 "Net-(RP5-Pad15)")
  (net 156 "Net-(RP6-Pad16)")
  (net 157 "Net-(RP6-Pad15)")
  (net 158 "Net-(RP2-Pad16)")
  (net 159 "Net-(RP3-Pad16)")
  (net 160 "Net-(RP4-Pad16)")
  (net 161 "Net-(RP5-Pad16)")
  (net 162 "Net-(SW1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.3556)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (diff_pair_width 0.3556)
    (diff_pair_gap 0.254)
    (add_net /1Hz)
    (add_net /2Hz)
    (add_net /HOURS)
    (add_net /HOURS_OUT)
    (add_net /MINUTES)
    (add_net /MINUTES_OUT)
    (add_net /SECONDS_RESET)
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(RP1-Pad1)")
    (add_net "Net-(RP1-Pad10)")
    (add_net "Net-(RP1-Pad11)")
    (add_net "Net-(RP1-Pad12)")
    (add_net "Net-(RP1-Pad13)")
    (add_net "Net-(RP1-Pad14)")
    (add_net "Net-(RP1-Pad15)")
    (add_net "Net-(RP1-Pad16)")
    (add_net "Net-(RP1-Pad2)")
    (add_net "Net-(RP1-Pad3)")
    (add_net "Net-(RP1-Pad4)")
    (add_net "Net-(RP1-Pad5)")
    (add_net "Net-(RP1-Pad6)")
    (add_net "Net-(RP1-Pad7)")
    (add_net "Net-(RP1-Pad8)")
    (add_net "Net-(RP1-Pad9)")
    (add_net "Net-(RP2-Pad1)")
    (add_net "Net-(RP2-Pad10)")
    (add_net "Net-(RP2-Pad11)")
    (add_net "Net-(RP2-Pad12)")
    (add_net "Net-(RP2-Pad13)")
    (add_net "Net-(RP2-Pad14)")
    (add_net "Net-(RP2-Pad15)")
    (add_net "Net-(RP2-Pad16)")
    (add_net "Net-(RP2-Pad2)")
    (add_net "Net-(RP2-Pad3)")
    (add_net "Net-(RP2-Pad4)")
    (add_net "Net-(RP2-Pad5)")
    (add_net "Net-(RP2-Pad6)")
    (add_net "Net-(RP2-Pad7)")
    (add_net "Net-(RP3-Pad1)")
    (add_net "Net-(RP3-Pad10)")
    (add_net "Net-(RP3-Pad11)")
    (add_net "Net-(RP3-Pad12)")
    (add_net "Net-(RP3-Pad13)")
    (add_net "Net-(RP3-Pad14)")
    (add_net "Net-(RP3-Pad15)")
    (add_net "Net-(RP3-Pad16)")
    (add_net "Net-(RP3-Pad2)")
    (add_net "Net-(RP3-Pad3)")
    (add_net "Net-(RP3-Pad4)")
    (add_net "Net-(RP3-Pad5)")
    (add_net "Net-(RP3-Pad6)")
    (add_net "Net-(RP3-Pad7)")
    (add_net "Net-(RP4-Pad1)")
    (add_net "Net-(RP4-Pad10)")
    (add_net "Net-(RP4-Pad11)")
    (add_net "Net-(RP4-Pad12)")
    (add_net "Net-(RP4-Pad13)")
    (add_net "Net-(RP4-Pad14)")
    (add_net "Net-(RP4-Pad15)")
    (add_net "Net-(RP4-Pad16)")
    (add_net "Net-(RP4-Pad2)")
    (add_net "Net-(RP4-Pad3)")
    (add_net "Net-(RP4-Pad4)")
    (add_net "Net-(RP4-Pad5)")
    (add_net "Net-(RP4-Pad6)")
    (add_net "Net-(RP4-Pad7)")
    (add_net "Net-(RP5-Pad1)")
    (add_net "Net-(RP5-Pad10)")
    (add_net "Net-(RP5-Pad11)")
    (add_net "Net-(RP5-Pad12)")
    (add_net "Net-(RP5-Pad13)")
    (add_net "Net-(RP5-Pad14)")
    (add_net "Net-(RP5-Pad15)")
    (add_net "Net-(RP5-Pad16)")
    (add_net "Net-(RP5-Pad2)")
    (add_net "Net-(RP5-Pad3)")
    (add_net "Net-(RP5-Pad4)")
    (add_net "Net-(RP5-Pad5)")
    (add_net "Net-(RP5-Pad6)")
    (add_net "Net-(RP5-Pad7)")
    (add_net "Net-(RP6-Pad1)")
    (add_net "Net-(RP6-Pad10)")
    (add_net "Net-(RP6-Pad11)")
    (add_net "Net-(RP6-Pad12)")
    (add_net "Net-(RP6-Pad13)")
    (add_net "Net-(RP6-Pad14)")
    (add_net "Net-(RP6-Pad15)")
    (add_net "Net-(RP6-Pad16)")
    (add_net "Net-(RP6-Pad2)")
    (add_net "Net-(RP6-Pad3)")
    (add_net "Net-(RP6-Pad4)")
    (add_net "Net-(RP6-Pad5)")
    (add_net "Net-(RP6-Pad6)")
    (add_net "Net-(RP6-Pad7)")
    (add_net "Net-(RP6-Pad8)")
    (add_net "Net-(RP6-Pad9)")
    (add_net "Net-(SW1-Pad3)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U10-Pad1)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad4)")
    (add_net "Net-(U10-Pad7)")
    (add_net "Net-(U11-Pad1)")
    (add_net "Net-(U11-Pad11)")
    (add_net "Net-(U11-Pad8)")
    (add_net "Net-(U11-Pad9)")
    (add_net "Net-(U12-Pad1)")
    (add_net "Net-(U12-Pad11)")
    (add_net "Net-(U12-Pad9)")
    (add_net "Net-(U13-Pad1)")
    (add_net "Net-(U13-Pad11)")
    (add_net "Net-(U13-Pad8)")
    (add_net "Net-(U13-Pad9)")
    (add_net "Net-(U14-Pad1)")
    (add_net "Net-(U14-Pad11)")
    (add_net "Net-(U14-Pad3)")
    (add_net "Net-(U15-Pad1)")
    (add_net "Net-(U15-Pad11)")
    (add_net "Net-(U15-Pad2)")
    (add_net "Net-(U15-Pad9)")
    (add_net "Net-(U17-Pad4)")
    (add_net "Net-(U17-Pad9)")
    (add_net "Net-(U18-Pad4)")
    (add_net "Net-(U18-Pad9)")
    (add_net "Net-(U19-Pad4)")
    (add_net "Net-(U19-Pad9)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U6-Pad4)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U8-Pad4)")
    (add_net "Net-(U9-Pad4)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (diff_pair_width 0.508)
    (diff_pair_gap 0.254)
    (add_net GND)
    (add_net VCC)
  )
  (module MountingHole:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 56DDBED4)
    (at 173.5 173.5 90)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference HOLE3 (at 0 -4 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 4 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.59099 -1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 -2.25 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -1.59099 -1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -2.25 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -1.59099 1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 2.25 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 1.59099 1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 2.25 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 8 GND))
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 97.79 171.45 270)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C4 (at 1.27 3.81 270) (layer F.SilkS))
    (fp_text value 100nF (at 1.27 2.54 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Display_7Segment:DA56-11SURKWA (layer F.Cu) (tedit 5A02FE84)
    (at 93.98 167.64 180)
    (descr "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA56-11SURKWA(Ver.11A).pdf")
    (tags "Double digit seven segment hyper red LED display")
    (fp_text reference U19 (at -3.175 15.24 270) (layer F.SilkS))
    (fp_text value DA56-11SRWA (at 4 24.5 180) (layer F.Fab))
    (fp_text user %R (at 8 10 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(RP6-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(RP6-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(RP6-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(U19-Pad4)"))
    (pad 5 thru_hole circle (at 0 10.16 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(RP5-Pad1)"))
    (pad 6 thru_hole circle (at 0 12.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(RP5-Pad2)"))
    (pad 7 thru_hole circle (at 0 15.24 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(RP5-Pad6)"))
    (pad 8 thru_hole circle (at 0 17.78 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(RP5-Pad3)"))
    (pad 9 thru_hole circle (at 0 20.32 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 149 "Net-(U19-Pad9)"))
    (pad 10 thru_hole circle (at 15.24 20.32 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(RP5-Pad4)"))
    (pad 11 thru_hole circle (at 15.24 17.78 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(RP5-Pad5)"))
    (pad 12 thru_hole circle (at 15.24 15.24 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(RP5-Pad7)"))
    (pad 13 thru_hole circle (at 15.24 12.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 14 thru_hole circle (at 15.24 10.16 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 15 thru_hole circle (at 15.24 7.62 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(RP6-Pad4)"))
    (pad 16 thru_hole circle (at 15.24 5.08 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(RP6-Pad5)"))
    (pad 17 thru_hole circle (at 15.24 2.54 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(RP6-Pad6)"))
    (pad 18 thru_hole circle (at 15.24 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(RP6-Pad7)"))
    (model ${KISYS3DMOD}/Display_7Segment.3dshapes/DA56-11SURKWA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 107.95 133.35)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference RP5 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 470 (at 7.62 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(RP5-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(RP5-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(RP5-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(RP5-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(RP5-Pad5)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(RP5-Pad6)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(RP5-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(D4-Pad1)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(RP5-Pad10)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 133 "Net-(RP5-Pad11)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(RP5-Pad12)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 135 "Net-(RP5-Pad13)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 136 "Net-(RP5-Pad14)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 155 "Net-(RP5-Pad15)"))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 161 "Net-(RP5-Pad16)"))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 107.95 120.65)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference RP4 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 470 (at 7.62 5.715) (layer F.SilkS))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 160 "Net-(RP4-Pad16)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 154 "Net-(RP4-Pad15)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 131 "Net-(RP4-Pad14)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 130 "Net-(RP4-Pad13)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 129 "Net-(RP4-Pad12)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 128 "Net-(RP4-Pad11)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 127 "Net-(RP4-Pad10)"))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(D3-Pad1)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(RP4-Pad7)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(RP4-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(RP4-Pad5)"))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(RP4-Pad4)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(RP4-Pad3)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(RP4-Pad2)"))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(RP4-Pad1)"))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 107.95 107.95)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference RP3 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 470 (at 7.62 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(RP3-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(RP3-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(RP3-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(RP3-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(RP3-Pad5)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(RP3-Pad6)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(RP3-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(D2-Pad1)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(RP3-Pad10)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(RP3-Pad11)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(RP3-Pad12)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(RP3-Pad13)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(RP3-Pad14)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(RP3-Pad15)"))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 159 "Net-(RP3-Pad16)"))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Display_7Segment:DA56-11SURKWA (layer F.Cu) (tedit 5A02FE84)
    (at 93.98 106.68 180)
    (descr "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA56-11SURKWA(Ver.11A).pdf")
    (tags "Double digit seven segment hyper red LED display")
    (fp_text reference U17 (at -3.175 5.3975 270) (layer F.SilkS))
    (fp_text value DA56-11SRWA (at 4 24.5 180) (layer F.Fab))
    (fp_text user %R (at 8 10 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(RP2-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(RP2-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(RP2-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 144 "Net-(U17-Pad4)"))
    (pad 5 thru_hole circle (at 0 10.16 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(RP1-Pad1)"))
    (pad 6 thru_hole circle (at 0 12.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(RP1-Pad2)"))
    (pad 7 thru_hole circle (at 0 15.24 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(RP1-Pad6)"))
    (pad 8 thru_hole circle (at 0 17.78 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(RP1-Pad3)"))
    (pad 9 thru_hole circle (at 0 20.32 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 145 "Net-(U17-Pad9)"))
    (pad 10 thru_hole circle (at 15.24 20.32 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(RP1-Pad4)"))
    (pad 11 thru_hole circle (at 15.24 17.78 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(RP1-Pad5)"))
    (pad 12 thru_hole circle (at 15.24 15.24 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(RP1-Pad7)"))
    (pad 13 thru_hole circle (at 15.24 12.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 14 thru_hole circle (at 15.24 10.16 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 15 thru_hole circle (at 15.24 7.62 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(RP2-Pad4)"))
    (pad 16 thru_hole circle (at 15.24 5.08 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(RP2-Pad5)"))
    (pad 17 thru_hole circle (at 15.24 2.54 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(RP2-Pad6)"))
    (pad 18 thru_hole circle (at 15.24 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(RP2-Pad7)"))
    (model ${KISYS3DMOD}/Display_7Segment.3dshapes/DA56-11SURKWA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 107.95 95.25)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference RP2 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 470 (at 7.62 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(RP2-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(RP2-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(RP2-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(RP2-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(RP2-Pad5)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(RP2-Pad6)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(RP2-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(D1-Pad1)"))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(RP2-Pad10)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(RP2-Pad11)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(RP2-Pad12)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(RP2-Pad13)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(RP2-Pad14)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 152 "Net-(RP2-Pad15)"))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 158 "Net-(RP2-Pad16)"))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 120.65 82.55 270)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C5 (at 5.715 0) (layer F.SilkS))
    (fp_text value 100nF (at 6.985 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 107.95 82.55)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference RP1 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 470 (at 7.62 5.715) (layer F.SilkS))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 150 "Net-(RP1-Pad16)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 151 "Net-(RP1-Pad15)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(RP1-Pad14)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(RP1-Pad13)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(RP1-Pad12)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(RP1-Pad11)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(RP1-Pad10)"))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(RP1-Pad9)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(RP1-Pad8)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(RP1-Pad7)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(RP1-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(RP1-Pad5)"))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(RP1-Pad4)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(RP1-Pad3)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(RP1-Pad2)"))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(RP1-Pad1)"))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 120.65 171.45 270)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C1 (at -5.715 1.905) (layer F.SilkS))
    (fp_text value 100nF (at -5.715 -1.905) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 97.79 158.75 270)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C2 (at 5.715 0) (layer F.SilkS))
    (fp_text value 100nF (at 6.985 -0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 120.65 158.75 270)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C3 (at 5.715 1.905) (layer F.SilkS))
    (fp_text value 100nF (at 5.715 -1.905) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 120.65 95.25 270)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C6 (at 5.715 0) (layer F.SilkS))
    (fp_text value 100nF (at 6.985 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 120.65 107.95 270)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C7 (at 5.715 0) (layer F.SilkS))
    (fp_text value 100nF (at 6.985 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 120.65 120.65 270)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C8 (at 5.715 0) (layer F.SilkS))
    (fp_text value 100nF (at 6.985 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 120.65 133.35 270)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C9 (at 5.715 0) (layer F.SilkS))
    (fp_text value 100nF (at 6.985 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 120.65 146.05 270)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C10 (at 5.715 0) (layer F.SilkS))
    (fp_text value 100nF (at 6.985 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 146.05 82.55 90)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C11 (at -5.715 0 180) (layer F.SilkS))
    (fp_text value 100nF (at -6.985 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 146.05 95.25 90)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C12 (at -5.715 0 180) (layer F.SilkS))
    (fp_text value 100nF (at -6.985 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 146.05 107.95 90)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C13 (at -5.715 0 180) (layer F.SilkS))
    (fp_text value 100nF (at -6.985 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 146.05 120.65 90)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C14 (at -5.715 0 180) (layer F.SilkS))
    (fp_text value 100nF (at -6.985 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 146.05 133.35 90)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C15 (at -5.715 0 180) (layer F.SilkS))
    (fp_text value 100nF (at -6.985 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_762 (layer F.Cu) (tedit 55B336B3)
    (at 146.05 146.05 90)
    (descr "Ceramic Capacitor, 7.62mm lead spacing")
    (tags CAPACITOR)
    (autoplace_cost180 10)
    (fp_text reference C16 (at -5.715 0 180) (layer F.SilkS))
    (fp_text value 100nF (at -6.985 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 162.8775 156.21)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C17 (at 5.715 2.54 90) (layer F.SilkS))
    (fp_text value 100uF (at 5.715 -1.905 90) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 146.685 171.45 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C18 (at 1.905 -1.905 270) (layer F.SilkS))
    (fp_text value 12pF (at -1.905 -1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C18-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:C_Trim_Murata (layer F.Cu) (tedit 5298D76A)
    (at 153.67 171.45 90)
    (descr "Trimmer Capacitor Murata")
    (tags "Trimmer Capacitor Murata")
    (fp_text reference C19 (at -3.175 -3.81 90) (layer F.SilkS))
    (fp_text value 5-30pF (at 1.5875 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.99898 1.99898) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C19-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.99898 1.99898) (drill 1.30048) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
  )
  (module LED_THT:LED_D3.0mm_FlatTop (layer F.Cu) (tedit 5880A862)
    (at 81.28 110.49 270)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.8575 270) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 106 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_FlatTop (layer F.Cu) (tedit 5880A862)
    (at 91.44 110.49 270)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.8575 270) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 107 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 VCC))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_FlatTop (layer F.Cu) (tedit 5880A862)
    (at 81.28 140.97 270)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -2.8575 270) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 108 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_FlatTop (layer F.Cu) (tedit 5880A862)
    (at 91.44 140.97 270)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.8575 270) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 109 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 VCC))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 56DDBED4)
    (at 80.5 173.5 90)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference HOLE1 (at 0 -4 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 4 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.59099 -1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 -2.25 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -1.59099 -1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -2.25 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -1.59099 1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 2.25 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 1.59099 1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 2.25 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 8 GND))
  )
  (module MountingHole:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 56DDBED4)
    (at 80.5 80.5 90)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference HOLE2 (at 0 -4 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 4 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 2.25 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 1.59099 1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 2.25 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -1.59099 1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -2.25 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -1.59099 -1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 -2.25 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 1.59099 -1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
  )
  (module MountingHole:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 56DDBED4)
    (at 173.4 80.5 90)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference HOLE4 (at 0 -4 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 4 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 2.25 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 1.59099 1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 2.25 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -1.59099 1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -2.25 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -1.59099 -1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 -2.25 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at 1.59099 -1.59099 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 GND))
  )
  (module My_Components:Conn_Power_Jack_Circular_Pads (layer F.Cu) (tedit 54E972BC)
    (at 163.6 169.4 90)
    (descr "Connector, Power Jack")
    (tags "CONN POWER JACK")
    (fp_text reference P1 (at -5.225 -5.485 90) (layer F.SilkS))
    (fp_text value 5V (at -0.145 -5.485 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0 90) (size 4 4) (drill 2.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 1 thru_hole circle (at 6.20014 0 90) (size 4.5 4.5) (drill 3.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 3 thru_hole circle (at 2.99974 4.8006 90) (size 4 4) (drill 2.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model connectors/POWER_21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 170.18 97.79 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 6.35 0 90) (layer F.SilkS))
    (fp_text value 4.7k (at 9.525 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R1-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 172.72 97.79 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 6.35 0 90) (layer F.SilkS))
    (fp_text value 4.7k (at 9.525 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 175.26 97.79 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R3 (at 6.35 0 90) (layer F.SilkS))
    (fp_text value 4.7k (at 9.525 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 170.815 156.21 270)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R4 (at 9.525 -0.635 270) (layer F.SilkS))
    (fp_text value 4.7k (at 6.35 -0.635 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(R4-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 173.355 156.21 270)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R5 (at 9.525 0 270) (layer F.SilkS))
    (fp_text value 4.7k (at 6.35 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(R5-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 149.225 162.56 270)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R6 (at -6.35 0.635 270) (layer F.SilkS))
    (fp_text value 330k (at -6.35 -1.27 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C19-Pad1)"))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(R6-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 146.685 162.56 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R7 (at -1.905 -1.905 90) (layer F.SilkS))
    (fp_text value 15M (at 1.27 -1.905 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C18-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(R6-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Switch_SPDP_D2F (layer F.Cu) (tedit 55B323A4)
    (at 172.72 111.76 90)
    (descr "Switch SPDP Omron D2F")
    (tags "SPDP OMRON D2F")
    (fp_text reference SW1 (at -4.445 -3.81 90) (layer F.SilkS))
    (fp_text value SECONDS (at 3.175 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -5.08 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 162 "Net-(SW1-Pad3)"))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Switch_SPDP_D2F (layer F.Cu) (tedit 55B323A4)
    (at 172.72 127 90)
    (descr "Switch SPDP Omron D2F")
    (tags "SPDP OMRON D2F")
    (fp_text reference SW2 (at -4.445 -3.81 90) (layer F.SilkS))
    (fp_text value MINUTES (at 3.175 -3.81 90) (layer F.SilkS))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(R3-Pad1)"))
    (pad 1 thru_hole rect (at -5.08 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Switch_SPDP_D2F (layer F.Cu) (tedit 55B323A4)
    (at 172.72 142.24 90)
    (descr "Switch SPDP Omron D2F")
    (tags "SPDP OMRON D2F")
    (fp_text reference SW3 (at -4.445 -3.81 90) (layer F.SilkS))
    (fp_text value HOURS (at 3.81 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -5.08 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(R5-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(R4-Pad1)"))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 133.35 171.45)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U1 (at -6.985 -5.715) (layer F.SilkS))
    (fp_text value 74HCT4060 (at 3.81 -5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /2Hz))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(R6-Pad1)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C18-Pad1)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(U1-Pad15)"))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP14_300 (layer F.Cu) (tedit 52978438)
    (at 109.22 158.75)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U2 (at -6.35 5.715) (layer F.SilkS))
    (fp_text value 74LS00 (at 5.08 5.715) (layer F.SilkS))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /MINUTES))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(U2-Pad12)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(U2-Pad11)"))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /2Hz))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(U2-Pad2)"))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(U2-Pad8)"))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(U2-Pad2)"))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(R3-Pad1)"))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(U2-Pad12)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(U2-Pad12)"))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(U2-Pad2)"))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(R2-Pad1)"))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP14_300 (layer F.Cu) (tedit 52978438)
    (at 132.08 158.75)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U3 (at -5.715 5.715) (layer F.SilkS))
    (fp_text value 74LS00 (at 5.08 5.715) (layer F.SilkS))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /HOURS))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(U3-Pad12)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(U3-Pad11)"))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /2Hz))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(U3-Pad2)"))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(U3-Pad8)"))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(U3-Pad2)"))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(R5-Pad1)"))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(U3-Pad12)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(U3-Pad12)"))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(U3-Pad2)"))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(R4-Pad1)"))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP14_300 (layer F.Cu) (tedit 52978438)
    (at 109.22 171.45)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U4 (at -6.35 -5.715) (layer F.SilkS))
    (fp_text value 74LS00 (at 5.08 -5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /MINUTES))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(U12-Pad9)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(U4-Pad3)"))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(U4-Pad3)"))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R1-Pad1)"))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SECONDS_RESET))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /HOURS_OUT))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(U3-Pad8)"))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(U3-Pad11)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /MINUTES_OUT))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(U2-Pad8)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(U2-Pad11)"))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 133.35 82.55)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U5 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 74LS47 (at 6.35 5.715) (layer F.SilkS))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(RP1-Pad10)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(RP1-Pad11)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(RP1-Pad12)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(RP1-Pad13)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(RP1-Pad14)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 151 "Net-(RP1-Pad15)"))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 150 "Net-(RP1-Pad16)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(U11-Pad1)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(U11-Pad11)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(U5-Pad4)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(U11-Pad8)"))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(U11-Pad9)"))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 133.35 95.25)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U6 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 74LS47 (at 6.35 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(U12-Pad9)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /MINUTES))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(U6-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(U12-Pad11)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(U12-Pad1)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 158 "Net-(RP2-Pad16)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 152 "Net-(RP2-Pad15)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(RP2-Pad14)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(RP2-Pad13)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(RP2-Pad12)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(RP2-Pad11)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(RP2-Pad10)"))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 133.35 107.95)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U7 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 74LS47 (at 6.35 5.715) (layer F.SilkS))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(RP3-Pad10)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(RP3-Pad11)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(RP3-Pad12)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(RP3-Pad13)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(RP3-Pad14)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(RP3-Pad15)"))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 159 "Net-(RP3-Pad16)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(U13-Pad1)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(U13-Pad11)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(U7-Pad4)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(U13-Pad8)"))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(U13-Pad9)"))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 133.35 120.65)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U8 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 74LS47 (at 6.35 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(U14-Pad3)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /HOURS))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(U8-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(U14-Pad11)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(U14-Pad1)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 160 "Net-(RP4-Pad16)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 154 "Net-(RP4-Pad15)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 131 "Net-(RP4-Pad14)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 130 "Net-(RP4-Pad13)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 129 "Net-(RP4-Pad12)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 128 "Net-(RP4-Pad11)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 127 "Net-(RP4-Pad10)"))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 133.35 133.35)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U9 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 74LS47 (at 6.35 5.715) (layer F.SilkS))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(RP5-Pad10)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 133 "Net-(RP5-Pad11)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(RP5-Pad12)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 135 "Net-(RP5-Pad13)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 136 "Net-(RP5-Pad14)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 155 "Net-(RP5-Pad15)"))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 161 "Net-(RP5-Pad16)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(U15-Pad1)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(U15-Pad11)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(U9-Pad4)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(U15-Pad2)"))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(U15-Pad9)"))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 133.35 146.05)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference U10 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 74LS47 (at 6.35 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(U10-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(U10-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(U10-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(U10-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 156 "Net-(RP6-Pad16)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 157 "Net-(RP6-Pad15)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 143 "Net-(RP6-Pad14)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 142 "Net-(RP6-Pad13)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 141 "Net-(RP6-Pad12)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 140 "Net-(RP6-Pad11)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 139 "Net-(RP6-Pad10)"))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP14_300 (layer F.Cu) (tedit 52978438)
    (at 157.48 82.55)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U11 (at -6.35 5.715) (layer F.SilkS))
    (fp_text value 74LS90 (at 5.08 5.715) (layer F.SilkS))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /1Hz))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(U11-Pad1)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(U11-Pad11)"))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(U11-Pad9)"))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(U11-Pad8)"))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SECONDS_RESET))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SECONDS_RESET))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(U11-Pad1)"))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP14_300 (layer F.Cu) (tedit 52978438)
    (at 157.48 95.25)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U12 (at -6.35 5.715) (layer F.SilkS))
    (fp_text value 74LS90 (at 5.08 5.715) (layer F.SilkS))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(U11-Pad11)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(U12-Pad1)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(U12-Pad11)"))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(U12-Pad9)"))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /MINUTES))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SECONDS_RESET))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SECONDS_RESET))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(U12-Pad1)"))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP14_300 (layer F.Cu) (tedit 52978438)
    (at 157.48 107.95)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U13 (at -6.35 5.715) (layer F.SilkS))
    (fp_text value 74LS90 (at 5.08 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(U13-Pad1)"))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(U13-Pad8)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(U13-Pad9)"))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(U13-Pad11)"))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(U13-Pad1)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /MINUTES_OUT))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP14_300 (layer F.Cu) (tedit 52978438)
    (at 157.48 120.65)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U14 (at -6.35 5.715) (layer F.SilkS))
    (fp_text value 74LS90 (at 5.08 5.715) (layer F.SilkS))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(U13-Pad11)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(U14-Pad1)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(U14-Pad11)"))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(U14-Pad3)"))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /HOURS))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(U14-Pad3)"))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /HOURS))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(U14-Pad1)"))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP14_300 (layer F.Cu) (tedit 52978438)
    (at 157.48 133.35)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U15 (at -6.35 5.715) (layer F.SilkS))
    (fp_text value 74LS90 (at 5.08 5.715) (layer F.SilkS))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /HOURS_OUT))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(U15-Pad1)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(U15-Pad11)"))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(U15-Pad9)"))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(U15-Pad2)"))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(U10-Pad1)"))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(U15-Pad2)"))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(U15-Pad1)"))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP14_300 (layer F.Cu) (tedit 52978438)
    (at 157.48 146.05)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U16 (at -6.35 5.715) (layer F.SilkS))
    (fp_text value 74LS90 (at 5.08 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(U15-Pad11)"))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(U15-Pad2)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(U10-Pad1)"))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(U10-Pad1)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(U10-Pad7)"))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(U10-Pad2)"))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /1Hz))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /2Hz))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Crystal_32K_Horiz (layer F.Cu) (tedit 5DAA8F5F)
    (at 153.67 166.37 180)
    (descr "crystal resonator for RTC, 32768 Hz")
    (tags "CRYSTAL RTC")
    (fp_text reference Y1 (at -2.54 3.175 270) (layer F.SilkS))
    (fp_text value 32768Hz (at -2.54 8.255 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C19-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C18-Pad1)"))
    (pad ~ thru_hole circle (at -1.27 5.08 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad ~ thru_hole circle (at 1.27 5.08 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/c_vert_c1v5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Display_7Segment:DA56-11SURKWA (layer F.Cu) (tedit 5A02FE84)
    (at 93.98 137.16 180)
    (descr "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA56-11SURKWA(Ver.11A).pdf")
    (tags "Double digit seven segment hyper red LED display")
    (fp_text reference U18 (at -3.175 10.16 270) (layer F.SilkS))
    (fp_text value DA56-11SRWA (at 4 24.5 180) (layer F.Fab))
    (fp_text user %R (at 8 10 180) (layer F.Fab))
    (pad 18 thru_hole circle (at 15.24 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(RP4-Pad7)"))
    (pad 17 thru_hole circle (at 15.24 2.54 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(RP4-Pad6)"))
    (pad 16 thru_hole circle (at 15.24 5.08 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(RP4-Pad5)"))
    (pad 15 thru_hole circle (at 15.24 7.62 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(RP4-Pad4)"))
    (pad 14 thru_hole circle (at 15.24 10.16 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 13 thru_hole circle (at 15.24 12.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 12 thru_hole circle (at 15.24 15.24 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(RP3-Pad7)"))
    (pad 11 thru_hole circle (at 15.24 17.78 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(RP3-Pad5)"))
    (pad 10 thru_hole circle (at 15.24 20.32 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(RP3-Pad4)"))
    (pad 9 thru_hole circle (at 0 20.32 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 146 "Net-(U18-Pad9)"))
    (pad 8 thru_hole circle (at 0 17.78 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(RP3-Pad3)"))
    (pad 7 thru_hole circle (at 0 15.24 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(RP3-Pad6)"))
    (pad 6 thru_hole circle (at 0 12.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(RP3-Pad2)"))
    (pad 5 thru_hole circle (at 0 10.16 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(RP3-Pad1)"))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(U18-Pad4)"))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(RP4-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(RP4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(RP4-Pad1)"))
    (model ${KISYS3DMOD}/Display_7Segment.3dshapes/DA56-11SURKWA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:IC_DIP16_300 (layer F.Cu) (tedit 5297847C)
    (at 107.95 146.05)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (fp_text reference RP6 (at -7.62 5.715) (layer F.SilkS))
    (fp_text value 470 (at 7.62 5.715) (layer F.SilkS))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 156 "Net-(RP6-Pad16)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 157 "Net-(RP6-Pad15)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 143 "Net-(RP6-Pad14)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 142 "Net-(RP6-Pad13)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 141 "Net-(RP6-Pad12)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 140 "Net-(RP6-Pad11)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 139 "Net-(RP6-Pad10)"))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 138 "Net-(RP6-Pad9)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 137 "Net-(RP6-Pad8)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(RP6-Pad7)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(RP6-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(RP6-Pad5)"))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(RP6-Pad4)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(RP6-Pad3)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(RP6-Pad2)"))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(RP6-Pad1)"))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Copyright\n(C) 2020\nSergey\nKiselev" (at 92.075 80.645 90) (layer F.SilkS))
  (gr_text "TTL\nClock\nV1.1" (at 88.5825 173.355 90) (layer F.SilkS))
  (gr_line (start 177 79) (end 177 175) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 77) (end 175 77) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 77 175.4) (end 77 79) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 175 177) (end 78.6 177) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 175 175) (end 177 175) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 78.6 175.4) (end 78.6 177) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 175 79) (end 175 77) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 79 79) (end 77 79) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 8) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177 177) (xy 77 177) (xy 77 77) (xy 177 76.8)
      )
    )
  )
)
